| NUC472_NUC442_BSP V3.03.003 The Board Support Package for NUC472/NUC442

Functions
lw_usbh.c File Reference

Light-Weight USB Host driver. More...

`#include <stdio.h>`
`#include <stdlib.h>`
`#include <string.h>`
`#include "NUC472_442.h"`
`#include "usb.h"`
`#include "lw_usbh.h"`
Include dependency graph for lw_usbh.c:

Go to the source code of this file.

## Functions
int | usbh_drv_ctrl_req (uint8_t requesttype, uint8_t request, uint16_t value, uint16_t index, uint16_t length, int data_len, uint8_t *buffer, int dir)
| Execute a control transfer request. More...
int | usbh_drv_bulk_xfer (uint16_t ep_addr, uint8_t *toggle, uint8_t *data_buff, int data_len, int timeout)
| Execute a control transfer request. More...
int | usbh_get_device_descriptor (uint8_t *desc_buff)
| Get device descriptor from the USB device. More...
int | get_config_descriptor (uint8_t *desc_buff)
| Get configuration descriptor from the USB device. More...
int | usbh_set_configuration (int conf_val)
| Issue a standard request SET_CONFIGURATION to USB device. More...
int | usbh_clear_halt (uint16_t ep_addr)
| Issue a standard request SET_FEATURE to clear USB device endpoint halt state. More...
int | usbh_probe_port (uint32_t port)
| Probe USB root-hub port connect/disconnect status. A newly connected device will be initialized in this function. More...
int | usbh_init (void)
| Initialized USB host controller driver. More...

## Detailed Description

Light-Weight USB Host driver.

Version
  V1.00

Revision
  5

Date
  14/10/07 5:47p

Note
  SPDX-License-Identifier: Apache-2.0 Copyright (C) 2014 Nuvoton Technology Corp. All rights reserved.

Definition in file lw_usbh.c.