| NUC472_NUC442_BSP V3.03.003 The Board Support Package for NUC472/NUC442

Data Fields
UART_T Struct Reference

`#include <NUC472_442.h>`

## Data Fields
__IO uint32_t | DAT
__IO uint32_t | INTEN
__IO uint32_t | FIFO
__IO uint32_t | LINE
__IO uint32_t | MODEM
__IO uint32_t | MODEMSTS
__IO uint32_t | FIFOSTS
__IO uint32_t | INTSTS
__IO uint32_t | TOUT
__IO uint32_t | BAUD
__IO uint32_t | IRDA
__IO uint32_t | ALTCTL
__IO uint32_t | FUNCSEL
__IO uint32_t | LINCTL
__IO uint32_t | LINSTS
__IO uint32_t | LINDEBUG

## Detailed Description

    @addtogroup UART Universal Asynchronous Receiver/Transmitter Controller(UART)
    Memory Mapped Structure for UART Controller

Definition at line 25170 of file NUC472_442.h.

The documentation for this struct was generated from the following file:

- Device/Nuvoton/NUC472_442/Include/NUC472_442.h