| NUC472_NUC442_BSP V3.03.003 The Board Support Package for NUC472/NUC442

Functions
Umas_FATFS.c File Reference

NUC472/NUC442 MCU USB Host Mass Storage driver for FATFS. More...

`#include <stdio.h>`
`#include <string.h>`
`#include "NUC472_442.h"`
`#include "usbh_core.h"`
`#include "Umas.h"`
`#include "diskio.h"`
`#include "usbh_umas.h"`
Include dependency graph for Umas_FATFS.c:

Go to the source code of this file.

## Functions
int32_t | USBH_MassRawRead (mass_disk_t *disk, uint32_t sectorN, int32_t scnt, uint8_t *buff)
| Read raw data from connected USB Mass Storage disk. More...
int32_t | USBH_MassRawWrite (mass_disk_t *disk, uint32_t sectorN, int32_t scnt, uint8_t *buff)
| Write raw data to connected USB Mass Storage disk. More...

## Detailed Description

NUC472/NUC442 MCU USB Host Mass Storage driver for FATFS.

Version
  V1.00

Revision
  8

Date
  15/12/03 10:22a

Note
  SPDX-License-Identifier: Apache-2.0 Copyright (C) 2013 Nuvoton Technology Corp. All rights reserved.

Definition in file Umas_FATFS.c.