| NUC472_NUC442_BSP V3.03.003 The Board Support Package for NUC472/NUC442

Functions | Variables
pdma.c File Reference

NUC472/NUC442 PDMA driver source file. More...

`#include "NUC472_442.h"`
Include dependency graph for pdma.c:

Go to the source code of this file.

## Functions
void | PDMA_Open (uint32_t u32Mask)
| PDMA Open. More...
void | PDMA_Close (void)
| PDMA Close. More...
void | PDMA_SetTransferCnt (uint32_t u32Ch, uint32_t u32Width, uint32_t u32TransCount)
| Set PDMA Transfer Count. More...
void | PDMA_SetTransferAddr (uint32_t u32Ch, uint32_t u32SrcAddr, uint32_t u32SrcCtrl, uint32_t u32DstAddr, uint32_t u32DstCtrl)
| Set PDMA Transfer Address. More...
void | PDMA_SetTransferMode (uint32_t u32Ch, uint32_t u32Peripheral, uint32_t u32ScatterEn, uint32_t u32DescAddr)
| Set PDMA Transfer Mode. More...
void | PDMA_SetBurstType (uint32_t u32Ch, uint32_t u32BurstType, uint32_t u32BurstSize)
| Set PDMA Burst Type. More...
void | PDMA_Trigger (uint32_t u32Ch)
| Trigger PDMA. More...
void | PDMA_EnableInt (uint32_t u32Ch, uint32_t u32Mask)
| Enable Interrupt. More...
void | PDMA_DisableInt (uint32_t u32Ch, uint32_t u32Mask)
| Disable Interrupt. More...

## Variables
static uint8_t | u32ChSelect [PDMA_CH_MAX]

## Detailed Description

NUC472/NUC442 PDMA driver source file.

Version
  V1.00

Revision
  8

Date
  15/03/16 3:17p

Note
  SPDX-License-Identifier: Apache-2.0 Copyright (C) 2013 Nuvoton Technology Corp. All rights reserved.

Definition in file pdma.c.

## Variable Documentation

## ◆ u32ChSelect

uint8_t u32ChSelect[PDMA_CH_MAX]
| static

Definition at line 15 of file pdma.c.