| NUC472_NUC442_BSP V3.03.003 The Board Support Package for NUC472/NUC442

Data Fields
GPIO_T Struct Reference

`#include <NUC472_442.h>`

## Data Fields
__IO uint32_t | MODE
__IO uint32_t | DINOFF
__IO uint32_t | DOUT
__IO uint32_t | DATMSK
__I uint32_t | PIN
__IO uint32_t | DBEN
__IO uint32_t | INTTYPE
__IO uint32_t | INTEN
__IO uint32_t | INTSRC
__IO uint32_t | SMTEN
__IO uint32_t | SLEWCTL

## Detailed Description

    @addtogroup GPIO General Purpose Input/Output Controller(GPIO)
    Memory Mapped Structure for GPIO Controller

Definition at line 15010 of file NUC472_442.h.

The documentation for this struct was generated from the following file:

- Device/Nuvoton/NUC472_442/Include/NUC472_442.h