| NUC472_NUC442_BSP V3.03.003 The Board Support Package for NUC472/NUC442

Data Fields
uac_dev_t Struct Reference
NUC472/NUC442 Device Driver » USB Host Audio Class Driver » USB Host Audio Class Driver Exported Constants » USB Host Audio Class Driver Exported Type Define » USB Host Audio Class Driver Exported Structures

`#include <usbh_uac.h>`

Collaboration diagram for uac_dev_t:
[legend]

## Data Fields
USB_DEV_T * | udev
int | ctrl_ifnum
int | au_in_ifnum
int | au_out_ifnum
void * | priv
struct uac_dev_t * | next
EP_INFO_T * | ep_au_in
EP_INFO_T * | ep_au_out
URB_T * | urbin [ISO_IN_URB_CNT]
URB_T * | urbout [ISO_OUT_URB_CNT]
uint8_t | iso_inbuf [ISO_IN_URB_CNT][AU_IN_MAX_PKTSZ *ISO_FRAME_COUNT]
uint8_t | iso_outbuf [ISO_OUT_URB_CNT][AU_OUT_MAX_PKTSZ *ISO_FRAME_COUNT]
uint8_t | in_streaming
uint8_t | out_streaming
UAC_CB_FUNC * | au_in_func
UAC_CB_FUNC * | au_out_func
uint8_t * | au_in_buff
int | au_in_bufsz
int | au_in_bufidx

## Detailed Description

Audio Class device structure

Definition at line 99 of file usbh_uac.h.

The documentation for this struct was generated from the following file:

- UsbHostLib/INCLUDE/usbh_uac.h