| NUC472_NUC442_BSP V3.03.003 The Board Support Package for NUC472/NUC442

### NUC472_442 → StdDriver Relation

File in Device/Nuvoton/NUC472_442 | Includes file in StdDriver
--- | ---
Include / NUC472_442.h | inc / acmp.h
Include / NUC472_442.h | inc / adc.h
Include / NUC472_442.h | inc / can.h
Include / NUC472_442.h | inc / cap.h
Include / NUC472_442.h | inc / clk.h
Include / NUC472_442.h | inc / crc.h
Include / NUC472_442.h | inc / crypto.h
Include / NUC472_442.h | inc / eadc.h
Include / NUC472_442.h | inc / ebi.h
Include / NUC472_442.h | inc / emac.h
Include / NUC472_442.h | inc / epwm.h
Include / NUC472_442.h | inc / fmc.h
Include / NUC472_442.h | inc / gpio.h
Include / NUC472_442.h | inc / i2c.h
Include / NUC472_442.h | inc / i2s.h
Include / NUC472_442.h | inc / pdma.h
Include / NUC472_442.h | inc / ps2.h
Include / NUC472_442.h | inc / pwm.h
Include / NUC472_442.h | inc / rtc.h
Include / NUC472_442.h | inc / sc.h
Include / NUC472_442.h | inc / scuart.h
Include / NUC472_442.h | inc / sd.h
Include / NUC472_442.h | inc / spi.h
Include / NUC472_442.h | inc / sys.h
Include / NUC472_442.h | inc / timer.h
Include / NUC472_442.h | inc / uart.h
Include / NUC472_442.h | inc / usbd.h
Include / NUC472_442.h | inc / wdt.h
Include / NUC472_442.h | inc / wwdt.h