| NUC472_NUC442_BSP V3.03.003 The Board Support Package for NUC472/NUC442

Functions
lw_umass.c File Reference

Light-weight USB mass storage class driver. More...

`#include <stdio.h>`
`#include <stdlib.h>`
`#include <string.h>`
`#include "NUC472_442.h"`
`#include "diskio.h"`
`#include "usb.h"`
`#include "lw_usbh.h"`
`#include "lw_umass.h"`
Include dependency graph for lw_umass.c:

Go to the source code of this file.

## Functions
int | usbh_probe_umass (void)
| Try to probe and initialize an USB mass storage device. More...

## Detailed Description

Light-weight USB mass storage class driver.

Version
  V1.00

Revision
  5

Date
  15/12/07 9:16a

Note
  SPDX-License-Identifier: Apache-2.0 Copyright (C) 2014 Nuvoton Technology Corp. All rights reserved.

Definition in file lw_umass.c.