| NUC472_NUC442_BSP V3.03.003 The Board Support Package for NUC472/NUC442

Data Fields
usbhid_dev Struct Reference
NUC472/NUC442 Device Driver » USB Host HID Driver » USB Host HID Driver Exported Constants » USB Host HID Driver Exported Type Define » USB Host HID Driver Exported Structures

`#include <usbh_hid.h>`

Collaboration diagram for usbhid_dev:
[legend]

## Data Fields
USB_DEV_T * | udev
int | ifnum
uint8_t | bSubClassCode
uint8_t | bProtocolCode
URB_T * | urbin
URB_T * | urbout
uint8_t | inbuf [HID_MAX_BUFFER_SIZE]
HID_IR_FUNC * | read_func
HID_IW_FUNC * | write_func
struct usbhid_dev * | next
uint8_t | client [HID_CLIENT_SIZE]

## Detailed Description

HID device structure

Definition at line 91 of file usbh_hid.h.

The documentation for this struct was generated from the following file:

- UsbHostLib/INCLUDE/usbh_hid.h