| NUC472_NUC442_BSP V3.03.003 The Board Support Package for NUC472/NUC442

Data Fields
urb_t Struct Reference
NUC472/NUC442 Device Driver » USBH Driver » USBH Exported Constants » USBH Exported Structures

`#include <usbh_core.h>`

Collaboration diagram for urb_t:
[legend]

## Data Fields
URB_PRIV_T | urb_hcpriv
USB_LIST_T | urb_list
struct urb_t * | next
struct usb_device * | dev
uint32_t | pipe
int | status
uint32_t | transfer_flags
void * | transfer_buffer
int | transfer_buffer_length
int | actual_length
uint8_t * | setup_packet
int | start_frame
int | number_of_packets
int | interval
int | error_count
int | timeout
void * | context
void(* | complete )(struct urb_t *)
ISO_PACKET_DESCRIPTOR_T | iso_frame_desc [8]

## Detailed Description

Isochronous packet structure

URB structure

Definition at line 536 of file usbh_core.h.

The documentation for this struct was generated from the following file:

- UsbHostLib/INCLUDE/usbh_core.h