CMSIS-DAP: DAP_TransferConfigure

| CMSIS-DAP Version 1.2.0 (Proposal) Interface Firmware for CoreSight Debug Access Port

- Main Page
- Usage and Description
- Reference

All Functions Groups Pages
DAP_TransferConfigure
Transfer Commands

Configure Transfers. More...

Configure Transfers.

The DAP_TransferConfigure Command sets parameters for DAP_Transfer and DAP_TransferBlock.

DAP_TransferConfigure Command:

| BYTE | BYTE ******** SHORT *****| SHORT ******|
> 0x04 | Idle Cycles | WAIT Retry | Match Retry |
|******|*************|************|*************|

- Idle Cycles: Number of extra idle cycles after each transfer.
- WAIT Retry: Number of transfer retries after WAIT response.
- Match Retry: Number of retries on reads with Value Match in DAP_Transfer. On value mismatch the Register is read again until its value matches or the Match Retry count exceeds.
  retry = Match_Retry;
  do {
  if ((Register_Value & Match_Mask) == Match_Value) break;
  } while (retry--);

DAP_TransferConfigure Response:

| BYTE | BYTE **|
< 0x04 | Status |
|******|********|

- Status: Response Status