CMSIS-DAP: DAP_WriteABORT

| CMSIS-DAP Version 1.2.0 (Proposal) Interface Firmware for CoreSight Debug Access Port

- Main Page
- Usage and Description
- Reference

All Functions Groups Pages
DAP_WriteABORT
General Commands

Write ABORT Register. More...

Write ABORT Register.

The DAP_WriteABORT Command writes an abort request to the CoreSight ABORT register of the Target Device.

DAP_WriteABORT Command:

| BYTE | BYTE *****| WORD *|
> 0x08 | DAP Index | Abort |
|******|***********|*******|

- DAP Index: Zero based device index of the selected JTAG device. For SWD mode the value is ignored.
- Abort: 32-bit value to write into the CoreSight ABORT register.

DAP_WriteABORT Response:

| BYTE | BYTE **|
< 0x08 | Status |
|******|********|

- Status: Response Status