CMSIS-DAP: DAP_SWO_Mode

| CMSIS-DAP Version 1.2.0 (Proposal) Interface Firmware for CoreSight Debug Access Port

- Main Page
- Usage and Description
- Reference

All Functions Groups Pages
DAP_SWO_Mode
SWO Commands

Set SWO capture mode. More...

Set SWO capture mode.

## DAP_SWO_Mode (0x18):

Sets the SWO trace capture mode.

DAP_SWO_Mode Request:

| BYTE | BYTE |
> 0x18 | Mode |
|******|******|

- Mode:
  - 0 - Off (default)
  - 1 - UART
  - 2 - Manchester

DAP_SWO_Mode Response:

| BYTE | BYTE |
< 0x18 | Status |
|******|********|

- Status: Response Status