CMSIS-DAP: Common SWD/JTAG Commands

| CMSIS-DAP Version 1.2.0 (Proposal) Interface Firmware for CoreSight Debug Access Port

- Main Page
- Usage and Description
- Reference

All Functions Groups Pages
Content
Common SWD/JTAG Commands
CMSIS-DAP Commands

Set SWD/JTAG clock and control/monitor SWD/JTAG I/O pins. More...

## Content
| DAP_SWJ_Pins
| Control and monitor SWD/JTAG Pins.
| DAP_SWJ_Clock
| Select SWD/JTAG Clock.
| DAP_SWJ_Sequence
| Generate SWJ sequence SWDIO/TMS @SWCLK/TCK.

## Description

Set SWD/JTAG clock and control/monitor SWD/JTAG I/O pins.

The Common SWD/JTAG Commands allow to:

- Read and Write the SWD/JTAG I/O pins including nRESET.
- Configure the SWD/JTAG clock speed.
- Generate a sequence on the SWD/JTAG I/O pins for SWD<->JTAG mode switch.