CMSIS-DAP: DAP_Delay

| CMSIS-DAP Version 1.2.0 (Proposal) Interface Firmware for CoreSight Debug Access Port

- Main Page
- Usage and Description
- Reference

All Functions Groups Pages
DAP_Delay
General Commands

Wait for specified delay. More...

Wait for specified delay.

The DAP_Delay< Command waits for a time period specified in micro-seconds.

DAP_Delay Command:

| BYTE | SHORT |
> 0x09 | Delay |
|******|*******|

- Delay: wait time in µs.

DAP_Delay Response:

| BYTE | BYTE |
< 0x09 | Status |
|******|********|

- Status: Response Status