CMSIS-DAP: Response Status

| CMSIS-DAP Version 1.2.0 (Proposal) Interface Firmware for CoreSight Debug Access Port

- Main Page
- Usage and Description
- Reference

All Functions Groups Pages
Response Status
CMSIS-DAP Commands

Status Information in Response Data. More...

Status Information in Response Data.

The Response data of a command frequently include a Status that indicates correct execution or command failures. Currently the following Status codes are returned:

- 0x00 = DAP_OK: Command has been successfully executed
- 0xFF = DAP_ERROR: Command did not execute due to communication failure with the device.