CMSIS-Driver: MCI Events

| CMSIS-Driver Version 2.05 Peripheral Interface for Middleware and Application Code

- Main Page
- Usage and Description
- Reference

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Macros
MCI Events
MCI Interface

The MCI driver generates call back events that are notified via the function ARM_MCI_SignalEvent. More...

## Macros
#define | ARM_MCI_EVENT_CARD_INSERTED (1UL << 0)
| Memory Card inserted. More...
#define | ARM_MCI_EVENT_CARD_REMOVED (1UL << 1)
| Memory Card removed. More...
#define | ARM_MCI_EVENT_COMMAND_COMPLETE (1UL << 2)
| Command completed. More...
#define | ARM_MCI_EVENT_COMMAND_TIMEOUT (1UL << 3)
| Command timeout. More...
#define | ARM_MCI_EVENT_COMMAND_ERROR (1UL << 4)
| Command response error (CRC error or invalid response) More...
#define | ARM_MCI_EVENT_TRANSFER_COMPLETE (1UL << 5)
| Data transfer completed. More...
#define | ARM_MCI_EVENT_TRANSFER_TIMEOUT (1UL << 6)
| Data transfer timeout. More...
#define | ARM_MCI_EVENT_TRANSFER_ERROR (1UL << 7)
| Data transfer CRC failed. More...
#define | ARM_MCI_EVENT_SDIO_INTERRUPT (1UL << 8)
| SD I/O Interrupt. More...
#define | ARM_MCI_EVENT_CCS (1UL << 9)
| Command Completion Signal (CCS) More...
#define | ARM_MCI_EVENT_CCS_TIMEOUT (1UL << 10)
| Command Completion Signal (CCS) Timeout. More...

## Description

The MCI driver generates call back events that are notified via the function ARM_MCI_SignalEvent.

This section provides the event values for the ARM_MCI_SignalEvent callback function.

The following call back notification events are generated:

## Macro Definition Documentation

#define ARM_MCI_EVENT_CARD_INSERTED (1UL << 0)

Memory Card inserted.

See Also
  ARM_MCI_SignalEvent

#define ARM_MCI_EVENT_CARD_REMOVED (1UL << 1)

Memory Card removed.

See Also
  ARM_MCI_SignalEvent

#define ARM_MCI_EVENT_COMMAND_COMPLETE (1UL << 2)

Command completed.

See Also
  ARM_MCI_SignalEvent

#define ARM_MCI_EVENT_COMMAND_TIMEOUT (1UL << 3)

Command timeout.

See Also
  ARM_MCI_SignalEvent

#define ARM_MCI_EVENT_COMMAND_ERROR (1UL << 4)

Command response error (CRC error or invalid response)

See Also
  ARM_MCI_SignalEvent

#define ARM_MCI_EVENT_TRANSFER_COMPLETE (1UL << 5)

Data transfer completed.

See Also
  ARM_MCI_SignalEvent

#define ARM_MCI_EVENT_TRANSFER_TIMEOUT (1UL << 6)

Data transfer timeout.

See Also
  ARM_MCI_SignalEvent

#define ARM_MCI_EVENT_TRANSFER_ERROR (1UL << 7)

Data transfer CRC failed.

See Also
  ARM_MCI_SignalEvent

#define ARM_MCI_EVENT_SDIO_INTERRUPT (1UL << 8)

SD I/O Interrupt.

See Also
  ARM_MCI_SignalEvent

#define ARM_MCI_EVENT_CCS (1UL << 9)

Command Completion Signal (CCS)

See Also
  ARM_MCI_SignalEvent

#define ARM_MCI_EVENT_CCS_TIMEOUT (1UL << 10)

Command Completion Signal (CCS) Timeout.

See Also
  ARM_MCI_SignalEvent