CMSIS-Core (Cortex-A): Auxiliary Control Register (ACTLR)

| CMSIS-Core (Cortex-A) Version 1.0.0 CMSIS-Core support for Cortex-A processor-based devices

- Main Page
- Usage and Description
- Reference

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Content | Data Structures | Functions
Auxiliary Control Register (ACTLR)
Core Register Access

The ACTLR provides IMPLEMENTATION DEFINED configuration and control options. More...

## Content
| ACTLR Bits
| Bit position and mask macros.

## Data Structures
struct | ACTLR_Type
| Bit field declaration for ACTLR layout. More...

## Functions
__STATIC_INLINE void | __set_ACTRL (uint32_t actrl)
| Set ACTRL (Auxiliary Control Register) More...
__STATIC_INLINE uint32_t | __get_ACTLR (void)
| Get ACTLR (Auxiliary Control Register) More...

## Description

The ACTLR characteristics are differs between various ARMv7-A implementations.

Cortex-A5

Bits | Name | Function
--- | --- | ---
[31:29] | - | Reserved.
[28] | DBDI | Disable Branch Dual Issue
[27:19] | - | Reserved.
[18] | BTDIS | Disable indirect Branch Target Address Cache (BTAC).
[17] | RSDIS | Disable return stack operation.
[16:15] | BP | Branch prediction policy.
[14:13] | L1PCTL | L1 Data prefetch control.
[12] | RADIS | Disable Data Cache read-allocate mode.
[11] | DWBST | Disable AXI data write bursts to Normal memory.
[10] | DODMBS | Disable optimized data memory barrier behavior.
[9:8] | - | Reserved.
[7] | EXCL | Exclusive L1/L2 cache control.
[6] | SMP | Enables coherent requests to the processor.
[5:1] | - | Reserved.
[0] | FW | Cache and TLB maintenance broadcast.

Cortex-A7

Bits | Name | Function
--- | --- | ---
[31:29] | - | Reserved.
[28] | DDI | Disable Dual Issue
[27:16] | - | Reserved.
[15] | DDVM | Disable Distributed Virtual Memory transactions.
[14:13] | L1PCTL | L1 Data prefetch control.
[12] | L1RADIS | L1 Data Cache read-allocate mode disable.
[11] | L2RADIS | L2 Data Cache read-allocate mode disable.
[10] | DODMBS | Disable optimized data memory barrier behavior.
[9:7] | - | Reserved.
[6] | SMP | Enables coherent requests to the processor.
[5:0] | - | Reserved.

Cortex-A9

Bits | Name | Function
--- | --- | ---
[31:10] | - | Reserved.
[9] | PARITY | Support for parity checking, if implemented.
[8] | AOW | Enable allocation in one cache way only.
[7] | EXCL | Exclusive L1/L2 cache control.
[6] | SMP | Enables coherent requests to the processor.
[5:4] | - | Reserved.
[3] | WFLZM | Enable write full line of zeros modea.
[2] | L1PE | Dside prefetch.
[1] | - | Reserved.
[0] | FW | Cache and TLB maintenance broadcast.

Consider using __get_ACTLR and __set_ACTRL to access ACTRL register.

## Function Documentation

__STATIC_INLINE uint32_t __get_ACTLR | ( | void |  | ) |

Returns
  Auxiliary Control Register value

This function returns the value of the Auxiliary Control Register (ACTLR).

__STATIC_INLINE void __set_ACTRL | ( | uint32_t | actrl | ) |

Parameters

  [in] | actrl | Auxiliary Control Register value to set

This function assigns the given value to the Auxiliary Control Register (ACTLR).