/* --------------------------------------------------------------------
 *  FMC
 * ---------------------------------------------------------------------*/

#define NUCODEGEN_FMC_UI                    0
#if (NUCODEGEN_FMC_UI)
 /* --------------------------------------------------------------------
 * IP UI configuration
 * ---------------------------------------------------------------------*/
#endif /* NUCODEGEN_FMC_UI */
 <!
 filter:{
         "M031_B": {
		              "APROM_SUPPORT":  "1",  "LDROM_SUPPORT":  "1",  "SPROM_SUPPORT":  "1",   "CONFIG_SUPPORT": "1"
				   },
				   
         "M031_C": {
		              "APROM_SUPPORT":  "1",  "LDROM_SUPPORT":  "1",  "SPROM_SUPPORT":  "1",   "CONFIG_SUPPORT": "1"
				   },
				   
         "M031_D": {
		              "APROM_SUPPORT":  "1",  "LDROM_SUPPORT":  "1",  "SPROM_SUPPORT":  "1",   "CONFIG_SUPPORT": "1"
				   },
				   
         "M031_E": {
		              "APROM_SUPPORT":  "1",  "LDROM_SUPPORT":  "1",  "SPROM_SUPPORT":  "1",   "CONFIG_SUPPORT": "1"
				   },	
	 "M031_I": {
		              "APROM_SUPPORT":  "1",  "LDROM_SUPPORT":  "1",  "SPROM_SUPPORT":  "1",   "CONFIG_SUPPORT": "1"
				   },
				   
         "M031_G": {
		              "APROM_SUPPORT":  "1",  "LDROM_SUPPORT":  "1",  "SPROM_SUPPORT":  "1",   "CONFIG_SUPPORT": "1"
				   },	
	 "M032_B": {
		              "APROM_SUPPORT":  "1",  "LDROM_SUPPORT":  "1",  "SPROM_SUPPORT":  "1",   "CONFIG_SUPPORT": "1"
				   },
				   
         "M032_C": {
		              "APROM_SUPPORT":  "1",  "LDROM_SUPPORT":  "1",  "SPROM_SUPPORT":  "1",   "CONFIG_SUPPORT": "1"
				   },
				   
         "M032_D": {
		              "APROM_SUPPORT":  "1",  "LDROM_SUPPORT":  "1",  "SPROM_SUPPORT":  "1",   "CONFIG_SUPPORT": "1"
				   },
				   
         "M032_E": {
		              "APROM_SUPPORT":  "1",  "LDROM_SUPPORT":  "1",  "SPROM_SUPPORT":  "1",   "CONFIG_SUPPORT": "1"
				   },	
	 "M032_I": {
		              "APROM_SUPPORT":  "1",  "LDROM_SUPPORT":  "1",  "SPROM_SUPPORT":  "1",   "CONFIG_SUPPORT": "1"
				   },
				   
         "M032_G": {
		              "APROM_SUPPORT":  "1",  "LDROM_SUPPORT":  "1",  "SPROM_SUPPORT":  "1",   "CONFIG_SUPPORT": "1"
				   }		   

        };!>

#if (NUCODEGEN_FMC_UI)
/* --------------------------------------------------------------------
 * FMC ISP & Flash update regions
 * ---------------------------------------------------------------------*/
#endif
#define NUCODEGEN_FMC_ISPEN                   <!id:NUCODEGENFMCIspEnBoolean;      type:checkbox;    label:FMC ISP enable.;                   data:1;         default:0;           enum:[1];    optionLabels:[<br>];        dependencies:none;     dependenciesOption:;     groupId:FMC;   groupName:FMC configuration;!>
#define NUCODEGEN_FMC_APROMEN                 <!id:NUCODEGENFMCApromMEnBoolean;   type:checkbox;    label:APROM update enable.;              data:1;         default:0;           enum:[1];    optionLabels:[<br>];        dependencies:none;     dependenciesOption:1;    groupId:FMC;   groupName:FMC configuration;    filterExp:APROM_SUPPORT>0;!>
#define NUCODEGEN_FMC_LDROMEN                 <!id:NUCODEGENFMCLdromEnBoolean;    type:checkbox;    label:LDROM update enable.;              data:1;         default:0;           enum:[1];    optionLabels:[<br>];        dependencies:none;     dependenciesOption:1;    groupId:FMC;   groupName:FMC configuration;    filterExp:LDROM_SUPPORT>0;!>
#define NUCODEGEN_FMC_SPROMEN                 <!id:NUCODEGENFMCSpromEnBoolean;    type:checkbox;    label:SPROM update enable.;              data:1;         default:0;           enum:[1];    optionLabels:[<br>];        dependencies:none;     dependenciesOption:1;    groupId:FMC;   groupName:FMC configuration;    filterExp:SPROM_SUPPORT>0;!>
#define NUCODEGEN_FMC_CONFIGEN                <!id:NUCODEGENFMCConfigEnBoolean;   type:checkbox;    label:CONFIG update enable.;             data:1;         default:0;           enum:[1];    optionLabels:[<br>];        dependencies:none;     dependenciesOption:1;    groupId:FMC;   groupName:FMC configuration;    filterExp:CONFIG_SUPPORT>0;!>