CMSIS-DSP: Linear Interpolate Example

| CMSIS-DSP Version 1.5.2 CMSIS DSP Software Library

- Main Page
- Usage and Description
- Reference

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Linear Interpolate Example
Examples

CMSIS DSP Software Library – Linear Interpolate Example

Description This example demonstrates usage of linear interpolate modules and fast math modules. Method 1 uses fast math sine function to calculate sine values using cubic interpolation and method 2 uses linear interpolation function and results are compared to reference output. Example shows linear interpolation function can be used to get higher precision compared to fast math sin calculation.

Block Diagram:

  Method 1: Sine caluclation using fast math

  Method 2: Sine caluclation using interpolation function

Variables Description:

  - `testInputSin_f32` points to the input values for sine calculation
  - `testRefSinOutput32_f32` points to the reference values caculated from sin() matlab function
  - `testOutput` points to output buffer calculation from cubic interpolation
  - `testLinIntOutput` points to output buffer calculation from linear interpolation
  - `snr1` Signal to noise ratio for reference and cubic interpolation output
  - `snr2` Signal to noise ratio for reference and linear interpolation output

CMSIS DSP Software Library Functions Used:

  - arm_sin_f32()
  - arm_linear_interp_f32()

Refer arm_linear_interp_example_f32.c