BLE_API v2.1.3

Macros
BLE SIG Defined Characteristic UUID Definitions
BLE Services » BLE UUIDs » BLE GATT Characteristic UUID Definitions

## Macros
#define | GATT_SPEC_CHARC_DEVICE_NAME 0x2A00
#define | GATT_SPEC_CHARC_APPEARANCE 0x2A01
#define | GATT_SPEC_CHARC_PERIPHERAL_PRIVACY_FLAG 0x2A02
#define | GATT_SPEC_CHARC_RECONNECTION_ADDRESS 0x2A03
#define | GATT_SPEC_CHARC_PERIPHERAL_PREFERRED_CONNECTION_PARAMETERS 0x2A04
#define | GATT_SPEC_CHARC_SERVICE_CHANGED 0x2A05
#define | GATT_SPEC_CHARC_ALERT_LEVEL 0x2A06
#define | GATT_SPEC_CHARC_TX_POWER_LEVEL 0x2A07
#define | GATT_SPEC_CHARC_DATE_TIME 0x2A08
#define | GATT_SPEC_CHARC_DAY_OF_WEEK 0x2A09
#define | GATT_SPEC_CHARC_DAY_DATE_TIME 0x2A0A
#define | GATT_SPEC_CHARC_EXACT_TIME_100 0x2A0B
#define | GATT_SPEC_CHARC_EXACT_TIME_256 0x2A0C
#define | GATT_SPEC_CHARC_DST_OFFSET 0x2A0D
#define | GATT_SPEC_CHARC_TIME_ZONE 0x2A0E
#define | GATT_SPEC_CHARC_LOCAL_TIME_INFORMATION 0x2A0F
#define | GATT_SPEC_CHARC_SECONDARY_TIME_ZONE 0x2A10
#define | GATT_SPEC_CHARC_TIME_WITH_DST 0x2A11
#define | GATT_SPEC_CHARC_TIME_ACCURACY 0x2A12
#define | GATT_SPEC_CHARC_TIME_SOURCE 0x2A13
#define | GATT_SPEC_CHARC_REFERENCE_TIME_INFORMATION 0x2A14
#define | GATT_SPEC_CHARC_TIME_BROADCAST 0x2A15
#define | GATT_SPEC_CHARC_TIME_UPDATE_CONTROL_POINT 0x2A16
#define | GATT_SPEC_CHARC_TIME_UPDATE_STATE 0x2A17
#define | GATT_SPEC_CHARC_GLUCOSE_MEASUREMENT 0x2A18
#define | GATT_SPEC_CHARC_BATTERY_LEVEL 0x2A19
#define | GATT_SPEC_CHARC_BATTERY_POWER_STATE 0x2A1A
#define | GATT_SPEC_CHARC_BATTERY_LEVEL_STATE 0x2A1B
#define | GATT_SPEC_CHARC_TEMPERATURE_MEASUREMENT 0x2A1C
#define | GATT_SPEC_CHARC_TEMPERATURE_TYPE 0x2A1D
#define | GATT_SPEC_CHARC_INTERMEDIATE_TEMPERATURE 0x2A1E
#define | GATT_SPEC_CHARC_TEMPERATURE_IN_CELSIUS 0x2A1F
#define | GATT_SPEC_CHARC_TEMPERATURE_IN_FAHRENHEIT 0x2A20
#define | GATT_SPEC_CHARC_MEASUREMENT_INTERVAL 0x2A21
#define | GATT_SPEC_CHARC_BOOT_KEYBOARD_INPUT_REPORT 0x2A22
#define | GATT_SPEC_CHARC_SYSTEM_ID 0x2A23
#define | GATT_SPEC_CHARC_MODEL_NUMBER_STRING 0x2A24
#define | GATT_SPEC_CHARC_SERIAL_NUMBER_STRING 0x2A25
#define | GATT_SPEC_CHARC_FIRMWARE_REVISION_STRING 0x2A26
#define | GATT_SPEC_CHARC_HARDWARE_REVISION_STRING 0x2A27
#define | GATT_SPEC_CHARC_SOFTWARE_REVISION_STRING 0x2A28
#define | GATT_SPEC_CHARC_MANUFACTURER_NAME_STRING 0x2A29
#define | GATT_SPEC_CHARC_IEEE_11073_REGULATORY_CERTIFICATION_DATA_LIST 0x2A2A
#define | GATT_SPEC_CHARC_CURRENT_TIME 0x2A2B
#define | GATT_SPEC_CHARC_SCAN_REFRESH 0x2A31
#define | GATT_SPEC_CHARC_BOOT_KEYBOARD_OUTPUT_REPORT 0x2A32
#define | GATT_SPEC_CHARC_BOOT_MOUSE_INPUT_REPORT 0x2A33
#define | GATT_SPEC_CHARC_GLUCOSE_MEASUREMENT_CONTEXT 0x2A34
#define | GATT_SPEC_CHARC_BLOOD_PRESSURE_MEASUREMENT 0x2A35
#define | GATT_SPEC_CHARC_INTERMEDIATE_CUFF_PRESSURE 0x2A36
#define | GATT_SPEC_CHARC_HEART_RATE_MEASUREMENT 0x2A37
#define | GATT_SPEC_CHARC_BODY_SENSOR_LOCATION 0x2A38
#define | GATT_SPEC_CHARC_HEART_RATE_CONTROL_POINT 0x2A39
#define | GATT_SPEC_CHARC_SCIENTIFIC_TEMPERATURE_IN_CELSIUS 0x2A3C
#define | GATT_SPEC_CHARC_STRING 0x2A3D
#define | GATT_SPEC_CHARC_NETWORK_AVAILABILITY 0x2A3E
#define | GATT_SPEC_CHARC_ALERT_STATUS 0x2A3F
#define | GATT_SPEC_CHARC_RINGER_CONTROL_POINT 0x2A40
#define | GATT_SPEC_CHARC_RINGER_SETTING 0x2A41
#define | GATT_SPEC_CHARC_ALERT_CATEGORY_ID_BIT_MASK 0x2A42
#define | GATT_SPEC_CHARC_ALERT_CATEGORY_ID 0x2A43
#define | GATT_SPEC_CHARC_ALERT_NOTIFICATION_CONTROL_POINT 0x2A44
#define | GATT_SPEC_CHARC_UNREAD_ALERT_STATUS 0x2A45
#define | GATT_SPEC_CHARC_NEW_ALERT 0x2A46
#define | GATT_SPEC_CHARC_SUPPORTED_NEW_ALERT_CATEGORY 0x2A47
#define | GATT_SPEC_CHARC_SUPPORTED_UNREAD_ALERT_CATEGORY 0x2A48
#define | GATT_SPEC_CHARC_BLOOD_PRESSURE_FEATURE 0x2A49
#define | GATT_SPEC_CHARC_HID_INFORMATION 0x2A4A
#define | GATT_SPEC_CHARC_REPORT_MAP 0x2A4B
#define | GATT_SPEC_CHARC_HID_CONTROL_POINT 0x2A4C
#define | GATT_SPEC_CHARC_REPORT 0x2A4D
#define | GATT_SPEC_CHARC_PROTOCOL_MODE 0x2A4E
#define | GATT_SPEC_CHARC_SCAN_INTERVAL_WINDOW 0x2A4F
#define | GATT_SPEC_CHARC_PNP_ID 0x2A50
#define | GATT_SPEC_CHARC_GLUCOSE_FEATURE 0x2A51
#define | GATT_SPEC_CHARC_RECORD_ACCESS_CONTROL_POINT 0x2A52
#define | GATT_SPEC_CHARC_RSC_MEASUREMENT 0x2A53
#define | GATT_SPEC_CHARC_RSC_FEATURE 0x2A54
#define | GATT_SPEC_CHARC_SC_CONTROL_POINT 0x2A55
#define | GATT_SPEC_CHARC_DIGITAL_INPUT 0x2A56
#define | GATT_SPEC_CHARC_DIGITAL_OUTPUT 0x2A57
#define | GATT_SPEC_CHARC_ANALOG_INPUT 0x2A58
#define | GATT_SPEC_CHARC_ANALOG_OUTPUT 0x2A59
#define | GATT_SPEC_CHARC_AGGREGATE_INPUT 0x2A5A
#define | GATT_SPEC_CHARC_CSC_MEASUREMENT 0x2A5B
#define | GATT_SPEC_CHARC_CSC_FEATURE 0x2A5C
#define | GATT_SPEC_CHARC_SENSOR_LOCATION 0x2A5D
#define | GATT_SPEC_CHARC_PULSE_OXIMETRY_CONTINUOUS_MEASUREMENT 0x2A5F
#define | GATT_SPEC_CHARC_CYCLING_POWER_MEASUREMENT 0x2A63
#define | GATT_SPEC_CHARC_CYCLING_POWER_VECTOR 0x2A64
#define | GATT_SPEC_CHARC_CYCLING_POWER_FEATURE 0x2A65
#define | GATT_SPEC_CHARC_CYCLING_POWER_CONTROL_POINT 0x2A66
#define | GATT_SPEC_CHARC_LOCATION_AND_SPEED 0x2A67
#define | GATT_SPEC_CHARC_NAVIGATION 0x2A68
#define | GATT_SPEC_CHARC_POSITION_QUALITY 0x2A69
#define | GATT_SPEC_CHARC_LN_FEATURE 0x2A6A
#define | GATT_SPEC_CHARC_LN_CONTROL_POINT 0x2A6B

## Detailed Description

BLE SIG defined characteristic UUID definitions.

Note
  https://www.bluetooth.com/specifications/gatt/characteristics/

## Macro Definition Documentation

## ◆ GATT_SPEC_CHARC_AGGREGATE_INPUT

#define GATT_SPEC_CHARC_AGGREGATE_INPUT 0x2A5A

Aggregate Input Characteristic UUID.

## ◆ GATT_SPEC_CHARC_ALERT_CATEGORY_ID

#define GATT_SPEC_CHARC_ALERT_CATEGORY_ID 0x2A43

Alert Category Id Characteristic UUID.

## ◆ GATT_SPEC_CHARC_ALERT_CATEGORY_ID_BIT_MASK

#define GATT_SPEC_CHARC_ALERT_CATEGORY_ID_BIT_MASK 0x2A42

Alert Category Id Bit Mask Characteristic UUID.

## ◆ GATT_SPEC_CHARC_ALERT_LEVEL

#define GATT_SPEC_CHARC_ALERT_LEVEL 0x2A06

Alert Level Characteristic UUID.

## ◆ GATT_SPEC_CHARC_ALERT_NOTIFICATION_CONTROL_POINT

#define GATT_SPEC_CHARC_ALERT_NOTIFICATION_CONTROL_POINT 0x2A44

Alert Notification Control Point Characteristic UUID.

## ◆ GATT_SPEC_CHARC_ALERT_STATUS

#define GATT_SPEC_CHARC_ALERT_STATUS 0x2A3F

Alert Status Characteristic UUID.

## ◆ GATT_SPEC_CHARC_ANALOG_INPUT

#define GATT_SPEC_CHARC_ANALOG_INPUT 0x2A58

Analog Input Characteristic UUID.

## ◆ GATT_SPEC_CHARC_ANALOG_OUTPUT

#define GATT_SPEC_CHARC_ANALOG_OUTPUT 0x2A59

Analog Output Characteristic UUID.

## ◆ GATT_SPEC_CHARC_APPEARANCE

#define GATT_SPEC_CHARC_APPEARANCE 0x2A01

Appearance Characteristic UUID.

## ◆ GATT_SPEC_CHARC_BATTERY_LEVEL

#define GATT_SPEC_CHARC_BATTERY_LEVEL 0x2A19

Battery Level Characteristic UUID.

## ◆ GATT_SPEC_CHARC_BATTERY_LEVEL_STATE

#define GATT_SPEC_CHARC_BATTERY_LEVEL_STATE 0x2A1B

Battery Level State Characteristic UUID.

## ◆ GATT_SPEC_CHARC_BATTERY_POWER_STATE

#define GATT_SPEC_CHARC_BATTERY_POWER_STATE 0x2A1A

Battery Power State Characteristic UUID.

## ◆ GATT_SPEC_CHARC_BLOOD_PRESSURE_FEATURE

#define GATT_SPEC_CHARC_BLOOD_PRESSURE_FEATURE 0x2A49

Blood Pressure Feature Characteristic UUID.

## ◆ GATT_SPEC_CHARC_BLOOD_PRESSURE_MEASUREMENT

#define GATT_SPEC_CHARC_BLOOD_PRESSURE_MEASUREMENT 0x2A35

Blood Pressure Measurement Characteristic UUID.

## ◆ GATT_SPEC_CHARC_BODY_SENSOR_LOCATION

#define GATT_SPEC_CHARC_BODY_SENSOR_LOCATION 0x2A38

Body Sensor Location Characteristic UUID.

## ◆ GATT_SPEC_CHARC_BOOT_KEYBOARD_INPUT_REPORT

#define GATT_SPEC_CHARC_BOOT_KEYBOARD_INPUT_REPORT 0x2A22

Boot Keyboard Input Report Characteristic UUID.

## ◆ GATT_SPEC_CHARC_BOOT_KEYBOARD_OUTPUT_REPORT

#define GATT_SPEC_CHARC_BOOT_KEYBOARD_OUTPUT_REPORT 0x2A32

Boot Keyboard Output Report Characteristic UUID.

## ◆ GATT_SPEC_CHARC_BOOT_MOUSE_INPUT_REPORT

#define GATT_SPEC_CHARC_BOOT_MOUSE_INPUT_REPORT 0x2A33

Boot Mouse Input Report Characteristic UUID.

## ◆ GATT_SPEC_CHARC_CSC_FEATURE

#define GATT_SPEC_CHARC_CSC_FEATURE 0x2A5C

Cycling Speed and Cadence Feature Characteristic UUID.

## ◆ GATT_SPEC_CHARC_CSC_MEASUREMENT

#define GATT_SPEC_CHARC_CSC_MEASUREMENT 0x2A5B

Cycling Speed and Cadence Measurement Characteristic UUID.

## ◆ GATT_SPEC_CHARC_CURRENT_TIME

#define GATT_SPEC_CHARC_CURRENT_TIME 0x2A2B

Current Time Characteristic UUID.

## ◆ GATT_SPEC_CHARC_CYCLING_POWER_CONTROL_POINT

#define GATT_SPEC_CHARC_CYCLING_POWER_CONTROL_POINT 0x2A66

Cycling Power Control Point Characteristic UUID.

## ◆ GATT_SPEC_CHARC_CYCLING_POWER_FEATURE

#define GATT_SPEC_CHARC_CYCLING_POWER_FEATURE 0x2A65

Cycling Power Feature Characteristic UUID.

## ◆ GATT_SPEC_CHARC_CYCLING_POWER_MEASUREMENT

#define GATT_SPEC_CHARC_CYCLING_POWER_MEASUREMENT 0x2A63

Cycling Power Measurement Characteristic UUID.

## ◆ GATT_SPEC_CHARC_CYCLING_POWER_VECTOR

#define GATT_SPEC_CHARC_CYCLING_POWER_VECTOR 0x2A64

Cycling Power Vector Characteristic UUID.

## ◆ GATT_SPEC_CHARC_DATE_TIME

#define GATT_SPEC_CHARC_DATE_TIME 0x2A08

Date Time Characteristic UUID.

## ◆ GATT_SPEC_CHARC_DAY_DATE_TIME

#define GATT_SPEC_CHARC_DAY_DATE_TIME 0x2A0A

Day Date Time Characteristic UUID.

## ◆ GATT_SPEC_CHARC_DAY_OF_WEEK

#define GATT_SPEC_CHARC_DAY_OF_WEEK 0x2A09

Day Of Week Characteristic UUID.

## ◆ GATT_SPEC_CHARC_DEVICE_NAME

#define GATT_SPEC_CHARC_DEVICE_NAME 0x2A00

Device Name Characteristic UUID.

## ◆ GATT_SPEC_CHARC_DIGITAL_INPUT

#define GATT_SPEC_CHARC_DIGITAL_INPUT 0x2A56

Digital Input Characteristic UUID.

## ◆ GATT_SPEC_CHARC_DIGITAL_OUTPUT

#define GATT_SPEC_CHARC_DIGITAL_OUTPUT 0x2A57

Digital Output Characteristic UUID.

## ◆ GATT_SPEC_CHARC_DST_OFFSET

#define GATT_SPEC_CHARC_DST_OFFSET 0x2A0D

Dst Offset Characteristic UUID.

## ◆ GATT_SPEC_CHARC_EXACT_TIME_100

#define GATT_SPEC_CHARC_EXACT_TIME_100 0x2A0B

Exact Time 100 Characteristic UUID.

## ◆ GATT_SPEC_CHARC_EXACT_TIME_256

#define GATT_SPEC_CHARC_EXACT_TIME_256 0x2A0C

Exact Time 256 Characteristic UUID.

## ◆ GATT_SPEC_CHARC_FIRMWARE_REVISION_STRING

#define GATT_SPEC_CHARC_FIRMWARE_REVISION_STRING 0x2A26

Firmware Revision String Characteristic UUID.

## ◆ GATT_SPEC_CHARC_GLUCOSE_FEATURE

#define GATT_SPEC_CHARC_GLUCOSE_FEATURE 0x2A51

Glucose Feature Characteristic UUID.

## ◆ GATT_SPEC_CHARC_GLUCOSE_MEASUREMENT

#define GATT_SPEC_CHARC_GLUCOSE_MEASUREMENT 0x2A18

Glucose Measurement Characteristic UUID.

## ◆ GATT_SPEC_CHARC_GLUCOSE_MEASUREMENT_CONTEXT

#define GATT_SPEC_CHARC_GLUCOSE_MEASUREMENT_CONTEXT 0x2A34

Glucose Measurement Context Characteristic UUID.

## ◆ GATT_SPEC_CHARC_HARDWARE_REVISION_STRING

#define GATT_SPEC_CHARC_HARDWARE_REVISION_STRING 0x2A27

Hardware Revision String Characteristic UUID.

## ◆ GATT_SPEC_CHARC_HEART_RATE_CONTROL_POINT

#define GATT_SPEC_CHARC_HEART_RATE_CONTROL_POINT 0x2A39

Heart Rate Control Point Characteristic UUID.

## ◆ GATT_SPEC_CHARC_HEART_RATE_MEASUREMENT

#define GATT_SPEC_CHARC_HEART_RATE_MEASUREMENT 0x2A37

Heart Rate Measurement Characteristic UUID.

## ◆ GATT_SPEC_CHARC_HID_CONTROL_POINT

#define GATT_SPEC_CHARC_HID_CONTROL_POINT 0x2A4C

Hid Control Point Characteristic UUID.

## ◆ GATT_SPEC_CHARC_HID_INFORMATION

#define GATT_SPEC_CHARC_HID_INFORMATION 0x2A4A

Hid Information Characteristic UUID.

## ◆ GATT_SPEC_CHARC_IEEE_11073_REGULATORY_CERTIFICATION_DATA_LIST

#define GATT_SPEC_CHARC_IEEE_11073_REGULATORY_CERTIFICATION_DATA_LIST 0x2A2A

IEEE Regulatory Certification Data List Characteristic UUID.

## ◆ GATT_SPEC_CHARC_INTERMEDIATE_CUFF_PRESSURE

#define GATT_SPEC_CHARC_INTERMEDIATE_CUFF_PRESSURE 0x2A36

Intermediate Cuff Pressure Characteristic UUID.

## ◆ GATT_SPEC_CHARC_INTERMEDIATE_TEMPERATURE

#define GATT_SPEC_CHARC_INTERMEDIATE_TEMPERATURE 0x2A1E

Intermediate Temperature Characteristic UUID.

## ◆ GATT_SPEC_CHARC_LN_CONTROL_POINT

#define GATT_SPEC_CHARC_LN_CONTROL_POINT 0x2A6B

Location Navigation Control point Characteristic UUID.

## ◆ GATT_SPEC_CHARC_LN_FEATURE

#define GATT_SPEC_CHARC_LN_FEATURE 0x2A6A

Location Navigation Feature Characteristic UUID.

## ◆ GATT_SPEC_CHARC_LOCAL_TIME_INFORMATION

#define GATT_SPEC_CHARC_LOCAL_TIME_INFORMATION 0x2A0F

Local Time Information Characteristic UUID.

## ◆ GATT_SPEC_CHARC_LOCATION_AND_SPEED

#define GATT_SPEC_CHARC_LOCATION_AND_SPEED 0x2A67

Location and Speed Characteristic UUID.

## ◆ GATT_SPEC_CHARC_MANUFACTURER_NAME_STRING

#define GATT_SPEC_CHARC_MANUFACTURER_NAME_STRING 0x2A29

Manufacturer Name String Characteristic UUID.

## ◆ GATT_SPEC_CHARC_MEASUREMENT_INTERVAL

#define GATT_SPEC_CHARC_MEASUREMENT_INTERVAL 0x2A21

Measurement Interval Characteristic UUID.

## ◆ GATT_SPEC_CHARC_MODEL_NUMBER_STRING

#define GATT_SPEC_CHARC_MODEL_NUMBER_STRING 0x2A24

Model Number String Characteristic UUID.

## ◆ GATT_SPEC_CHARC_NAVIGATION

#define GATT_SPEC_CHARC_NAVIGATION 0x2A68

Navigation Characteristic UUID.

## ◆ GATT_SPEC_CHARC_NETWORK_AVAILABILITY

#define GATT_SPEC_CHARC_NETWORK_AVAILABILITY 0x2A3E

Network Availability Characteristic UUID.

## ◆ GATT_SPEC_CHARC_NEW_ALERT

#define GATT_SPEC_CHARC_NEW_ALERT 0x2A46

New Alert Characteristic UUID.

## ◆ GATT_SPEC_CHARC_PERIPHERAL_PREFERRED_CONNECTION_PARAMETERS

#define GATT_SPEC_CHARC_PERIPHERAL_PREFERRED_CONNECTION_PARAMETERS 0x2A04

Peripheral Preferred Connection Parameters Characteristic UUID.

## ◆ GATT_SPEC_CHARC_PERIPHERAL_PRIVACY_FLAG

#define GATT_SPEC_CHARC_PERIPHERAL_PRIVACY_FLAG 0x2A02

Peripheral Privacy Flag Characteristic UUID.

## ◆ GATT_SPEC_CHARC_PNP_ID

#define GATT_SPEC_CHARC_PNP_ID 0x2A50

PnP Id Characteristic UUID.

## ◆ GATT_SPEC_CHARC_POSITION_QUALITY

#define GATT_SPEC_CHARC_POSITION_QUALITY 0x2A69

Position Quality Characteristic UUID.

## ◆ GATT_SPEC_CHARC_PROTOCOL_MODE

#define GATT_SPEC_CHARC_PROTOCOL_MODE 0x2A4E

Protocol Mode Characteristic UUID.

## ◆ GATT_SPEC_CHARC_PULSE_OXIMETRY_CONTINUOUS_MEASUREMENT

#define GATT_SPEC_CHARC_PULSE_OXIMETRY_CONTINUOUS_MEASUREMENT 0x2A5F

Pulse Oximetry Continuous Measurement Characteristic UUID.

## ◆ GATT_SPEC_CHARC_RECONNECTION_ADDRESS

#define GATT_SPEC_CHARC_RECONNECTION_ADDRESS 0x2A03

Reconnection Address Characteristic UUID.

## ◆ GATT_SPEC_CHARC_RECORD_ACCESS_CONTROL_POINT

#define GATT_SPEC_CHARC_RECORD_ACCESS_CONTROL_POINT 0x2A52

Record Access Control Point Characteristic UUID.

## ◆ GATT_SPEC_CHARC_REFERENCE_TIME_INFORMATION

#define GATT_SPEC_CHARC_REFERENCE_TIME_INFORMATION 0x2A14

Reference Time Information Characteristic UUID.

## ◆ GATT_SPEC_CHARC_REPORT

#define GATT_SPEC_CHARC_REPORT 0x2A4D

Report Characteristic UUID.

## ◆ GATT_SPEC_CHARC_REPORT_MAP

#define GATT_SPEC_CHARC_REPORT_MAP 0x2A4B

Report Map Characteristic UUID.

## ◆ GATT_SPEC_CHARC_RINGER_CONTROL_POINT

#define GATT_SPEC_CHARC_RINGER_CONTROL_POINT 0x2A40

Ringer Control Point Characteristic UUID.

## ◆ GATT_SPEC_CHARC_RINGER_SETTING

#define GATT_SPEC_CHARC_RINGER_SETTING 0x2A41

Ringer Setting Characteristic UUID.

## ◆ GATT_SPEC_CHARC_RSC_FEATURE

#define GATT_SPEC_CHARC_RSC_FEATURE 0x2A54

Running Speed and Cadence Feature Characteristic UUID.

## ◆ GATT_SPEC_CHARC_RSC_MEASUREMENT

#define GATT_SPEC_CHARC_RSC_MEASUREMENT 0x2A53

Running Speed and Cadence Measurement Characteristic UUID.

## ◆ GATT_SPEC_CHARC_SC_CONTROL_POINT

#define GATT_SPEC_CHARC_SC_CONTROL_POINT 0x2A55

Speed and Cadence Control Point Characteristic UUID.

## ◆ GATT_SPEC_CHARC_SCAN_INTERVAL_WINDOW

#define GATT_SPEC_CHARC_SCAN_INTERVAL_WINDOW 0x2A4F

Scan Interval Window Characteristic UUID.

## ◆ GATT_SPEC_CHARC_SCAN_REFRESH

#define GATT_SPEC_CHARC_SCAN_REFRESH 0x2A31

Scan Refresh Characteristic UUID.

## ◆ GATT_SPEC_CHARC_SCIENTIFIC_TEMPERATURE_IN_CELSIUS

#define GATT_SPEC_CHARC_SCIENTIFIC_TEMPERATURE_IN_CELSIUS 0x2A3C

Scientific Temperature in Celsius Characteristic UUID.

## ◆ GATT_SPEC_CHARC_SECONDARY_TIME_ZONE

#define GATT_SPEC_CHARC_SECONDARY_TIME_ZONE 0x2A10

Secondary Time Zone Characteristic UUID.

## ◆ GATT_SPEC_CHARC_SENSOR_LOCATION

#define GATT_SPEC_CHARC_SENSOR_LOCATION 0x2A5D

Sensor Location Characteristic UUID.

## ◆ GATT_SPEC_CHARC_SERIAL_NUMBER_STRING

#define GATT_SPEC_CHARC_SERIAL_NUMBER_STRING 0x2A25

Serial Number String Characteristic UUID.

## ◆ GATT_SPEC_CHARC_SERVICE_CHANGED

#define GATT_SPEC_CHARC_SERVICE_CHANGED 0x2A05

Service Changed Characteristic UUID.

## ◆ GATT_SPEC_CHARC_SOFTWARE_REVISION_STRING

#define GATT_SPEC_CHARC_SOFTWARE_REVISION_STRING 0x2A28

Software Revision String Characteristic UUID.

## ◆ GATT_SPEC_CHARC_STRING

#define GATT_SPEC_CHARC_STRING 0x2A3D

String Characteristic UUID.

## ◆ GATT_SPEC_CHARC_SUPPORTED_NEW_ALERT_CATEGORY

#define GATT_SPEC_CHARC_SUPPORTED_NEW_ALERT_CATEGORY 0x2A47

Supported New Alert Category Characteristic UUID.

## ◆ GATT_SPEC_CHARC_SUPPORTED_UNREAD_ALERT_CATEGORY

#define GATT_SPEC_CHARC_SUPPORTED_UNREAD_ALERT_CATEGORY 0x2A48

Supported Unread Alert Category Characteristic UUID.

## ◆ GATT_SPEC_CHARC_SYSTEM_ID

#define GATT_SPEC_CHARC_SYSTEM_ID 0x2A23

System Id Characteristic UUID.

## ◆ GATT_SPEC_CHARC_TEMPERATURE_IN_CELSIUS

#define GATT_SPEC_CHARC_TEMPERATURE_IN_CELSIUS 0x2A1F

Temperature in Celsius Characteristic UUID.

## ◆ GATT_SPEC_CHARC_TEMPERATURE_IN_FAHRENHEIT

#define GATT_SPEC_CHARC_TEMPERATURE_IN_FAHRENHEIT 0x2A20

Temperature in Fahrenheit Characteristic UUID.

## ◆ GATT_SPEC_CHARC_TEMPERATURE_MEASUREMENT

#define GATT_SPEC_CHARC_TEMPERATURE_MEASUREMENT 0x2A1C

Temperature Measurement Characteristic UUID.

## ◆ GATT_SPEC_CHARC_TEMPERATURE_TYPE

#define GATT_SPEC_CHARC_TEMPERATURE_TYPE 0x2A1D

Temperature Type Characteristic UUID.

## ◆ GATT_SPEC_CHARC_TIME_ACCURACY

#define GATT_SPEC_CHARC_TIME_ACCURACY 0x2A12

Time Accuracy Characteristic UUID.

## ◆ GATT_SPEC_CHARC_TIME_BROADCAST

#define GATT_SPEC_CHARC_TIME_BROADCAST 0x2A15

Time Broadcast Characteristic UUID.

## ◆ GATT_SPEC_CHARC_TIME_SOURCE

#define GATT_SPEC_CHARC_TIME_SOURCE 0x2A13

Time Source Characteristic UUID.

## ◆ GATT_SPEC_CHARC_TIME_UPDATE_CONTROL_POINT

#define GATT_SPEC_CHARC_TIME_UPDATE_CONTROL_POINT 0x2A16

Time Update Control Point Characteristic UUID.

## ◆ GATT_SPEC_CHARC_TIME_UPDATE_STATE

#define GATT_SPEC_CHARC_TIME_UPDATE_STATE 0x2A17

Update State Characteristic UUID.

## ◆ GATT_SPEC_CHARC_TIME_WITH_DST

#define GATT_SPEC_CHARC_TIME_WITH_DST 0x2A11

Time With Dst Characteristic UUID.

## ◆ GATT_SPEC_CHARC_TIME_ZONE

#define GATT_SPEC_CHARC_TIME_ZONE 0x2A0E

Time Zone Characteristic UUID.

## ◆ GATT_SPEC_CHARC_TX_POWER_LEVEL

#define GATT_SPEC_CHARC_TX_POWER_LEVEL 0x2A07

TX Power Level Characteristic UUID.

## ◆ GATT_SPEC_CHARC_UNREAD_ALERT_STATUS

#define GATT_SPEC_CHARC_UNREAD_ALERT_STATUS 0x2A45

Unread Alert Status Characteristic UUID.