BLE_API v2.1.3

BLE Address Type Definition
BLE Common » BLE Command Definition

## BleAddrType
Define different BLE address types.
typedef uint8_t | BleAddrType
#define | PUBLIC_ADDR 0x00
#define | RANDOM_ADDR 0x01
#define | PUBLIC_IDENTITY_ADDR 0x02
#define | RANDOM_IDENTITY_ADDR 0x03

## Detailed Description

BLE device address type.

## Macro Definition Documentation

## ◆ PUBLIC_ADDR

#define PUBLIC_ADDR 0x00

Public device address.

## ◆ PUBLIC_IDENTITY_ADDR

#define PUBLIC_IDENTITY_ADDR 0x02

Public identity address (corresponds to resolved private address).

## ◆ RANDOM_ADDR

#define RANDOM_ADDR 0x01

Random device address.

## ◆ RANDOM_IDENTITY_ADDR

#define RANDOM_IDENTITY_ADDR 0x03

Random (static) identity address (corresponds to resolved private address).