BLE_API v2.1.3

BLE Connection Event Status Definition
BLE Common » BLE Command Definition

## BleConnStatus
Define BLE connection event status.
typedef uint8_t | BleConnStatus
#define | COMMAND_SUCCESS 0x00
#define | COMMAND_DISALLOWED 0x0C
#define | COMMAND_REJECTED_DUE_TO_LIMITED_RESOURCES 0x0D
#define | COMMAND_ADVERTISING_TIMEOUT 0x3C

## Detailed Description

BLE connection event status definition.

## Macro Definition Documentation

## ◆ COMMAND_ADVERTISING_TIMEOUT

#define COMMAND_ADVERTISING_TIMEOUT 0x3C

Advertising timeout.

## ◆ COMMAND_DISALLOWED

#define COMMAND_DISALLOWED 0x0C

Disallowed.

## ◆ COMMAND_REJECTED_DUE_TO_LIMITED_RESOURCES

#define COMMAND_REJECTED_DUE_TO_LIMITED_RESOURCES 0x0D

Rejected due to the limited resources.

## ◆ COMMAND_SUCCESS

#define COMMAND_SUCCESS 0x00

Success.