BLE_API v2.1.3

BLE Phy Update Status Definition
BLE Common » BLE Command Definition

## BlePhyUpdateStatus
Define BLE Phy update status.
typedef uint8_t | BlePhyUpdateStatus
#define | PHY_UPDATE_SUCCESS 0x00
#define | PHY_UPDATE_REMOTE_FEATURE_UNSUPPORTED 0x1A
#define | PHY_UDDATE_TRANSACTION_COLLISION 0x2A

## Detailed Description

BLE Phy update status definition.

## Macro Definition Documentation

## ◆ PHY_UDDATE_TRANSACTION_COLLISION

#define PHY_UDDATE_TRANSACTION_COLLISION 0x2A

Command cancel due to transaction collision.

## ◆ PHY_UPDATE_REMOTE_FEATURE_UNSUPPORTED

#define PHY_UPDATE_REMOTE_FEATURE_UNSUPPORTED 0x1A

Command cancel due to remote feature unsupported.

## ◆ PHY_UPDATE_SUCCESS

#define PHY_UPDATE_SUCCESS 0x00

Success.