BLE_API v2.1.3

Macros
BLE GATT Service and Characteristic Definitions
BLE Services » BLE Defined-Services » BLE GATT Service Definitions » BLE GATT Application Definitions

## Macros
#define | BLESERVICE_GATT_SERVICE_CHANGED_INDICATE_EVENT 0x01
#define | BLESERVICE_GATT_SERVICE_CHANGED_CCCD_WRITE_EVENT 0x02
#define | BLESERVICE_GATT_SERVICE_CHANGED_CCCD_READ_EVENT 0x03
#define | BLESERVICE_GATT_SERVICE_CHANGED_CCCD_WRITE_RSP_EVENT 0x04

## Detailed Description

Here shows the event definitions of the GATT service.

## Macro Definition Documentation

## ◆ BLESERVICE_GATT_SERVICE_CHANGED_CCCD_READ_EVENT

#define BLESERVICE_GATT_SERVICE_CHANGED_CCCD_READ_EVENT 0x03

GATT characteristic service cahnged cccd read event.

## ◆ BLESERVICE_GATT_SERVICE_CHANGED_CCCD_WRITE_EVENT

#define BLESERVICE_GATT_SERVICE_CHANGED_CCCD_WRITE_EVENT 0x02

GATT characteristic service cahnged cccd write event.

## ◆ BLESERVICE_GATT_SERVICE_CHANGED_CCCD_WRITE_RSP_EVENT

#define BLESERVICE_GATT_SERVICE_CHANGED_CCCD_WRITE_RSP_EVENT 0x04

GATT characteristic service cahnged cccd write response event.

## ◆ BLESERVICE_GATT_SERVICE_CHANGED_INDICATE_EVENT

#define BLESERVICE_GATT_SERVICE_CHANGED_INDICATE_EVENT 0x01

GATT characteristic service cahnged indicate event.