BLE_API v2.1.3

BLE Connection Interval Definition
BLE Common » BLE Command Definition » BLE Connection Parameter Definition

## BleConnInt
Define BLE connection interval minimum and maximum.
typedef uint8_t | BleConnectionIntervalRange
#define | CONN_INTERVAL_MIN 0x0006
#define | CONN_INTERVAL_MAX 0x0C80

## Detailed Description

BLE connection interval range definition.

## Macro Definition Documentation

## ◆ CONN_INTERVAL_MAX

#define CONN_INTERVAL_MAX 0x0C80

The unit of connection interval is 1.25ms
Maximum connection interval is 4s = (0x0C80 * 1.25) ms

## ◆ CONN_INTERVAL_MIN

#define CONN_INTERVAL_MIN 0x0006

The unit of connection interval is 1.25ms
Minimum connection interval is 7.5ms = (0x0006 * 1.25) ms