BLE_API v2.1.3

BLE Connection Update Status Definition
BLE Common » BLE Command Definition

## BleConnUpdateStatus
Define BLE connection update status.
typedef uint8_t | BleConnUpdateStatus
#define | CMD_SUCCESS 0x00
#define | CMD_REJECTED 0x01
#define | CMD_TIMEOUT 0x02

## Detailed Description

BLE connection update status definition.

## Macro Definition Documentation

## ◆ CMD_REJECTED

#define CMD_REJECTED 0x01

Rejected.

## ◆ CMD_SUCCESS

#define CMD_SUCCESS 0x00

Success.

## ◆ CMD_TIMEOUT

#define CMD_TIMEOUT 0x02

Timeout.