BLE_API v2.1.3

Variables
BLE DIS UUID Definitions
BLE Services » BLE Defined-Services » BLE DIS Definitions

## Variables
const uint16_t | ATTR_UUID_DIS_PRIMARY_SERVICE []
const uint16_t | ATTR_UUID_DIS_CHARC_SERIAL_NUMBER_STRING []
const uint16_t | ATTR_UUID_DIS_CHARC_MANUFACTURER_NAME_STRING []
const uint16_t | ATTR_UUID_DIS_CHARC_SYSTEM_ID []
const uint16_t | ATTR_UUID_DIS_CHARC_FIRMWARE_REVISION_STRING []
const uint16_t | ATTR_UUID_DIS_CHARC_MODEL_NUMBER_STRING []
const uint16_t | ATTR_UUID_DIS_CHARC_HARDWARE_REVISION_STRING []
const uint16_t | ATTR_UUID_DIS_CHARC_SOFTWARE_REVISION_STRING []
const uint16_t | ATTR_UUID_DIS_CHARC_PNP_ID []

## Detailed Description

Here shows the definitions of the BLE DIS UUID Definitions.

## Variable Documentation

## ◆ ATTR_UUID_DIS_CHARC_FIRMWARE_REVISION_STRING

const uint16_t ATTR_UUID_DIS_CHARC_FIRMWARE_REVISION_STRING[]
| extern

DIS characteristic firmware revision string UUID.

## ◆ ATTR_UUID_DIS_CHARC_HARDWARE_REVISION_STRING

const uint16_t ATTR_UUID_DIS_CHARC_HARDWARE_REVISION_STRING[]
| extern

DIS characteristic hardware revision string UUID.

## ◆ ATTR_UUID_DIS_CHARC_MANUFACTURER_NAME_STRING

const uint16_t ATTR_UUID_DIS_CHARC_MANUFACTURER_NAME_STRING[]
| extern

DIS characteristic manufacturer name string UUID.

## ◆ ATTR_UUID_DIS_CHARC_MODEL_NUMBER_STRING

const uint16_t ATTR_UUID_DIS_CHARC_MODEL_NUMBER_STRING[]
| extern

DIS characteristic model number string UUID.

## ◆ ATTR_UUID_DIS_CHARC_PNP_ID

const uint16_t ATTR_UUID_DIS_CHARC_PNP_ID[]
| extern

DIS characteristic PnP ID UUID.

## ◆ ATTR_UUID_DIS_CHARC_SERIAL_NUMBER_STRING

const uint16_t ATTR_UUID_DIS_CHARC_SERIAL_NUMBER_STRING[]
| extern

DIS characteristic serial number string UUID.

## ◆ ATTR_UUID_DIS_CHARC_SOFTWARE_REVISION_STRING

const uint16_t ATTR_UUID_DIS_CHARC_SOFTWARE_REVISION_STRING[]
| extern

DIS characteristic software revision string UUID.

## ◆ ATTR_UUID_DIS_CHARC_SYSTEM_ID

const uint16_t ATTR_UUID_DIS_CHARC_SYSTEM_ID[]
| extern

DIS characteristic system ID UUID.

## ◆ ATTR_UUID_DIS_PRIMARY_SERVICE

const uint16_t ATTR_UUID_DIS_PRIMARY_SERVICE[]
| extern

DIS service UUID.