| MINI58_BSP V3.01.003 The Board Support Package for Mini58 Series MCU

Modules | Macros
Mini58 Peripheral Declaration
Mini58 Peripheral Memory Map
Collaboration diagram for Mini58 Peripheral Declaration:

## Modules
| Mini58 I/O Routines

## Macros
#define | WDT ((WDT_T *) WDT_BASE)
| Pointer to WDT register structure. More...
#define | WWDT ((WWDT_T *) WWDT_BASE)
| Pointer to WWDT register structure. More...
#define | TIMER0 ((TIMER_T *) TIMER0_BASE)
| Pointer to Timer 0 register structure. More...
#define | TIMER1 ((TIMER_T *) TIMER1_BASE)
| Pointer to Timer 1 register structure. More...
#define | I2C ((I2C_T *) I2C0_BASE)
| Pointer to I2C0 register structure. More...
#define | I2C0 ((I2C_T *) I2C0_BASE)
| Pointer to I2C0 register structure. More...
#define | I2C1 ((I2C_T *) I2C1_BASE)
| Pointer to I2C1 register structure. More...
#define | SPI ((SPI_T *) SPI_BASE)
| Pointer to SPI register structure. More...
#define | SPI0 ((SPI_T *) SPI_BASE)
| Pointer to SPI register structure. More...
#define | PWM ((PWM_T *) PWM_BASE)
| Pointer to PWM register structure. More...
#define | UART ((UART_T *) UART0_BASE)
| Pointer to UART0 register structure. More...
#define | UART0 ((UART_T *) UART0_BASE)
| Pointer to UART0 register structure. More...
#define | UART1 ((UART_T *) UART1_BASE)
| Pointer to UART1 register structure. More...
#define | ADC ((ADC_T *) ADC_BASE)
| Pointer to ADC register structure. More...
#define | ACMP ((ACMP_T *) ACMP_BASE)
| Pointer to ACMP register structure. More...
#define | SYS ((SYS_T *) SYS_BASE)
| Pointer to SYS register structure. More...
#define | CLK ((CLK_T *) CLK_BASE)
| Pointer to CLK register structure. More...
#define | INTR ((INTR_T *) INTR_BASE)
| Pointer to INT register structure. More...
#define | P0 ((GPIO_T *) P0_BASE)
| Pointer to GPIO port 0 register structure. More...
#define | P1 ((GPIO_T *) P1_BASE)
| Pointer to GPIO port 1 register structure. More...
#define | P2 ((GPIO_T *) P2_BASE)
| Pointer to GPIO port 2 register structure. More...
#define | P3 ((GPIO_T *) P3_BASE)
| Pointer to GPIO port 3 register structure. More...
#define | P4 ((GPIO_T *) P4_BASE)
| Pointer to GPIO port 4 register structure. More...
#define | P5 ((GPIO_T *) P5_BASE)
| Pointer to GPIO port 5 register structure. More...
#define | GPIO ((GPIO_DB_T *) GPIO_DBNCECON_BASE)
| Pointer to GPIO de-bounce register structure. More...
#define | FMC ((FMC_T *) FMC_BASE)
| Pointer to FMC register structure. More...

## Detailed Description

The Declaration of Mini58 Series Peripheral

## Macro Definition Documentation

## ◆ ACMP

#define ACMP ((ACMP_T *) ACMP_BASE)

Pointer to ACMP register structure.

Definition at line 11727 of file Mini58Series.h.

## ◆ ADC

#define ADC ((ADC_T *) ADC_BASE)

Pointer to ADC register structure.

Definition at line 11726 of file Mini58Series.h.

## ◆ CLK

#define CLK ((CLK_T *) CLK_BASE)

Pointer to CLK register structure.

Definition at line 11730 of file Mini58Series.h.

## ◆ FMC

#define FMC ((FMC_T *) FMC_BASE)

Pointer to FMC register structure.

Definition at line 11739 of file Mini58Series.h.

## ◆ GPIO

#define GPIO ((GPIO_DB_T *) GPIO_DBNCECON_BASE)

Pointer to GPIO de-bounce register structure.

Definition at line 11738 of file Mini58Series.h.

## ◆ I2C

#define I2C ((I2C_T *) I2C0_BASE)

Pointer to I2C0 register structure.

Definition at line 11717 of file Mini58Series.h.

## ◆ I2C0

#define I2C0 ((I2C_T *) I2C0_BASE)

Pointer to I2C0 register structure.

Definition at line 11718 of file Mini58Series.h.

## ◆ I2C1

#define I2C1 ((I2C_T *) I2C1_BASE)

Pointer to I2C1 register structure.

Definition at line 11719 of file Mini58Series.h.

## ◆ INTR

#define INTR ((INTR_T *) INTR_BASE)

Pointer to INT register structure.

Definition at line 11731 of file Mini58Series.h.

## ◆ P0

#define P0 ((GPIO_T *) P0_BASE)

Pointer to GPIO port 0 register structure.

Definition at line 11732 of file Mini58Series.h.

## ◆ P1

#define P1 ((GPIO_T *) P1_BASE)

Pointer to GPIO port 1 register structure.

Definition at line 11733 of file Mini58Series.h.

## ◆ P2

#define P2 ((GPIO_T *) P2_BASE)

Pointer to GPIO port 2 register structure.

Definition at line 11734 of file Mini58Series.h.

## ◆ P3

#define P3 ((GPIO_T *) P3_BASE)

Pointer to GPIO port 3 register structure.

Definition at line 11735 of file Mini58Series.h.

## ◆ P4

#define P4 ((GPIO_T *) P4_BASE)

Pointer to GPIO port 4 register structure.

Definition at line 11736 of file Mini58Series.h.

## ◆ P5

#define P5 ((GPIO_T *) P5_BASE)

Pointer to GPIO port 5 register structure.

Definition at line 11737 of file Mini58Series.h.

## ◆ PWM

#define PWM ((PWM_T *) PWM_BASE)

Pointer to PWM register structure.

Definition at line 11722 of file Mini58Series.h.

## ◆ SPI

#define SPI ((SPI_T *) SPI_BASE)

Pointer to SPI register structure.

Definition at line 11720 of file Mini58Series.h.

## ◆ SPI0

#define SPI0 ((SPI_T *) SPI_BASE)

Pointer to SPI register structure.

Definition at line 11721 of file Mini58Series.h.

## ◆ SYS

#define SYS ((SYS_T *) SYS_BASE)

Pointer to SYS register structure.

Definition at line 11729 of file Mini58Series.h.

## ◆ TIMER0

#define TIMER0 ((TIMER_T *) TIMER0_BASE)

Pointer to Timer 0 register structure.

Definition at line 11715 of file Mini58Series.h.

## ◆ TIMER1

#define TIMER1 ((TIMER_T *) TIMER1_BASE)

Pointer to Timer 1 register structure.

Definition at line 11716 of file Mini58Series.h.

## ◆ UART

#define UART ((UART_T *) UART0_BASE)

Pointer to UART0 register structure.

Definition at line 11723 of file Mini58Series.h.

## ◆ UART0

#define UART0 ((UART_T *) UART0_BASE)

Pointer to UART0 register structure.

Definition at line 11724 of file Mini58Series.h.

## ◆ UART1

#define UART1 ((UART_T *) UART1_BASE)

Pointer to UART1 register structure.

Definition at line 11725 of file Mini58Series.h.

## ◆ WDT

#define WDT ((WDT_T *) WDT_BASE)

Pointer to WDT register structure.

Definition at line 11713 of file Mini58Series.h.

## ◆ WWDT

#define WWDT ((WWDT_T *) WWDT_BASE)

Pointer to WWDT register structure.

Definition at line 11714 of file Mini58Series.h.