| NUC029FAE BSP V3.01.002 The Board Support Package for NUC029FAE

Data Fields
TIMER_T Struct Reference
NUC029FAE Control Register » Timer Controller(TIMER)

`#include <NUC029FAE.h>`

## Data Fields
__IO uint32_t | TCSR
__IO uint32_t | TCMPR
__IO uint32_t | TISR
__I uint32_t | TDR
__I uint32_t | TCAP
__IO uint32_t | TEXCON
__IO uint32_t | TEXISR

## Detailed Description

Definition at line 2759 of file NUC029FAE.h.

## Field Documentation

## ◆ TCAP

__I uint32_t TIMER_T::TCAP

Offset: 0x0010 Timer Capture Data Register

Definition at line 2765 of file NUC029FAE.h.

## ◆ TCMPR

__IO uint32_t TIMER_T::TCMPR

Offset: 0x0004 Timer Compare Register

Definition at line 2762 of file NUC029FAE.h.

## ◆ TCSR

__IO uint32_t TIMER_T::TCSR

Offset: 0x0000 Timer Control and Status Register

Definition at line 2761 of file NUC029FAE.h.

## ◆ TDR

__I uint32_t TIMER_T::TDR

Offset: 0x000C Timer Data Register

Definition at line 2764 of file NUC029FAE.h.

## ◆ TEXCON

__IO uint32_t TIMER_T::TEXCON

Offset: 0x0014 Timer External Control Register

Definition at line 2766 of file NUC029FAE.h.

## ◆ TEXISR

__IO uint32_t TIMER_T::TEXISR

Offset: 0x0018 Timer External Interrupt Status Register

Definition at line 2767 of file NUC029FAE.h.

## ◆ TISR

__IO uint32_t TIMER_T::TISR

Offset: 0x0008 Timer Interrupt Status Register

Definition at line 2763 of file NUC029FAE.h.

The documentation for this struct was generated from the following file:

- C:/Users/yachen/workzone/bsp/nuc029faebsp/Library/Device/Nuvoton/NUC029FAE/Include/NUC029FAE.h