| Nano100AN Series BSP V3.02.002 The Board Support Package for Nano100AN Series

Modules | Data Structures
NANO100 Definitions

## Modules
| Device CMSIS Definitions
| NANO100 Peripherals

## Data Structures
struct | CLK_T
#define | CLK_PWRCTL_HXT_EN_Pos (0)
#define | CLK_PWRCTL_HXT_EN_Msk (0x1ul << CLK_PWRCTL_HXT_EN_Pos)
#define | CLK_PWRCTL_LXT_EN_Pos (1)
#define | CLK_PWRCTL_LXT_EN_Msk (0x1ul << CLK_PWRCTL_LXT_EN_Pos)
#define | CLK_PWRCTL_HIRC_EN_Pos (2)
#define | CLK_PWRCTL_HIRC_EN_Msk (0x1ul << CLK_PWRCTL_HIRC_EN_Pos)
#define | CLK_PWRCTL_LIRC_EN_Pos (3)
#define | CLK_PWRCTL_LIRC_EN_Msk (0x1ul << CLK_PWRCTL_LIRC_EN_Pos)
#define | CLK_PWRCTL_WK_DLY_Pos (4)
#define | CLK_PWRCTL_WK_DLY_Msk (0x1ul << CLK_PWRCTL_WK_DLY_Pos)
#define | CLK_PWRCTL_PD_WK_IE_Pos (5)
#define | CLK_PWRCTL_PD_WK_IE_Msk (0x1ul << CLK_PWRCTL_PD_WK_IE_Pos)
#define | CLK_PWRCTL_PD_EN_Pos (6)
#define | CLK_PWRCTL_PD_EN_Msk (0x1ul << CLK_PWRCTL_PD_EN_Pos)
#define | CLK_PWRCTL_HXT_SELXT_Pos (8)
#define | CLK_PWRCTL_HXT_SELXT_Msk (0x1ul << CLK_PWRCTL_HXT_SELXT_Pos)
#define | CLK_PWRCTL_HXT_GAIN_Pos (9)
#define | CLK_PWRCTL_HXT_GAIN_Msk (0x1ul << CLK_PWRCTL_HXT_GAIN_Pos)
#define | CLK_PWRCTL_LXT_SCNT_Pos (10)
#define | CLK_PWRCTL_LXT_SCNT_Msk (0x1ul << CLK_PWRCTL_LXT_SCNT_Pos)
#define | CLK_AHBCLK_GPIO_EN_Pos (0)
#define | CLK_AHBCLK_GPIO_EN_Msk (0x1ul << CLK_AHBCLK_GPIO_EN_Pos)
#define | CLK_AHBCLK_DMA_EN_Pos (1)
#define | CLK_AHBCLK_DMA_EN_Msk (0x1ul << CLK_AHBCLK_DMA_EN_Pos)
#define | CLK_AHBCLK_ISP_EN_Pos (2)
#define | CLK_AHBCLK_ISP_EN_Msk (0x1ul << CLK_AHBCLK_ISP_EN_Pos)
#define | CLK_AHBCLK_EBI_EN_Pos (3)
#define | CLK_AHBCLK_EBI_EN_Msk (0x1ul << CLK_AHBCLK_EBI_EN_Pos)
#define | CLK_AHBCLK_SRAM_EN_Pos (4)
#define | CLK_AHBCLK_SRAM_EN_Msk (0x1ul << CLK_AHBCLK_SRAM_EN_Pos)
#define | CLK_AHBCLK_TICK_EN_Pos (5)
#define | CLK_AHBCLK_TICK_EN_Msk (0x1ul << CLK_AHBCLK_TICK_EN_Pos)
#define | CLK_APBCLK_WDT_EN_Pos (0)
#define | CLK_APBCLK_WDT_EN_Msk (0x1ul << CLK_APBCLK_WDT_EN_Pos)
#define | CLK_APBCLK_RTC_EN_Pos (1)
#define | CLK_APBCLK_RTC_EN_Msk (0x1ul << CLK_APBCLK_RTC_EN_Pos)
#define | CLK_APBCLK_TMR0_EN_Pos (2)
#define | CLK_APBCLK_TMR0_EN_Msk (0x1ul << CLK_APBCLK_TMR0_EN_Pos)
#define | CLK_APBCLK_TMR1_EN_Pos (3)
#define | CLK_APBCLK_TMR1_EN_Msk (0x1ul << CLK_APBCLK_TMR1_EN_Pos)
#define | CLK_APBCLK_TMR2_EN_Pos (4)
#define | CLK_APBCLK_TMR2_EN_Msk (0x1ul << CLK_APBCLK_TMR2_EN_Pos)
#define | CLK_APBCLK_TMR3_EN_Pos (5)
#define | CLK_APBCLK_TMR3_EN_Msk (0x1ul << CLK_APBCLK_TMR3_EN_Pos)
#define | CLK_APBCLK_FDIV_EN_Pos (6)
#define | CLK_APBCLK_FDIV_EN_Msk (0x1ul << CLK_APBCLK_FDIV_EN_Pos)
#define | CLK_APBCLK_I2C0_EN_Pos (8)
#define | CLK_APBCLK_I2C0_EN_Msk (0x1ul << CLK_APBCLK_I2C0_EN_Pos)
#define | CLK_APBCLK_I2C1_EN_Pos (9)
#define | CLK_APBCLK_I2C1_EN_Msk (0x1ul << CLK_APBCLK_I2C1_EN_Pos)
#define | CLK_APBCLK_SPI0_EN_Pos (12)
#define | CLK_APBCLK_SPI0_EN_Msk (0x1ul << CLK_APBCLK_SPI0_EN_Pos)
#define | CLK_APBCLK_SPI1_EN_Pos (13)
#define | CLK_APBCLK_SPI1_EN_Msk (0x1ul << CLK_APBCLK_SPI1_EN_Pos)
#define | CLK_APBCLK_SPI2_EN_Pos (14)
#define | CLK_APBCLK_SPI2_EN_Msk (0x1ul << CLK_APBCLK_SPI2_EN_Pos)
#define | CLK_APBCLK_UART0_EN_Pos (16)
#define | CLK_APBCLK_UART0_EN_Msk (0x1ul << CLK_APBCLK_UART0_EN_Pos)
#define | CLK_APBCLK_UART1_EN_Pos (17)
#define | CLK_APBCLK_UART1_EN_Msk (0x1ul << CLK_APBCLK_UART1_EN_Pos)
#define | CLK_APBCLK_PWM0_CH01_EN_Pos (20)
#define | CLK_APBCLK_PWM0_CH01_EN_Msk (0x1ul << CLK_APBCLK_PWM0_CH01_EN_Pos)
#define | CLK_APBCLK_PWM0_CH23_EN_Pos (21)
#define | CLK_APBCLK_PWM0_CH23_EN_Msk (0x1ul << CLK_APBCLK_PWM0_CH23_EN_Pos)
#define | CLK_APBCLK_PWM1_CH01_EN_Pos (22)
#define | CLK_APBCLK_PWM1_CH01_EN_Msk (0x1ul << CLK_APBCLK_PWM1_CH01_EN_Pos)
#define | CLK_APBCLK_PWM1_CH23_EN_Pos (23)
#define | CLK_APBCLK_PWM1_CH23_EN_Msk (0x1ul << CLK_APBCLK_PWM1_CH23_EN_Pos)
#define | CLK_APBCLK_USBD_EN_Pos (27)
#define | CLK_APBCLK_USBD_EN_Msk (0x1ul << CLK_APBCLK_USBD_EN_Pos)
#define | CLK_APBCLK_ADC_EN_Pos (28)
#define | CLK_APBCLK_ADC_EN_Msk (0x1ul << CLK_APBCLK_ADC_EN_Pos)
#define | CLK_APBCLK_I2S_EN_Pos (29)
#define | CLK_APBCLK_I2S_EN_Msk (0x1ul << CLK_APBCLK_I2S_EN_Pos)
#define | CLK_APBCLK_SC0_EN_Pos (30)
#define | CLK_APBCLK_SC0_EN_Msk (0x1ul << CLK_APBCLK_SC0_EN_Pos)
#define | CLK_APBCLK_SC1_EN_Pos (31)
#define | CLK_APBCLK_SC1_EN_Msk (0x1ul << CLK_APBCLK_SC1_EN_Pos)
#define | CLK_CLKSTATUS_HXT_STB_Pos (0)
#define | CLK_CLKSTATUS_HXT_STB_Msk (0x1ul << CLK_CLKSTATUS_HXT_STB_Pos)
#define | CLK_CLKSTATUS_LXT_STB_Pos (1)
#define | CLK_CLKSTATUS_LXT_STB_Msk (0x1ul << CLK_CLKSTATUS_LXT_STB_Pos)
#define | CLK_CLKSTATUS_PLL_STB_Pos (2)
#define | CLK_CLKSTATUS_PLL_STB_Msk (0x1ul << CLK_CLKSTATUS_PLL_STB_Pos)
#define | CLK_CLKSTATUS_LIRC_STB_Pos (3)
#define | CLK_CLKSTATUS_LIRC_STB_Msk (0x1ul << CLK_CLKSTATUS_LIRC_STB_Pos)
#define | CLK_CLKSTATUS_HIRC_STB_Pos (4)
#define | CLK_CLKSTATUS_HIRC_STB_Msk (0x1ul << CLK_CLKSTATUS_HIRC_STB_Pos)
#define | CLK_CLKSTATUS_CLK_SW_FAIL_Pos (7)
#define | CLK_CLKSTATUS_CLK_SW_FAIL_Msk (0x1ul << CLK_CLKSTATUS_CLK_SW_FAIL_Pos)
#define | CLK_CLKSEL0_HCLK_S_Pos (0)
#define | CLK_CLKSEL0_HCLK_S_Msk (0x7ul << CLK_CLKSEL0_HCLK_S_Pos)
#define | CLK_CLKSEL1_UART_S_Pos (0)
#define | CLK_CLKSEL1_UART_S_Msk (0x3ul << CLK_CLKSEL1_UART_S_Pos)
#define | CLK_CLKSEL1_ADC_S_Pos (2)
#define | CLK_CLKSEL1_ADC_S_Msk (0x3ul << CLK_CLKSEL1_ADC_S_Pos)
#define | CLK_CLKSEL1_PWM0_CH01_S_Pos (4)
#define | CLK_CLKSEL1_PWM0_CH01_S_Msk (0x3ul << CLK_CLKSEL1_PWM0_CH01_S_Pos)
#define | CLK_CLKSEL1_PWM0_CH23_S_Pos (6)
#define | CLK_CLKSEL1_PWM0_CH23_S_Msk (0x3ul << CLK_CLKSEL1_PWM0_CH23_S_Pos)
#define | CLK_CLKSEL1_TMR0_S_Pos (8)
#define | CLK_CLKSEL1_TMR0_S_Msk (0x7ul << CLK_CLKSEL1_TMR0_S_Pos)
#define | CLK_CLKSEL1_TMR1_S_Pos (12)
#define | CLK_CLKSEL1_TMR1_S_Msk (0x7ul << CLK_CLKSEL1_TMR1_S_Pos)
#define | CLK_CLKSEL2_FRQDIV_S_Pos (2)
#define | CLK_CLKSEL2_FRQDIV_S_Msk (0x3ul << CLK_CLKSEL2_FRQDIV_S_Pos)
#define | CLK_CLKSEL2_PWM1_CH01_S_Pos (4)
#define | CLK_CLKSEL2_PWM1_CH01_S_Msk (0x3ul << CLK_CLKSEL2_PWM1_CH01_S_Pos)
#define | CLK_CLKSEL2_PWM1_CH23_S_Pos (6)
#define | CLK_CLKSEL2_PWM1_CH23_S_Msk (0x3ul << CLK_CLKSEL2_PWM1_CH23_S_Pos)
#define | CLK_CLKSEL2_TMR2_S_Pos (8)
#define | CLK_CLKSEL2_TMR2_S_Msk (0x7ul << CLK_CLKSEL2_TMR2_S_Pos)
#define | CLK_CLKSEL2_TMR3_S_Pos (12)
#define | CLK_CLKSEL2_TMR3_S_Msk (0x7ul << CLK_CLKSEL2_TMR3_S_Pos)
#define | CLK_CLKSEL2_I2S_S_Pos (16)
#define | CLK_CLKSEL2_I2S_S_Msk (0x3ul << CLK_CLKSEL2_I2S_S_Pos)
#define | CLK_CLKSEL2_SC_S_Pos (18)
#define | CLK_CLKSEL2_SC_S_Msk (0x3ul << CLK_CLKSEL2_SC_S_Pos)
#define | CLK_CLKDIV0_HCLK_N_Pos (0)
#define | CLK_CLKDIV0_HCLK_N_Msk (0xful << CLK_CLKDIV0_HCLK_N_Pos)
#define | CLK_CLKDIV0_USB_N_Pos (4)
#define | CLK_CLKDIV0_USB_N_Msk (0xful << CLK_CLKDIV0_USB_N_Pos)
#define | CLK_CLKDIV0_UART_N_Pos (8)
#define | CLK_CLKDIV0_UART_N_Msk (0xful << CLK_CLKDIV0_UART_N_Pos)
#define | CLK_CLKDIV0_I2S_N_Pos (12)
#define | CLK_CLKDIV0_I2S_N_Msk (0xful << CLK_CLKDIV0_I2S_N_Pos)
#define | CLK_CLKDIV0_ADC_N_Pos (16)
#define | CLK_CLKDIV0_ADC_N_Msk (0xfful << CLK_CLKDIV0_ADC_N_Pos)
#define | CLK_CLKDIV0_SC0_N_Pos (28)
#define | CLK_CLKDIV0_SC0_N_Msk (0xful << CLK_CLKDIV0_SC0_N_Pos)
#define | CLK_CLKDIV1_SC1_N_Pos (0)
#define | CLK_CLKDIV1_SC1_N_Msk (0xful << CLK_CLKDIV1_SC1_N_Pos)
#define | CLK_PLLCTL_FB_DV_Pos (0)
#define | CLK_PLLCTL_FB_DV_Msk (0x3ful << CLK_PLLCTL_FB_DV_Pos)
#define | CLK_PLLCTL_IN_DV_Pos (8)
#define | CLK_PLLCTL_IN_DV_Msk (0x3ul << CLK_PLLCTL_IN_DV_Pos)
#define | CLK_PLLCTL_OUT_DV_Pos (12)
#define | CLK_PLLCTL_OUT_DV_Msk (0x1ul << CLK_PLLCTL_OUT_DV_Pos)
#define | CLK_PLLCTL_PD_Pos (16)
#define | CLK_PLLCTL_PD_Msk (0x1ul << CLK_PLLCTL_PD_Pos)
#define | CLK_PLLCTL_PLL_SRC_Pos (17)
#define | CLK_PLLCTL_PLL_SRC_Msk (0x1ul << CLK_PLLCTL_PLL_SRC_Pos)
#define | CLK_FRQDIV_FSEL_Pos (0)
#define | CLK_FRQDIV_FSEL_Msk (0xful << CLK_FRQDIV_FSEL_Pos)
#define | CLK_FRQDIV_FDIV_EN_Pos (4)
#define | CLK_FRQDIV_FDIV_EN_Msk (0x1ul << CLK_FRQDIV_FDIV_EN_Pos)
#define | CLK_PD_WK_IS_PD_WK_IS_Pos (0)
#define | CLK_PD_WK_IS_PD_WK_IS_Msk (0x1ul << CLK_PD_WK_IS_PD_WK_IS_Pos)

## Detailed Description

This file defines all structures and symbols for Nano100:

- interrupt numbers
- registers and bit fields
- peripheral base address
- peripheral ID
- Peripheral definitions

## Macro Definition Documentation

## ◆ CLK_AHBCLK_DMA_EN_Msk

#define CLK_AHBCLK_DMA_EN_Msk (0x1ul << CLK_AHBCLK_DMA_EN_Pos)

CLK_T::AHBCLK: DMA_EN Mask

Definition at line 1072 of file Nano100Series.h.

## ◆ CLK_AHBCLK_DMA_EN_Pos

#define CLK_AHBCLK_DMA_EN_Pos (1)

CLK_T::AHBCLK: DMA_EN Position

Definition at line 1071 of file Nano100Series.h.

## ◆ CLK_AHBCLK_EBI_EN_Msk

#define CLK_AHBCLK_EBI_EN_Msk (0x1ul << CLK_AHBCLK_EBI_EN_Pos)

CLK_T::AHBCLK: EBI_EN Mask

Definition at line 1078 of file Nano100Series.h.

## ◆ CLK_AHBCLK_EBI_EN_Pos

#define CLK_AHBCLK_EBI_EN_Pos (3)

CLK_T::AHBCLK: EBI_EN Position

Definition at line 1077 of file Nano100Series.h.

## ◆ CLK_AHBCLK_GPIO_EN_Msk

#define CLK_AHBCLK_GPIO_EN_Msk (0x1ul << CLK_AHBCLK_GPIO_EN_Pos)

CLK_T::AHBCLK: GPIO_EN Mask

Definition at line 1069 of file Nano100Series.h.

## ◆ CLK_AHBCLK_GPIO_EN_Pos

#define CLK_AHBCLK_GPIO_EN_Pos (0)

CLK_T::AHBCLK: GPIO_EN Position

Definition at line 1068 of file Nano100Series.h.

## ◆ CLK_AHBCLK_ISP_EN_Msk

#define CLK_AHBCLK_ISP_EN_Msk (0x1ul << CLK_AHBCLK_ISP_EN_Pos)

CLK_T::AHBCLK: ISP_EN Mask

Definition at line 1075 of file Nano100Series.h.

## ◆ CLK_AHBCLK_ISP_EN_Pos

#define CLK_AHBCLK_ISP_EN_Pos (2)

CLK_T::AHBCLK: ISP_EN Position

Definition at line 1074 of file Nano100Series.h.

## ◆ CLK_AHBCLK_SRAM_EN_Msk

#define CLK_AHBCLK_SRAM_EN_Msk (0x1ul << CLK_AHBCLK_SRAM_EN_Pos)

CLK_T::AHBCLK: SRAM_EN Mask

Definition at line 1081 of file Nano100Series.h.

## ◆ CLK_AHBCLK_SRAM_EN_Pos

#define CLK_AHBCLK_SRAM_EN_Pos (4)

CLK_T::AHBCLK: SRAM_EN Position

Definition at line 1080 of file Nano100Series.h.

## ◆ CLK_AHBCLK_TICK_EN_Msk

#define CLK_AHBCLK_TICK_EN_Msk (0x1ul << CLK_AHBCLK_TICK_EN_Pos)

CLK_T::AHBCLK: TICK_EN Mask

Definition at line 1084 of file Nano100Series.h.

## ◆ CLK_AHBCLK_TICK_EN_Pos

#define CLK_AHBCLK_TICK_EN_Pos (5)

CLK_T::AHBCLK: TICK_EN Position

Definition at line 1083 of file Nano100Series.h.

## ◆ CLK_APBCLK_ADC_EN_Msk

#define CLK_APBCLK_ADC_EN_Msk (0x1ul << CLK_APBCLK_ADC_EN_Pos)

CLK_T::APBCLK: ADC_EN Mask

Definition at line 1144 of file Nano100Series.h.

## ◆ CLK_APBCLK_ADC_EN_Pos

#define CLK_APBCLK_ADC_EN_Pos (28)

CLK_T::APBCLK: ADC_EN Position

Definition at line 1143 of file Nano100Series.h.

## ◆ CLK_APBCLK_FDIV_EN_Msk

#define CLK_APBCLK_FDIV_EN_Msk (0x1ul << CLK_APBCLK_FDIV_EN_Pos)

CLK_T::APBCLK: FDIV_EN Mask

Definition at line 1105 of file Nano100Series.h.

## ◆ CLK_APBCLK_FDIV_EN_Pos

#define CLK_APBCLK_FDIV_EN_Pos (6)

CLK_T::APBCLK: FDIV_EN Position

Definition at line 1104 of file Nano100Series.h.

## ◆ CLK_APBCLK_I2C0_EN_Msk

#define CLK_APBCLK_I2C0_EN_Msk (0x1ul << CLK_APBCLK_I2C0_EN_Pos)

CLK_T::APBCLK: I2C0_EN Mask

Definition at line 1108 of file Nano100Series.h.

## ◆ CLK_APBCLK_I2C0_EN_Pos

#define CLK_APBCLK_I2C0_EN_Pos (8)

CLK_T::APBCLK: I2C0_EN Position

Definition at line 1107 of file Nano100Series.h.

## ◆ CLK_APBCLK_I2C1_EN_Msk

#define CLK_APBCLK_I2C1_EN_Msk (0x1ul << CLK_APBCLK_I2C1_EN_Pos)

CLK_T::APBCLK: I2C1_EN Mask

Definition at line 1111 of file Nano100Series.h.

## ◆ CLK_APBCLK_I2C1_EN_Pos

#define CLK_APBCLK_I2C1_EN_Pos (9)

CLK_T::APBCLK: I2C1_EN Position

Definition at line 1110 of file Nano100Series.h.

## ◆ CLK_APBCLK_I2S_EN_Msk

#define CLK_APBCLK_I2S_EN_Msk (0x1ul << CLK_APBCLK_I2S_EN_Pos)

CLK_T::APBCLK: I2S_EN Mask

Definition at line 1147 of file Nano100Series.h.

## ◆ CLK_APBCLK_I2S_EN_Pos

#define CLK_APBCLK_I2S_EN_Pos (29)

CLK_T::APBCLK: I2S_EN Position

Definition at line 1146 of file Nano100Series.h.

## ◆ CLK_APBCLK_PWM0_CH01_EN_Msk

#define CLK_APBCLK_PWM0_CH01_EN_Msk (0x1ul << CLK_APBCLK_PWM0_CH01_EN_Pos)

CLK_T::APBCLK: PWM0_CH01_EN Mask

Definition at line 1129 of file Nano100Series.h.

## ◆ CLK_APBCLK_PWM0_CH01_EN_Pos

#define CLK_APBCLK_PWM0_CH01_EN_Pos (20)

CLK_T::APBCLK: PWM0_CH01_EN Position

Definition at line 1128 of file Nano100Series.h.

## ◆ CLK_APBCLK_PWM0_CH23_EN_Msk

#define CLK_APBCLK_PWM0_CH23_EN_Msk (0x1ul << CLK_APBCLK_PWM0_CH23_EN_Pos)

CLK_T::APBCLK: PWM0_CH23_EN Mask

Definition at line 1132 of file Nano100Series.h.

## ◆ CLK_APBCLK_PWM0_CH23_EN_Pos

#define CLK_APBCLK_PWM0_CH23_EN_Pos (21)

CLK_T::APBCLK: PWM0_CH23_EN Position

Definition at line 1131 of file Nano100Series.h.

## ◆ CLK_APBCLK_PWM1_CH01_EN_Msk

#define CLK_APBCLK_PWM1_CH01_EN_Msk (0x1ul << CLK_APBCLK_PWM1_CH01_EN_Pos)

CLK_T::APBCLK: PWM1_CH01_EN Mask

Definition at line 1135 of file Nano100Series.h.

## ◆ CLK_APBCLK_PWM1_CH01_EN_Pos

#define CLK_APBCLK_PWM1_CH01_EN_Pos (22)

CLK_T::APBCLK: PWM1_CH01_EN Position

Definition at line 1134 of file Nano100Series.h.

## ◆ CLK_APBCLK_PWM1_CH23_EN_Msk

#define CLK_APBCLK_PWM1_CH23_EN_Msk (0x1ul << CLK_APBCLK_PWM1_CH23_EN_Pos)

CLK_T::APBCLK: PWM1_CH23_EN Mask

Definition at line 1138 of file Nano100Series.h.

## ◆ CLK_APBCLK_PWM1_CH23_EN_Pos

#define CLK_APBCLK_PWM1_CH23_EN_Pos (23)

CLK_T::APBCLK: PWM1_CH23_EN Position

Definition at line 1137 of file Nano100Series.h.

## ◆ CLK_APBCLK_RTC_EN_Msk

#define CLK_APBCLK_RTC_EN_Msk (0x1ul << CLK_APBCLK_RTC_EN_Pos)

CLK_T::APBCLK: RTC_EN Mask

Definition at line 1090 of file Nano100Series.h.

## ◆ CLK_APBCLK_RTC_EN_Pos

#define CLK_APBCLK_RTC_EN_Pos (1)

CLK_T::APBCLK: RTC_EN Position

Definition at line 1089 of file Nano100Series.h.

## ◆ CLK_APBCLK_SC0_EN_Msk

#define CLK_APBCLK_SC0_EN_Msk (0x1ul << CLK_APBCLK_SC0_EN_Pos)

CLK_T::APBCLK: SC0_EN Mask

Definition at line 1150 of file Nano100Series.h.

## ◆ CLK_APBCLK_SC0_EN_Pos

#define CLK_APBCLK_SC0_EN_Pos (30)

CLK_T::APBCLK: SC0_EN Position

Definition at line 1149 of file Nano100Series.h.

## ◆ CLK_APBCLK_SC1_EN_Msk

#define CLK_APBCLK_SC1_EN_Msk (0x1ul << CLK_APBCLK_SC1_EN_Pos)

CLK_T::APBCLK: SC1_EN Mask

Definition at line 1153 of file Nano100Series.h.

## ◆ CLK_APBCLK_SC1_EN_Pos

#define CLK_APBCLK_SC1_EN_Pos (31)

CLK_T::APBCLK: SC1_EN Position

Definition at line 1152 of file Nano100Series.h.

## ◆ CLK_APBCLK_SPI0_EN_Msk

#define CLK_APBCLK_SPI0_EN_Msk (0x1ul << CLK_APBCLK_SPI0_EN_Pos)

CLK_T::APBCLK: SPI0_EN Mask

Definition at line 1114 of file Nano100Series.h.

## ◆ CLK_APBCLK_SPI0_EN_Pos

#define CLK_APBCLK_SPI0_EN_Pos (12)

CLK_T::APBCLK: SPI0_EN Position

Definition at line 1113 of file Nano100Series.h.

## ◆ CLK_APBCLK_SPI1_EN_Msk

#define CLK_APBCLK_SPI1_EN_Msk (0x1ul << CLK_APBCLK_SPI1_EN_Pos)

CLK_T::APBCLK: SPI1_EN Mask

Definition at line 1117 of file Nano100Series.h.

## ◆ CLK_APBCLK_SPI1_EN_Pos

#define CLK_APBCLK_SPI1_EN_Pos (13)

CLK_T::APBCLK: SPI1_EN Position

Definition at line 1116 of file Nano100Series.h.

## ◆ CLK_APBCLK_SPI2_EN_Msk

#define CLK_APBCLK_SPI2_EN_Msk (0x1ul << CLK_APBCLK_SPI2_EN_Pos)

CLK_T::APBCLK: SPI2_EN Mask

Definition at line 1120 of file Nano100Series.h.

## ◆ CLK_APBCLK_SPI2_EN_Pos

#define CLK_APBCLK_SPI2_EN_Pos (14)

CLK_T::APBCLK: SPI2_EN Position

Definition at line 1119 of file Nano100Series.h.

## ◆ CLK_APBCLK_TMR0_EN_Msk

#define CLK_APBCLK_TMR0_EN_Msk (0x1ul << CLK_APBCLK_TMR0_EN_Pos)

CLK_T::APBCLK: TMR0_EN Mask

Definition at line 1093 of file Nano100Series.h.

## ◆ CLK_APBCLK_TMR0_EN_Pos

#define CLK_APBCLK_TMR0_EN_Pos (2)

CLK_T::APBCLK: TMR0_EN Position

Definition at line 1092 of file Nano100Series.h.

## ◆ CLK_APBCLK_TMR1_EN_Msk

#define CLK_APBCLK_TMR1_EN_Msk (0x1ul << CLK_APBCLK_TMR1_EN_Pos)

CLK_T::APBCLK: TMR1_EN Mask

Definition at line 1096 of file Nano100Series.h.

## ◆ CLK_APBCLK_TMR1_EN_Pos

#define CLK_APBCLK_TMR1_EN_Pos (3)

CLK_T::APBCLK: TMR1_EN Position

Definition at line 1095 of file Nano100Series.h.

## ◆ CLK_APBCLK_TMR2_EN_Msk

#define CLK_APBCLK_TMR2_EN_Msk (0x1ul << CLK_APBCLK_TMR2_EN_Pos)

CLK_T::APBCLK: TMR2_EN Mask

Definition at line 1099 of file Nano100Series.h.

## ◆ CLK_APBCLK_TMR2_EN_Pos

#define CLK_APBCLK_TMR2_EN_Pos (4)

CLK_T::APBCLK: TMR2_EN Position

Definition at line 1098 of file Nano100Series.h.

## ◆ CLK_APBCLK_TMR3_EN_Msk

#define CLK_APBCLK_TMR3_EN_Msk (0x1ul << CLK_APBCLK_TMR3_EN_Pos)

CLK_T::APBCLK: TMR3_EN Mask

Definition at line 1102 of file Nano100Series.h.

## ◆ CLK_APBCLK_TMR3_EN_Pos

#define CLK_APBCLK_TMR3_EN_Pos (5)

CLK_T::APBCLK: TMR3_EN Position

Definition at line 1101 of file Nano100Series.h.

## ◆ CLK_APBCLK_UART0_EN_Msk

#define CLK_APBCLK_UART0_EN_Msk (0x1ul << CLK_APBCLK_UART0_EN_Pos)

CLK_T::APBCLK: UART0_EN Mask

Definition at line 1123 of file Nano100Series.h.

## ◆ CLK_APBCLK_UART0_EN_Pos

#define CLK_APBCLK_UART0_EN_Pos (16)

CLK_T::APBCLK: UART0_EN Position

Definition at line 1122 of file Nano100Series.h.

## ◆ CLK_APBCLK_UART1_EN_Msk

#define CLK_APBCLK_UART1_EN_Msk (0x1ul << CLK_APBCLK_UART1_EN_Pos)

CLK_T::APBCLK: UART1_EN Mask

Definition at line 1126 of file Nano100Series.h.

## ◆ CLK_APBCLK_UART1_EN_Pos

#define CLK_APBCLK_UART1_EN_Pos (17)

CLK_T::APBCLK: UART1_EN Position

Definition at line 1125 of file Nano100Series.h.

## ◆ CLK_APBCLK_USBD_EN_Msk

#define CLK_APBCLK_USBD_EN_Msk (0x1ul << CLK_APBCLK_USBD_EN_Pos)

CLK_T::APBCLK: USBD_EN Mask

Definition at line 1141 of file Nano100Series.h.

## ◆ CLK_APBCLK_USBD_EN_Pos

#define CLK_APBCLK_USBD_EN_Pos (27)

CLK_T::APBCLK: USBD_EN Position

Definition at line 1140 of file Nano100Series.h.

## ◆ CLK_APBCLK_WDT_EN_Msk

#define CLK_APBCLK_WDT_EN_Msk (0x1ul << CLK_APBCLK_WDT_EN_Pos)

CLK_T::APBCLK: WDT_EN Mask

Definition at line 1087 of file Nano100Series.h.

## ◆ CLK_APBCLK_WDT_EN_Pos

#define CLK_APBCLK_WDT_EN_Pos (0)

CLK_T::APBCLK: WDT_EN Position

Definition at line 1086 of file Nano100Series.h.

## ◆ CLK_CLKDIV0_ADC_N_Msk

#define CLK_CLKDIV0_ADC_N_Msk (0xfful << CLK_CLKDIV0_ADC_N_Pos)

CLK_T::CLKDIV0: ADC_N Mask

Definition at line 1228 of file Nano100Series.h.

## ◆ CLK_CLKDIV0_ADC_N_Pos

#define CLK_CLKDIV0_ADC_N_Pos (16)

CLK_T::CLKDIV0: ADC_N Position

Definition at line 1227 of file Nano100Series.h.

## ◆ CLK_CLKDIV0_HCLK_N_Msk

#define CLK_CLKDIV0_HCLK_N_Msk (0xful << CLK_CLKDIV0_HCLK_N_Pos)

CLK_T::CLKDIV0: HCLK_N Mask

Definition at line 1216 of file Nano100Series.h.

## ◆ CLK_CLKDIV0_HCLK_N_Pos

#define CLK_CLKDIV0_HCLK_N_Pos (0)

CLK_T::CLKDIV0: HCLK_N Position

Definition at line 1215 of file Nano100Series.h.

## ◆ CLK_CLKDIV0_I2S_N_Msk

#define CLK_CLKDIV0_I2S_N_Msk (0xful << CLK_CLKDIV0_I2S_N_Pos)

CLK_T::CLKDIV0: I2S_N Mask

Definition at line 1225 of file Nano100Series.h.

## ◆ CLK_CLKDIV0_I2S_N_Pos

#define CLK_CLKDIV0_I2S_N_Pos (12)

CLK_T::CLKDIV0: I2S_N Position

Definition at line 1224 of file Nano100Series.h.

## ◆ CLK_CLKDIV0_SC0_N_Msk

#define CLK_CLKDIV0_SC0_N_Msk (0xful << CLK_CLKDIV0_SC0_N_Pos)

CLK_T::CLKDIV0: SC0_N Mask

Definition at line 1231 of file Nano100Series.h.

## ◆ CLK_CLKDIV0_SC0_N_Pos

#define CLK_CLKDIV0_SC0_N_Pos (28)

CLK_T::CLKDIV0: SC0_N Position

Definition at line 1230 of file Nano100Series.h.

## ◆ CLK_CLKDIV0_UART_N_Msk

#define CLK_CLKDIV0_UART_N_Msk (0xful << CLK_CLKDIV0_UART_N_Pos)

CLK_T::CLKDIV0: UART_N Mask

Definition at line 1222 of file Nano100Series.h.

## ◆ CLK_CLKDIV0_UART_N_Pos

#define CLK_CLKDIV0_UART_N_Pos (8)

CLK_T::CLKDIV0: UART_N Position

Definition at line 1221 of file Nano100Series.h.

## ◆ CLK_CLKDIV0_USB_N_Msk

#define CLK_CLKDIV0_USB_N_Msk (0xful << CLK_CLKDIV0_USB_N_Pos)

CLK_T::CLKDIV0: USB_N Mask

Definition at line 1219 of file Nano100Series.h.

## ◆ CLK_CLKDIV0_USB_N_Pos

#define CLK_CLKDIV0_USB_N_Pos (4)

CLK_T::CLKDIV0: USB_N Position

Definition at line 1218 of file Nano100Series.h.

## ◆ CLK_CLKDIV1_SC1_N_Msk

#define CLK_CLKDIV1_SC1_N_Msk (0xful << CLK_CLKDIV1_SC1_N_Pos)

CLK_T::CLKDIV1: SC1_N Mask

Definition at line 1234 of file Nano100Series.h.

## ◆ CLK_CLKDIV1_SC1_N_Pos

#define CLK_CLKDIV1_SC1_N_Pos (0)

CLK_T::CLKDIV1: SC1_N Position

Definition at line 1233 of file Nano100Series.h.

## ◆ CLK_CLKSEL0_HCLK_S_Msk

#define CLK_CLKSEL0_HCLK_S_Msk (0x7ul << CLK_CLKSEL0_HCLK_S_Pos)

CLK_T::CLKSEL0: HCLK_S Mask

Definition at line 1174 of file Nano100Series.h.

## ◆ CLK_CLKSEL0_HCLK_S_Pos

#define CLK_CLKSEL0_HCLK_S_Pos (0)

CLK_T::CLKSEL0: HCLK_S Position

Definition at line 1173 of file Nano100Series.h.

## ◆ CLK_CLKSEL1_ADC_S_Msk

#define CLK_CLKSEL1_ADC_S_Msk (0x3ul << CLK_CLKSEL1_ADC_S_Pos)

CLK_T::CLKSEL1: ADC_S Mask

Definition at line 1180 of file Nano100Series.h.

## ◆ CLK_CLKSEL1_ADC_S_Pos

#define CLK_CLKSEL1_ADC_S_Pos (2)

CLK_T::CLKSEL1: ADC_S Position

Definition at line 1179 of file Nano100Series.h.

## ◆ CLK_CLKSEL1_PWM0_CH01_S_Msk

#define CLK_CLKSEL1_PWM0_CH01_S_Msk (0x3ul << CLK_CLKSEL1_PWM0_CH01_S_Pos)

CLK_T::CLKSEL1: PWM0_CH01_S Mask

Definition at line 1183 of file Nano100Series.h.

## ◆ CLK_CLKSEL1_PWM0_CH01_S_Pos

#define CLK_CLKSEL1_PWM0_CH01_S_Pos (4)

CLK_T::CLKSEL1: PWM0_CH01_S Position

Definition at line 1182 of file Nano100Series.h.

## ◆ CLK_CLKSEL1_PWM0_CH23_S_Msk

#define CLK_CLKSEL1_PWM0_CH23_S_Msk (0x3ul << CLK_CLKSEL1_PWM0_CH23_S_Pos)

CLK_T::CLKSEL1: PWM0_CH23_S Mask

Definition at line 1186 of file Nano100Series.h.

## ◆ CLK_CLKSEL1_PWM0_CH23_S_Pos

#define CLK_CLKSEL1_PWM0_CH23_S_Pos (6)

CLK_T::CLKSEL1: PWM0_CH23_S Position

Definition at line 1185 of file Nano100Series.h.

## ◆ CLK_CLKSEL1_TMR0_S_Msk

#define CLK_CLKSEL1_TMR0_S_Msk (0x7ul << CLK_CLKSEL1_TMR0_S_Pos)

CLK_T::CLKSEL1: TMR0_S Mask

Definition at line 1189 of file Nano100Series.h.

## ◆ CLK_CLKSEL1_TMR0_S_Pos

#define CLK_CLKSEL1_TMR0_S_Pos (8)

CLK_T::CLKSEL1: TMR0_S Position

Definition at line 1188 of file Nano100Series.h.

## ◆ CLK_CLKSEL1_TMR1_S_Msk

#define CLK_CLKSEL1_TMR1_S_Msk (0x7ul << CLK_CLKSEL1_TMR1_S_Pos)

CLK_T::CLKSEL1: TMR1_S Mask

Definition at line 1192 of file Nano100Series.h.

## ◆ CLK_CLKSEL1_TMR1_S_Pos

#define CLK_CLKSEL1_TMR1_S_Pos (12)

CLK_T::CLKSEL1: TMR1_S Position

Definition at line 1191 of file Nano100Series.h.

## ◆ CLK_CLKSEL1_UART_S_Msk

#define CLK_CLKSEL1_UART_S_Msk (0x3ul << CLK_CLKSEL1_UART_S_Pos)

CLK_T::CLKSEL1: UART_S Mask

Definition at line 1177 of file Nano100Series.h.

## ◆ CLK_CLKSEL1_UART_S_Pos

#define CLK_CLKSEL1_UART_S_Pos (0)

CLK_T::CLKSEL1: UART_S Position

Definition at line 1176 of file Nano100Series.h.

## ◆ CLK_CLKSEL2_FRQDIV_S_Msk

#define CLK_CLKSEL2_FRQDIV_S_Msk (0x3ul << CLK_CLKSEL2_FRQDIV_S_Pos)

CLK_T::CLKSEL2: FRQDIV_S Mask

Definition at line 1195 of file Nano100Series.h.

## ◆ CLK_CLKSEL2_FRQDIV_S_Pos

#define CLK_CLKSEL2_FRQDIV_S_Pos (2)

CLK_T::CLKSEL2: FRQDIV_S Position

Definition at line 1194 of file Nano100Series.h.

## ◆ CLK_CLKSEL2_I2S_S_Msk

#define CLK_CLKSEL2_I2S_S_Msk (0x3ul << CLK_CLKSEL2_I2S_S_Pos)

CLK_T::CLKSEL2: I2S_S Mask

Definition at line 1210 of file Nano100Series.h.

## ◆ CLK_CLKSEL2_I2S_S_Pos

#define CLK_CLKSEL2_I2S_S_Pos (16)

CLK_T::CLKSEL2: I2S_S Position

Definition at line 1209 of file Nano100Series.h.

## ◆ CLK_CLKSEL2_PWM1_CH01_S_Msk

#define CLK_CLKSEL2_PWM1_CH01_S_Msk (0x3ul << CLK_CLKSEL2_PWM1_CH01_S_Pos)

CLK_T::CLKSEL2: PWM1_CH01_S Mask

Definition at line 1198 of file Nano100Series.h.

## ◆ CLK_CLKSEL2_PWM1_CH01_S_Pos

#define CLK_CLKSEL2_PWM1_CH01_S_Pos (4)

CLK_T::CLKSEL2: PWM1_CH01_S Position

Definition at line 1197 of file Nano100Series.h.

## ◆ CLK_CLKSEL2_PWM1_CH23_S_Msk

#define CLK_CLKSEL2_PWM1_CH23_S_Msk (0x3ul << CLK_CLKSEL2_PWM1_CH23_S_Pos)

CLK_T::CLKSEL2: PWM1_CH23_S Mask

Definition at line 1201 of file Nano100Series.h.

## ◆ CLK_CLKSEL2_PWM1_CH23_S_Pos

#define CLK_CLKSEL2_PWM1_CH23_S_Pos (6)

CLK_T::CLKSEL2: PWM1_CH23_S Position

Definition at line 1200 of file Nano100Series.h.

## ◆ CLK_CLKSEL2_SC_S_Msk

#define CLK_CLKSEL2_SC_S_Msk (0x3ul << CLK_CLKSEL2_SC_S_Pos)

CLK_T::CLKSEL2: SC_S Mask

Definition at line 1213 of file Nano100Series.h.

## ◆ CLK_CLKSEL2_SC_S_Pos

#define CLK_CLKSEL2_SC_S_Pos (18)

CLK_T::CLKSEL2: SC_S Position

Definition at line 1212 of file Nano100Series.h.

## ◆ CLK_CLKSEL2_TMR2_S_Msk

#define CLK_CLKSEL2_TMR2_S_Msk (0x7ul << CLK_CLKSEL2_TMR2_S_Pos)

CLK_T::CLKSEL2: TMR2_S Mask

Definition at line 1204 of file Nano100Series.h.

## ◆ CLK_CLKSEL2_TMR2_S_Pos

#define CLK_CLKSEL2_TMR2_S_Pos (8)

CLK_T::CLKSEL2: TMR2_S Position

Definition at line 1203 of file Nano100Series.h.

## ◆ CLK_CLKSEL2_TMR3_S_Msk

#define CLK_CLKSEL2_TMR3_S_Msk (0x7ul << CLK_CLKSEL2_TMR3_S_Pos)

CLK_T::CLKSEL2: TMR3_S Mask

Definition at line 1207 of file Nano100Series.h.

## ◆ CLK_CLKSEL2_TMR3_S_Pos

#define CLK_CLKSEL2_TMR3_S_Pos (12)

CLK_T::CLKSEL2: TMR3_S Position

Definition at line 1206 of file Nano100Series.h.

## ◆ CLK_CLKSTATUS_CLK_SW_FAIL_Msk

#define CLK_CLKSTATUS_CLK_SW_FAIL_Msk (0x1ul << CLK_CLKSTATUS_CLK_SW_FAIL_Pos)

CLK_T::CLKSTATUS: CLK_SW_FAIL Mask

Definition at line 1171 of file Nano100Series.h.

## ◆ CLK_CLKSTATUS_CLK_SW_FAIL_Pos

#define CLK_CLKSTATUS_CLK_SW_FAIL_Pos (7)

CLK_T::CLKSTATUS: CLK_SW_FAIL Position

Definition at line 1170 of file Nano100Series.h.

## ◆ CLK_CLKSTATUS_HIRC_STB_Msk

#define CLK_CLKSTATUS_HIRC_STB_Msk (0x1ul << CLK_CLKSTATUS_HIRC_STB_Pos)

CLK_T::CLKSTATUS: HIRC_STB Mask

Definition at line 1168 of file Nano100Series.h.

## ◆ CLK_CLKSTATUS_HIRC_STB_Pos

#define CLK_CLKSTATUS_HIRC_STB_Pos (4)

CLK_T::CLKSTATUS: HIRC_STB Position

Definition at line 1167 of file Nano100Series.h.

## ◆ CLK_CLKSTATUS_HXT_STB_Msk

#define CLK_CLKSTATUS_HXT_STB_Msk (0x1ul << CLK_CLKSTATUS_HXT_STB_Pos)

CLK_T::CLKSTATUS: HXT_STB Mask

Definition at line 1156 of file Nano100Series.h.

## ◆ CLK_CLKSTATUS_HXT_STB_Pos

#define CLK_CLKSTATUS_HXT_STB_Pos (0)

CLK_T::CLKSTATUS: HXT_STB Position

Definition at line 1155 of file Nano100Series.h.

## ◆ CLK_CLKSTATUS_LIRC_STB_Msk

#define CLK_CLKSTATUS_LIRC_STB_Msk (0x1ul << CLK_CLKSTATUS_LIRC_STB_Pos)

CLK_T::CLKSTATUS: LIRC_STB Mask

Definition at line 1165 of file Nano100Series.h.

## ◆ CLK_CLKSTATUS_LIRC_STB_Pos

#define CLK_CLKSTATUS_LIRC_STB_Pos (3)

CLK_T::CLKSTATUS: LIRC_STB Position

Definition at line 1164 of file Nano100Series.h.

## ◆ CLK_CLKSTATUS_LXT_STB_Msk

#define CLK_CLKSTATUS_LXT_STB_Msk (0x1ul << CLK_CLKSTATUS_LXT_STB_Pos)

CLK_T::CLKSTATUS: LXT_STB Mask

Definition at line 1159 of file Nano100Series.h.

## ◆ CLK_CLKSTATUS_LXT_STB_Pos

#define CLK_CLKSTATUS_LXT_STB_Pos (1)

CLK_T::CLKSTATUS: LXT_STB Position

Definition at line 1158 of file Nano100Series.h.

## ◆ CLK_CLKSTATUS_PLL_STB_Msk

#define CLK_CLKSTATUS_PLL_STB_Msk (0x1ul << CLK_CLKSTATUS_PLL_STB_Pos)

CLK_T::CLKSTATUS: PLL_STB Mask

Definition at line 1162 of file Nano100Series.h.

## ◆ CLK_CLKSTATUS_PLL_STB_Pos

#define CLK_CLKSTATUS_PLL_STB_Pos (2)

CLK_T::CLKSTATUS: PLL_STB Position

Definition at line 1161 of file Nano100Series.h.

## ◆ CLK_FRQDIV_FDIV_EN_Msk

#define CLK_FRQDIV_FDIV_EN_Msk (0x1ul << CLK_FRQDIV_FDIV_EN_Pos)

CLK_T::FRQDIV: FDIV_EN Mask

Definition at line 1255 of file Nano100Series.h.

## ◆ CLK_FRQDIV_FDIV_EN_Pos

#define CLK_FRQDIV_FDIV_EN_Pos (4)

CLK_T::FRQDIV: FDIV_EN Position

Definition at line 1254 of file Nano100Series.h.

## ◆ CLK_FRQDIV_FSEL_Msk

#define CLK_FRQDIV_FSEL_Msk (0xful << CLK_FRQDIV_FSEL_Pos)

CLK_T::FRQDIV: FSEL Mask

Definition at line 1252 of file Nano100Series.h.

## ◆ CLK_FRQDIV_FSEL_Pos

#define CLK_FRQDIV_FSEL_Pos (0)

CLK_T::FRQDIV: FSEL Position

Definition at line 1251 of file Nano100Series.h.

## ◆ CLK_PD_WK_IS_PD_WK_IS_Msk

#define CLK_PD_WK_IS_PD_WK_IS_Msk (0x1ul << CLK_PD_WK_IS_PD_WK_IS_Pos)

CLK_T::WK_IS: PD_WK_IS Mask

Definition at line 1258 of file Nano100Series.h.

## ◆ CLK_PD_WK_IS_PD_WK_IS_Pos

#define CLK_PD_WK_IS_PD_WK_IS_Pos (0)

CLK_T::WK_IS: PD_WK_IS Position

Definition at line 1257 of file Nano100Series.h.

## ◆ CLK_PLLCTL_FB_DV_Msk

#define CLK_PLLCTL_FB_DV_Msk (0x3ful << CLK_PLLCTL_FB_DV_Pos)

CLK_T::PLLCTL: FB_DV Mask

Definition at line 1237 of file Nano100Series.h.

## ◆ CLK_PLLCTL_FB_DV_Pos

#define CLK_PLLCTL_FB_DV_Pos (0)

CLK_T::PLLCTL: FB_DV Position

Definition at line 1236 of file Nano100Series.h.

## ◆ CLK_PLLCTL_IN_DV_Msk

#define CLK_PLLCTL_IN_DV_Msk (0x3ul << CLK_PLLCTL_IN_DV_Pos)

CLK_T::PLLCTL: IN_DV Mask

Definition at line 1240 of file Nano100Series.h.

## ◆ CLK_PLLCTL_IN_DV_Pos

#define CLK_PLLCTL_IN_DV_Pos (8)

CLK_T::PLLCTL: IN_DV Position

Definition at line 1239 of file Nano100Series.h.

## ◆ CLK_PLLCTL_OUT_DV_Msk

#define CLK_PLLCTL_OUT_DV_Msk (0x1ul << CLK_PLLCTL_OUT_DV_Pos)

CLK_T::PLLCTL: OUT_DV Mask

Definition at line 1243 of file Nano100Series.h.

## ◆ CLK_PLLCTL_OUT_DV_Pos

#define CLK_PLLCTL_OUT_DV_Pos (12)

CLK_T::PLLCTL: OUT_DV Position

Definition at line 1242 of file Nano100Series.h.

## ◆ CLK_PLLCTL_PD_Msk

#define CLK_PLLCTL_PD_Msk (0x1ul << CLK_PLLCTL_PD_Pos)

CLK_T::PLLCTL: PD Mask

Definition at line 1246 of file Nano100Series.h.

## ◆ CLK_PLLCTL_PD_Pos

#define CLK_PLLCTL_PD_Pos (16)

CLK_T::PLLCTL: PD Position

Definition at line 1245 of file Nano100Series.h.

## ◆ CLK_PLLCTL_PLL_SRC_Msk

#define CLK_PLLCTL_PLL_SRC_Msk (0x1ul << CLK_PLLCTL_PLL_SRC_Pos)

CLK_T::PLLCTL: PLL_SRC Mask

Definition at line 1249 of file Nano100Series.h.

## ◆ CLK_PLLCTL_PLL_SRC_Pos

#define CLK_PLLCTL_PLL_SRC_Pos (17)

CLK_T::PLLCTL: PLL_SRC Position

Definition at line 1248 of file Nano100Series.h.

## ◆ CLK_PWRCTL_HIRC_EN_Msk

#define CLK_PWRCTL_HIRC_EN_Msk (0x1ul << CLK_PWRCTL_HIRC_EN_Pos)

CLK_T::PWRCTL: HIRC_EN Mask

Definition at line 1045 of file Nano100Series.h.

## ◆ CLK_PWRCTL_HIRC_EN_Pos

#define CLK_PWRCTL_HIRC_EN_Pos (2)

CLK_T::PWRCTL: HIRC_EN Position

Definition at line 1044 of file Nano100Series.h.

## ◆ CLK_PWRCTL_HXT_EN_Msk

#define CLK_PWRCTL_HXT_EN_Msk (0x1ul << CLK_PWRCTL_HXT_EN_Pos)

CLK_T::PWRCTL: HXT_EN Mask

Definition at line 1039 of file Nano100Series.h.

## ◆ CLK_PWRCTL_HXT_EN_Pos

#define CLK_PWRCTL_HXT_EN_Pos (0)

    @addtogroup CLK_CONST CLK Bit Field Definition
    Constant Definitions for CLK Controller

CLK_T::PWRCTL: HXT_EN Position

Definition at line 1038 of file Nano100Series.h.

## ◆ CLK_PWRCTL_HXT_GAIN_Msk

#define CLK_PWRCTL_HXT_GAIN_Msk (0x1ul << CLK_PWRCTL_HXT_GAIN_Pos)

CLK_T::PWRCTL: HXT_GAIN Mask

Definition at line 1063 of file Nano100Series.h.

## ◆ CLK_PWRCTL_HXT_GAIN_Pos

#define CLK_PWRCTL_HXT_GAIN_Pos (9)

CLK_T::PWRCTL: HXT_GAIN Position

Definition at line 1062 of file Nano100Series.h.

## ◆ CLK_PWRCTL_HXT_SELXT_Msk

#define CLK_PWRCTL_HXT_SELXT_Msk (0x1ul << CLK_PWRCTL_HXT_SELXT_Pos)

CLK_T::PWRCTL: HXT_SELXT Mask

Definition at line 1060 of file Nano100Series.h.

## ◆ CLK_PWRCTL_HXT_SELXT_Pos

#define CLK_PWRCTL_HXT_SELXT_Pos (8)

CLK_T::PWRCTL: HXT_SELXT Position

Definition at line 1059 of file Nano100Series.h.

## ◆ CLK_PWRCTL_LIRC_EN_Msk

#define CLK_PWRCTL_LIRC_EN_Msk (0x1ul << CLK_PWRCTL_LIRC_EN_Pos)

CLK_T::PWRCTL: LIRC_EN Mask

Definition at line 1048 of file Nano100Series.h.

## ◆ CLK_PWRCTL_LIRC_EN_Pos

#define CLK_PWRCTL_LIRC_EN_Pos (3)

CLK_T::PWRCTL: LIRC_EN Position

Definition at line 1047 of file Nano100Series.h.

## ◆ CLK_PWRCTL_LXT_EN_Msk

#define CLK_PWRCTL_LXT_EN_Msk (0x1ul << CLK_PWRCTL_LXT_EN_Pos)

CLK_T::PWRCTL: LXT_EN Mask

Definition at line 1042 of file Nano100Series.h.

## ◆ CLK_PWRCTL_LXT_EN_Pos

#define CLK_PWRCTL_LXT_EN_Pos (1)

CLK_T::PWRCTL: LXT_EN Position

Definition at line 1041 of file Nano100Series.h.

## ◆ CLK_PWRCTL_LXT_SCNT_Msk

#define CLK_PWRCTL_LXT_SCNT_Msk (0x1ul << CLK_PWRCTL_LXT_SCNT_Pos)

CLK_T::PWRCTL: LXT_SCNT Mask

Definition at line 1066 of file Nano100Series.h.

## ◆ CLK_PWRCTL_LXT_SCNT_Pos

#define CLK_PWRCTL_LXT_SCNT_Pos (10)

CLK_T::PWRCTL: LXT_SCNT Position

Definition at line 1065 of file Nano100Series.h.

## ◆ CLK_PWRCTL_PD_EN_Msk

#define CLK_PWRCTL_PD_EN_Msk (0x1ul << CLK_PWRCTL_PD_EN_Pos)

CLK_T::PWRCTL: PD_EN Mask

Definition at line 1057 of file Nano100Series.h.

## ◆ CLK_PWRCTL_PD_EN_Pos

#define CLK_PWRCTL_PD_EN_Pos (6)

CLK_T::PWRCTL: PD_EN Position

Definition at line 1056 of file Nano100Series.h.

## ◆ CLK_PWRCTL_PD_WK_IE_Msk

#define CLK_PWRCTL_PD_WK_IE_Msk (0x1ul << CLK_PWRCTL_PD_WK_IE_Pos)

CLK_T::PWRCTL: PD_WK_IE Mask

Definition at line 1054 of file Nano100Series.h.

## ◆ CLK_PWRCTL_PD_WK_IE_Pos

#define CLK_PWRCTL_PD_WK_IE_Pos (5)

CLK_T::PWRCTL: PD_WK_IE Position

Definition at line 1053 of file Nano100Series.h.

## ◆ CLK_PWRCTL_WK_DLY_Msk

#define CLK_PWRCTL_WK_DLY_Msk (0x1ul << CLK_PWRCTL_WK_DLY_Pos)

CLK_T::PWRCTL: WK_DLY Mask

Definition at line 1051 of file Nano100Series.h.

## ◆ CLK_PWRCTL_WK_DLY_Pos

#define CLK_PWRCTL_WK_DLY_Pos (4)

CLK_T::PWRCTL: WK_DLY Position

Definition at line 1050 of file Nano100Series.h.