| Nano100AN Series BSP V3.02.002 The Board Support Package for Nano100AN Series

Data Structures
NANO100 Peripherals
NANO100 Definitions

## Data Structures
struct | ADC_T
#define | ADC_RESULT_RSLT_Pos (0)
#define | ADC_RESULT_RSLT_Msk (0xffful << ADC_RESULT_RSLT_Pos)
#define | ADC_CR_ADEN_Pos (0)
#define | ADC_CR_ADEN_Msk (0x1ul << ADC_CR_ADEN_Pos)
#define | ADC_CR_ADIE_Pos (1)
#define | ADC_CR_ADIE_Msk (0x1ul << ADC_CR_ADIE_Pos)
#define | ADC_CR_ADMD_Pos (2)
#define | ADC_CR_ADMD_Msk (0x3ul << ADC_CR_ADMD_Pos)
#define | ADC_CR_TRGS_Pos (4)
#define | ADC_CR_TRGS_Msk (0x3ul << ADC_CR_TRGS_Pos)
#define | ADC_CR_TRGCOND_Pos (6)
#define | ADC_CR_TRGCOND_Msk (0x3ul << ADC_CR_TRGCOND_Pos)
#define | ADC_CR_TRGE_Pos (8)
#define | ADC_CR_TRGE_Msk (0x1ul << ADC_CR_TRGE_Pos)
#define | ADC_CR_PTEN_Pos (9)
#define | ADC_CR_PTEN_Msk (0x1ul << ADC_CR_PTEN_Pos)
#define | ADC_CR_ADST_Pos (11)
#define | ADC_CR_ADST_Msk (0x1ul << ADC_CR_ADST_Pos)
#define | ADC_CR_TMSEL_Pos (12)
#define | ADC_CR_TMSEL_Msk (0x3ul << ADC_CR_TMSEL_Pos)
#define | ADC_CR_TMTRGMOD_Pos (15)
#define | ADC_CR_TMTRGMOD_Msk (0x1ul << ADC_CR_TMTRGMOD_Pos)
#define | ADC_CR_REFSEL_Pos (16)
#define | ADC_CR_REFSEL_Msk (0x3ul << ADC_CR_REFSEL_Pos)
#define | ADC_CHEN_CHEN0_Pos (0)
#define | ADC_CHEN_CHEN0_Msk (0x1ul << ADC_CHEN_CHEN0_Pos)
#define | ADC_CHEN_CHEN1_Pos (1)
#define | ADC_CHEN_CHEN1_Msk (0x1ul << ADC_CHEN_CHEN1_Pos)
#define | ADC_CHEN_CHEN2_Pos (2)
#define | ADC_CHEN_CHEN2_Msk (0x1ul << ADC_CHEN_CHEN2_Pos)
#define | ADC_CHEN_CHEN3_Pos (3)
#define | ADC_CHEN_CHEN3_Msk (0x1ul << ADC_CHEN_CHEN3_Pos)
#define | ADC_CHEN_CHEN4_Pos (4)
#define | ADC_CHEN_CHEN4_Msk (0x1ul << ADC_CHEN_CHEN4_Pos)
#define | ADC_CHEN_CHEN5_Pos (5)
#define | ADC_CHEN_CHEN5_Msk (0x1ul << ADC_CHEN_CHEN5_Pos)
#define | ADC_CHEN_CHEN6_Pos (6)
#define | ADC_CHEN_CHEN6_Msk (0x1ul << ADC_CHEN_CHEN6_Pos)
#define | ADC_CHEN_CHEN7_Pos (7)
#define | ADC_CHEN_CHEN7_Msk (0x1ul << ADC_CHEN_CHEN7_Pos)
#define | ADC_CHEN_CHEN10_Pos (10)
#define | ADC_CHEN_CHEN10_Msk (0x1ul << ADC_CHEN_CHEN10_Pos)
#define | ADC_CHEN_CH10SEL_Pos (11)
#define | ADC_CHEN_CH10SEL_Msk (0x3ul << ADC_CHEN_CH10SEL_Pos)
#define | ADC_CMPR0_CMPEN_Pos (0)
#define | ADC_CMPR0_CMPEN_Msk (0x1ul << ADC_CMPR0_CMPEN_Pos)
#define | ADC_CMPR0_CMPIE_Pos (1)
#define | ADC_CMPR0_CMPIE_Msk (0x1ul << ADC_CMPR0_CMPIE_Pos)
#define | ADC_CMPR0_CMPCOND_Pos (2)
#define | ADC_CMPR0_CMPCOND_Msk (0x1ul << ADC_CMPR0_CMPCOND_Pos)
#define | ADC_CMPR0_CMPCH_Pos (3)
#define | ADC_CMPR0_CMPCH_Msk (0xful << ADC_CMPR0_CMPCH_Pos)
#define | ADC_CMPR0_CMPMATCNT_Pos (8)
#define | ADC_CMPR0_CMPMATCNT_Msk (0xful << ADC_CMPR0_CMPMATCNT_Pos)
#define | ADC_CMPR0_CMPD_Pos (16)
#define | ADC_CMPR0_CMPD_Msk (0xffful << ADC_CMPR0_CMPD_Pos)
#define | ADC_CMPR1_CMPEN_Pos (0)
#define | ADC_CMPR1_CMPEN_Msk (0x1ul << ADC_CMPR1_CMPEN_Pos)
#define | ADC_CMPR1_CMPIE_Pos (1)
#define | ADC_CMPR1_CMPIE_Msk (0x1ul << ADC_CMPR1_CMPIE_Pos)
#define | ADC_CMPR1_CMPCOND_Pos (2)
#define | ADC_CMPR1_CMPCOND_Msk (0x1ul << ADC_CMPR1_CMPCOND_Pos)
#define | ADC_CMPR1_CMPCH_Pos (3)
#define | ADC_CMPR1_CMPCH_Msk (0xful << ADC_CMPR1_CMPCH_Pos)
#define | ADC_CMPR1_CMPMATCNT_Pos (8)
#define | ADC_CMPR1_CMPMATCNT_Msk (0xful << ADC_CMPR1_CMPMATCNT_Pos)
#define | ADC_CMPR1_CMPD_Pos (16)
#define | ADC_CMPR1_CMPD_Msk (0xffful << ADC_CMPR1_CMPD_Pos)
#define | ADC_SR_ADF_Pos (0)
#define | ADC_SR_ADF_Msk (0x1ul << ADC_SR_ADF_Pos)
#define | ADC_SR_CMPF0_Pos (1)
#define | ADC_SR_CMPF0_Msk (0x1ul << ADC_SR_CMPF0_Pos)
#define | ADC_SR_CMPF1_Pos (2)
#define | ADC_SR_CMPF1_Msk (0x1ul << ADC_SR_CMPF1_Pos)
#define | ADC_SR_BUSY_Pos (3)
#define | ADC_SR_BUSY_Msk (0x1ul << ADC_SR_BUSY_Pos)
#define | ADC_SR_CHANNEL_Pos (4)
#define | ADC_SR_CHANNEL_Msk (0xful << ADC_SR_CHANNEL_Pos)
#define | ADC_SR_VALID_Pos (8)
#define | ADC_SR_VALID_Msk (0x4fful << ADC_SR_VALID_Pos)
#define | ADC_SR_OVERRUN_Pos (20)
#define | ADC_SR_OVERRUN_Msk (0x4fful << ADC_SR_OVERRUN_Pos)
#define | ADC_PDMA_AD_PDMA_Pos (0)
#define | ADC_PDMA_AD_PDMA_Msk (0xffful << ADC_PDMA_AD_PDMA_Pos)
#define | ADC_DELSEL_En2StDelay_Pos (0)
#define | ADC_DELSEL_En2StDelay_Msk (0xfful << ADC_DELSEL_En2StDelay_Pos)
#define | ADC_DELSEL_TMPDMACNT_Pos (8)
#define | ADC_DELSEL_TMPDMACNT_Msk (0xfful << ADC_DELSEL_TMPDMACNT_Pos)
#define | ADC_DELSEL_ADCSTHOLDCNT_Pos (16)
#define | ADC_DELSEL_ADCSTHOLDCNT_Msk (0xfful << ADC_DELSEL_ADCSTHOLDCNT_Pos)

## Detailed Description

NANO100 Device Specific Peripheral registers structures

## Macro Definition Documentation

## ◆ ADC_CHEN_CH10SEL_Msk

#define ADC_CHEN_CH10SEL_Msk (0x3ul << ADC_CHEN_CH10SEL_Pos)

ADC_T::CHEN: CH10SEL Mask

Definition at line 527 of file Nano100Series.h.

## ◆ ADC_CHEN_CH10SEL_Pos

#define ADC_CHEN_CH10SEL_Pos (11)

ADC_T::CHEN: CH10SEL Position

Definition at line 526 of file Nano100Series.h.

## ◆ ADC_CHEN_CHEN0_Msk

#define ADC_CHEN_CHEN0_Msk (0x1ul << ADC_CHEN_CHEN0_Pos)

ADC_T::CHEN: CHEN0 Mask

Definition at line 500 of file Nano100Series.h.

## ◆ ADC_CHEN_CHEN0_Pos

#define ADC_CHEN_CHEN0_Pos (0)

ADC_T::CHEN: CHEN0 Position

Definition at line 499 of file Nano100Series.h.

## ◆ ADC_CHEN_CHEN10_Msk

#define ADC_CHEN_CHEN10_Msk (0x1ul << ADC_CHEN_CHEN10_Pos)

ADC_T::CHEN: CHEN10 Mask

Definition at line 524 of file Nano100Series.h.

## ◆ ADC_CHEN_CHEN10_Pos

#define ADC_CHEN_CHEN10_Pos (10)

ADC_T::CHEN: CHEN10 Position

Definition at line 523 of file Nano100Series.h.

## ◆ ADC_CHEN_CHEN1_Msk

#define ADC_CHEN_CHEN1_Msk (0x1ul << ADC_CHEN_CHEN1_Pos)

ADC_T::CHEN: CHEN1 Mask

Definition at line 503 of file Nano100Series.h.

## ◆ ADC_CHEN_CHEN1_Pos

#define ADC_CHEN_CHEN1_Pos (1)

ADC_T::CHEN: CHEN1 Position

Definition at line 502 of file Nano100Series.h.

## ◆ ADC_CHEN_CHEN2_Msk

#define ADC_CHEN_CHEN2_Msk (0x1ul << ADC_CHEN_CHEN2_Pos)

ADC_T::CHEN: CHEN2 Mask

Definition at line 506 of file Nano100Series.h.

## ◆ ADC_CHEN_CHEN2_Pos

#define ADC_CHEN_CHEN2_Pos (2)

ADC_T::CHEN: CHEN2 Position

Definition at line 505 of file Nano100Series.h.

## ◆ ADC_CHEN_CHEN3_Msk

#define ADC_CHEN_CHEN3_Msk (0x1ul << ADC_CHEN_CHEN3_Pos)

ADC_T::CHEN: CHEN3 Mask

Definition at line 509 of file Nano100Series.h.

## ◆ ADC_CHEN_CHEN3_Pos

#define ADC_CHEN_CHEN3_Pos (3)

ADC_T::CHEN: CHEN3 Position

Definition at line 508 of file Nano100Series.h.

## ◆ ADC_CHEN_CHEN4_Msk

#define ADC_CHEN_CHEN4_Msk (0x1ul << ADC_CHEN_CHEN4_Pos)

ADC_T::CHEN: CHEN4 Mask

Definition at line 512 of file Nano100Series.h.

## ◆ ADC_CHEN_CHEN4_Pos

#define ADC_CHEN_CHEN4_Pos (4)

ADC_T::CHEN: CHEN4 Position

Definition at line 511 of file Nano100Series.h.

## ◆ ADC_CHEN_CHEN5_Msk

#define ADC_CHEN_CHEN5_Msk (0x1ul << ADC_CHEN_CHEN5_Pos)

ADC_T::CHEN: CHEN5 Mask

Definition at line 515 of file Nano100Series.h.

## ◆ ADC_CHEN_CHEN5_Pos

#define ADC_CHEN_CHEN5_Pos (5)

ADC_T::CHEN: CHEN5 Position

Definition at line 514 of file Nano100Series.h.

## ◆ ADC_CHEN_CHEN6_Msk

#define ADC_CHEN_CHEN6_Msk (0x1ul << ADC_CHEN_CHEN6_Pos)

ADC_T::CHEN: CHEN6 Mask

Definition at line 518 of file Nano100Series.h.

## ◆ ADC_CHEN_CHEN6_Pos

#define ADC_CHEN_CHEN6_Pos (6)

ADC_T::CHEN: CHEN6 Position

Definition at line 517 of file Nano100Series.h.

## ◆ ADC_CHEN_CHEN7_Msk

#define ADC_CHEN_CHEN7_Msk (0x1ul << ADC_CHEN_CHEN7_Pos)

ADC_T::CHEN: CHEN7 Mask

Definition at line 521 of file Nano100Series.h.

## ◆ ADC_CHEN_CHEN7_Pos

#define ADC_CHEN_CHEN7_Pos (7)

ADC_T::CHEN: CHEN7 Position

Definition at line 520 of file Nano100Series.h.

## ◆ ADC_CMPR0_CMPCH_Msk

#define ADC_CMPR0_CMPCH_Msk (0xful << ADC_CMPR0_CMPCH_Pos)

ADC_T::CMPR0: CMPCH Mask

Definition at line 539 of file Nano100Series.h.

## ◆ ADC_CMPR0_CMPCH_Pos

#define ADC_CMPR0_CMPCH_Pos (3)

ADC_T::CMPR0: CMPCH Position

Definition at line 538 of file Nano100Series.h.

## ◆ ADC_CMPR0_CMPCOND_Msk

#define ADC_CMPR0_CMPCOND_Msk (0x1ul << ADC_CMPR0_CMPCOND_Pos)

ADC_T::CMPR0: CMPCOND Mask

Definition at line 536 of file Nano100Series.h.

## ◆ ADC_CMPR0_CMPCOND_Pos

#define ADC_CMPR0_CMPCOND_Pos (2)

ADC_T::CMPR0: CMPCOND Position

Definition at line 535 of file Nano100Series.h.

## ◆ ADC_CMPR0_CMPD_Msk

#define ADC_CMPR0_CMPD_Msk (0xffful << ADC_CMPR0_CMPD_Pos)

ADC_T::CMPR0: CMPD Mask

Definition at line 545 of file Nano100Series.h.

## ◆ ADC_CMPR0_CMPD_Pos

#define ADC_CMPR0_CMPD_Pos (16)

ADC_T::CMPR0: CMPD Position

Definition at line 544 of file Nano100Series.h.

## ◆ ADC_CMPR0_CMPEN_Msk

#define ADC_CMPR0_CMPEN_Msk (0x1ul << ADC_CMPR0_CMPEN_Pos)

ADC_T::CMPR0: CMPEN Mask

Definition at line 530 of file Nano100Series.h.

## ◆ ADC_CMPR0_CMPEN_Pos

#define ADC_CMPR0_CMPEN_Pos (0)

ADC_T::CMPR0: CMPEN Position

Definition at line 529 of file Nano100Series.h.

## ◆ ADC_CMPR0_CMPIE_Msk

#define ADC_CMPR0_CMPIE_Msk (0x1ul << ADC_CMPR0_CMPIE_Pos)

ADC_T::CMPR0: CMPIE Mask

Definition at line 533 of file Nano100Series.h.

## ◆ ADC_CMPR0_CMPIE_Pos

#define ADC_CMPR0_CMPIE_Pos (1)

ADC_T::CMPR0: CMPIE Position

Definition at line 532 of file Nano100Series.h.

## ◆ ADC_CMPR0_CMPMATCNT_Msk

#define ADC_CMPR0_CMPMATCNT_Msk (0xful << ADC_CMPR0_CMPMATCNT_Pos)

ADC_T::CMPR0: CMPMATCNT Mask

Definition at line 542 of file Nano100Series.h.

## ◆ ADC_CMPR0_CMPMATCNT_Pos

#define ADC_CMPR0_CMPMATCNT_Pos (8)

ADC_T::CMPR0: CMPMATCNT Position

Definition at line 541 of file Nano100Series.h.

## ◆ ADC_CMPR1_CMPCH_Msk

#define ADC_CMPR1_CMPCH_Msk (0xful << ADC_CMPR1_CMPCH_Pos)

ADC_T::CMPR1: CMPCH Mask

Definition at line 557 of file Nano100Series.h.

## ◆ ADC_CMPR1_CMPCH_Pos

#define ADC_CMPR1_CMPCH_Pos (3)

ADC_T::CMPR1: CMPCH Position

Definition at line 556 of file Nano100Series.h.

## ◆ ADC_CMPR1_CMPCOND_Msk

#define ADC_CMPR1_CMPCOND_Msk (0x1ul << ADC_CMPR1_CMPCOND_Pos)

ADC_T::CMPR1: CMPCOND Mask

Definition at line 554 of file Nano100Series.h.

## ◆ ADC_CMPR1_CMPCOND_Pos

#define ADC_CMPR1_CMPCOND_Pos (2)

ADC_T::CMPR1: CMPCOND Position

Definition at line 553 of file Nano100Series.h.

## ◆ ADC_CMPR1_CMPD_Msk

#define ADC_CMPR1_CMPD_Msk (0xffful << ADC_CMPR1_CMPD_Pos)

ADC_T::CMPR1: CMPD Mask

Definition at line 563 of file Nano100Series.h.

## ◆ ADC_CMPR1_CMPD_Pos

#define ADC_CMPR1_CMPD_Pos (16)

ADC_T::CMPR1: CMPD Position

Definition at line 562 of file Nano100Series.h.

## ◆ ADC_CMPR1_CMPEN_Msk

#define ADC_CMPR1_CMPEN_Msk (0x1ul << ADC_CMPR1_CMPEN_Pos)

ADC_T::CMPR1: CMPEN Mask

Definition at line 548 of file Nano100Series.h.

## ◆ ADC_CMPR1_CMPEN_Pos

#define ADC_CMPR1_CMPEN_Pos (0)

ADC_T::CMPR1: CMPEN Position

Definition at line 547 of file Nano100Series.h.

## ◆ ADC_CMPR1_CMPIE_Msk

#define ADC_CMPR1_CMPIE_Msk (0x1ul << ADC_CMPR1_CMPIE_Pos)

ADC_T::CMPR1: CMPIE Mask

Definition at line 551 of file Nano100Series.h.

## ◆ ADC_CMPR1_CMPIE_Pos

#define ADC_CMPR1_CMPIE_Pos (1)

ADC_T::CMPR1: CMPIE Position

Definition at line 550 of file Nano100Series.h.

## ◆ ADC_CMPR1_CMPMATCNT_Msk

#define ADC_CMPR1_CMPMATCNT_Msk (0xful << ADC_CMPR1_CMPMATCNT_Pos)

ADC_T::CMPR1: CMPMATCNT Mask

Definition at line 560 of file Nano100Series.h.

## ◆ ADC_CMPR1_CMPMATCNT_Pos

#define ADC_CMPR1_CMPMATCNT_Pos (8)

ADC_T::CMPR1: CMPMATCNT Position

Definition at line 559 of file Nano100Series.h.

## ◆ ADC_CR_ADEN_Msk

#define ADC_CR_ADEN_Msk (0x1ul << ADC_CR_ADEN_Pos)

ADC_T::CR: ADEN Mask

Definition at line 467 of file Nano100Series.h.

## ◆ ADC_CR_ADEN_Pos

#define ADC_CR_ADEN_Pos (0)

ADC_T::CR: ADEN Position

Definition at line 466 of file Nano100Series.h.

## ◆ ADC_CR_ADIE_Msk

#define ADC_CR_ADIE_Msk (0x1ul << ADC_CR_ADIE_Pos)

ADC_T::CR: ADIE Mask

Definition at line 470 of file Nano100Series.h.

## ◆ ADC_CR_ADIE_Pos

#define ADC_CR_ADIE_Pos (1)

ADC_T::CR: ADIE Position

Definition at line 469 of file Nano100Series.h.

## ◆ ADC_CR_ADMD_Msk

#define ADC_CR_ADMD_Msk (0x3ul << ADC_CR_ADMD_Pos)

ADC_T::CR: ADMD Mask

Definition at line 473 of file Nano100Series.h.

## ◆ ADC_CR_ADMD_Pos

#define ADC_CR_ADMD_Pos (2)

ADC_T::CR: ADMD Position

Definition at line 472 of file Nano100Series.h.

## ◆ ADC_CR_ADST_Msk

#define ADC_CR_ADST_Msk (0x1ul << ADC_CR_ADST_Pos)

ADC_T::CR: ADST Mask

Definition at line 488 of file Nano100Series.h.

## ◆ ADC_CR_ADST_Pos

#define ADC_CR_ADST_Pos (11)

ADC_T::CR: ADST Position

Definition at line 487 of file Nano100Series.h.

## ◆ ADC_CR_PTEN_Msk

#define ADC_CR_PTEN_Msk (0x1ul << ADC_CR_PTEN_Pos)

ADC_T::CR: PTEN Mask

Definition at line 485 of file Nano100Series.h.

## ◆ ADC_CR_PTEN_Pos

#define ADC_CR_PTEN_Pos (9)

ADC_T::CR: PTEN Position

Definition at line 484 of file Nano100Series.h.

## ◆ ADC_CR_REFSEL_Msk

#define ADC_CR_REFSEL_Msk (0x3ul << ADC_CR_REFSEL_Pos)

ADC_T::CR: REFSEL Mask

Definition at line 497 of file Nano100Series.h.

## ◆ ADC_CR_REFSEL_Pos

#define ADC_CR_REFSEL_Pos (16)

ADC_T::CR: REFSEL Position

Definition at line 496 of file Nano100Series.h.

## ◆ ADC_CR_TMSEL_Msk

#define ADC_CR_TMSEL_Msk (0x3ul << ADC_CR_TMSEL_Pos)

ADC_T::CR: TMSEL Mask

Definition at line 491 of file Nano100Series.h.

## ◆ ADC_CR_TMSEL_Pos

#define ADC_CR_TMSEL_Pos (12)

ADC_T::CR: TMSEL Position

Definition at line 490 of file Nano100Series.h.

## ◆ ADC_CR_TMTRGMOD_Msk

#define ADC_CR_TMTRGMOD_Msk (0x1ul << ADC_CR_TMTRGMOD_Pos)

ADC_T::CR: TMTRGMOD Mask

Definition at line 494 of file Nano100Series.h.

## ◆ ADC_CR_TMTRGMOD_Pos

#define ADC_CR_TMTRGMOD_Pos (15)

ADC_T::CR: TMTRGMOD Position

Definition at line 493 of file Nano100Series.h.

## ◆ ADC_CR_TRGCOND_Msk

#define ADC_CR_TRGCOND_Msk (0x3ul << ADC_CR_TRGCOND_Pos)

ADC_T::CR: TRGCOND Mask

Definition at line 479 of file Nano100Series.h.

## ◆ ADC_CR_TRGCOND_Pos

#define ADC_CR_TRGCOND_Pos (6)

ADC_T::CR: TRGCOND Position

Definition at line 478 of file Nano100Series.h.

## ◆ ADC_CR_TRGE_Msk

#define ADC_CR_TRGE_Msk (0x1ul << ADC_CR_TRGE_Pos)

ADC_T::CR: TRGE Mask

Definition at line 482 of file Nano100Series.h.

## ◆ ADC_CR_TRGE_Pos

#define ADC_CR_TRGE_Pos (8)

ADC_T::CR: TRGE Position

Definition at line 481 of file Nano100Series.h.

## ◆ ADC_CR_TRGS_Msk

#define ADC_CR_TRGS_Msk (0x3ul << ADC_CR_TRGS_Pos)

ADC_T::CR: TRGS Mask

Definition at line 476 of file Nano100Series.h.

## ◆ ADC_CR_TRGS_Pos

#define ADC_CR_TRGS_Pos (4)

ADC_T::CR: TRGS Position

Definition at line 475 of file Nano100Series.h.

## ◆ ADC_DELSEL_ADCSTHOLDCNT_Msk

#define ADC_DELSEL_ADCSTHOLDCNT_Msk (0xfful << ADC_DELSEL_ADCSTHOLDCNT_Pos)

ADC_T::DELSEL: ADCSTHOLDCNT Mask

Definition at line 596 of file Nano100Series.h.

## ◆ ADC_DELSEL_ADCSTHOLDCNT_Pos

#define ADC_DELSEL_ADCSTHOLDCNT_Pos (16)

ADC_T::DELSEL: ADCSTHOLDCNT Position

Definition at line 595 of file Nano100Series.h.

## ◆ ADC_DELSEL_En2StDelay_Msk

#define ADC_DELSEL_En2StDelay_Msk (0xfful << ADC_DELSEL_En2StDelay_Pos)

ADC_T::DELSEL: En2StDelay Mask

Definition at line 590 of file Nano100Series.h.

## ◆ ADC_DELSEL_En2StDelay_Pos

#define ADC_DELSEL_En2StDelay_Pos (0)

ADC_T::DELSEL: En2StDelay Position

Definition at line 589 of file Nano100Series.h.

## ◆ ADC_DELSEL_TMPDMACNT_Msk

#define ADC_DELSEL_TMPDMACNT_Msk (0xfful << ADC_DELSEL_TMPDMACNT_Pos)

ADC_T::DELSEL: TMPDMACNT Mask

Definition at line 593 of file Nano100Series.h.

## ◆ ADC_DELSEL_TMPDMACNT_Pos

#define ADC_DELSEL_TMPDMACNT_Pos (8)

ADC_T::DELSEL: TMPDMACNT Position

Definition at line 592 of file Nano100Series.h.

## ◆ ADC_PDMA_AD_PDMA_Msk

#define ADC_PDMA_AD_PDMA_Msk (0xffful << ADC_PDMA_AD_PDMA_Pos)

ADC_T::PDMA: AD_PDMA Mask

Definition at line 587 of file Nano100Series.h.

## ◆ ADC_PDMA_AD_PDMA_Pos

#define ADC_PDMA_AD_PDMA_Pos (0)

ADC_T::PDMA: AD_PDMA Position

Definition at line 586 of file Nano100Series.h.

## ◆ ADC_RESULT_RSLT_Msk

#define ADC_RESULT_RSLT_Msk (0xffful << ADC_RESULT_RSLT_Pos)

ADC_T::RESULT: RSLT Mask

Definition at line 464 of file Nano100Series.h.

## ◆ ADC_RESULT_RSLT_Pos

#define ADC_RESULT_RSLT_Pos (0)

    @addtogroup ADC_CONST ADC Bit Field Definition
    Constant Definitions for ADC Controller

ADC_T::RESULT: RSLT Position

Definition at line 463 of file Nano100Series.h.

## ◆ ADC_SR_ADF_Msk

#define ADC_SR_ADF_Msk (0x1ul << ADC_SR_ADF_Pos)

ADC_T::SR: ADF Mask

Definition at line 566 of file Nano100Series.h.

## ◆ ADC_SR_ADF_Pos

#define ADC_SR_ADF_Pos (0)

ADC_T::SR: ADF Position

Definition at line 565 of file Nano100Series.h.

## ◆ ADC_SR_BUSY_Msk

#define ADC_SR_BUSY_Msk (0x1ul << ADC_SR_BUSY_Pos)

ADC_T::SR: BUSY Mask

Definition at line 575 of file Nano100Series.h.

## ◆ ADC_SR_BUSY_Pos

#define ADC_SR_BUSY_Pos (3)

ADC_T::SR: BUSY Position

Definition at line 574 of file Nano100Series.h.

## ◆ ADC_SR_CHANNEL_Msk

#define ADC_SR_CHANNEL_Msk (0xful << ADC_SR_CHANNEL_Pos)

ADC_T::SR: CHANNEL Mask

Definition at line 578 of file Nano100Series.h.

## ◆ ADC_SR_CHANNEL_Pos

#define ADC_SR_CHANNEL_Pos (4)

ADC_T::SR: CHANNEL Position

Definition at line 577 of file Nano100Series.h.

## ◆ ADC_SR_CMPF0_Msk

#define ADC_SR_CMPF0_Msk (0x1ul << ADC_SR_CMPF0_Pos)

ADC_T::SR: CMPF0 Mask

Definition at line 569 of file Nano100Series.h.

## ◆ ADC_SR_CMPF0_Pos

#define ADC_SR_CMPF0_Pos (1)

ADC_T::SR: CMPF0 Position

Definition at line 568 of file Nano100Series.h.

## ◆ ADC_SR_CMPF1_Msk

#define ADC_SR_CMPF1_Msk (0x1ul << ADC_SR_CMPF1_Pos)

ADC_T::SR: CMPF1 Mask

Definition at line 572 of file Nano100Series.h.

## ◆ ADC_SR_CMPF1_Pos

#define ADC_SR_CMPF1_Pos (2)

ADC_T::SR: CMPF1 Position

Definition at line 571 of file Nano100Series.h.

## ◆ ADC_SR_OVERRUN_Msk

#define ADC_SR_OVERRUN_Msk (0x4fful << ADC_SR_OVERRUN_Pos)

ADC_T::SR: OVERRUN Mask

Definition at line 584 of file Nano100Series.h.

## ◆ ADC_SR_OVERRUN_Pos

#define ADC_SR_OVERRUN_Pos (20)

ADC_T::SR: OVERRUN Position

Definition at line 583 of file Nano100Series.h.

## ◆ ADC_SR_VALID_Msk

#define ADC_SR_VALID_Msk (0x4fful << ADC_SR_VALID_Pos)

ADC_T::SR: VALID Mask

Definition at line 581 of file Nano100Series.h.

## ◆ ADC_SR_VALID_Pos

#define ADC_SR_VALID_Pos (8)

ADC_T::SR: VALID Position

Definition at line 580 of file Nano100Series.h.