| Airoha M0 BLE API 1.0.5.4

Data Fields
ble_gatt_evt_uuid_char_discovered_t Struct Reference
ble_gatt_client.h

Event parameter of gatt event BLE_GATT_EVT_UUID_CHAR_DISCOVERED. More...

## Data Fields
uint8_t | uuid_len
uint8_t | uuid [16]
struct {
uint16_t value_handle
uint8_t property
} | charact [1]

## Detailed Description

Event parameter of gatt event BLE_GATT_EVT_UUID_CHAR_DISCOVERED.

## Field Documentation

## ◆ uuid_len

uint8_t ble_gatt_evt_uuid_char_discovered_t::uuid_len

number of characteristics in this event

## ◆ uuid

uint8_t ble_gatt_evt_uuid_char_discovered_t::uuid[16]

uuid length of these characteristics

## ◆ value_handle

uint16_t ble_gatt_evt_uuid_char_discovered_t::value_handle

handle of the characteristic declaration

## ◆ property

uint8_t ble_gatt_evt_uuid_char_discovered_t::property

handle of the characteristic value

## ◆ charact

struct { ... } ble_gatt_evt_uuid_char_discovered_t::charact[1]

uuid of these characteristics