| Airoha M0 BLE API 1.0.5.4

Data Fields
ble_gatt_evt_included_service_found_t Struct Reference
ble_gatt_client.h

Event parameter of gatt event BLE_GATT_EVT_INCLUDED_SERVICE_FOUND. More...

## Data Fields
struct {
uint16_t service_start
uint16_t service_end
uint8_t service_uuid_len
uint8_t service_uuid [16]
} | include [1]

## Detailed Description

Event parameter of gatt event BLE_GATT_EVT_INCLUDED_SERVICE_FOUND.

## Field Documentation

## ◆ service_start

uint16_t ble_gatt_evt_included_service_found_t::service_start

handle of the include declaration attribute

## ◆ service_end

uint16_t ble_gatt_evt_included_service_found_t::service_end

handle of the first attribute of the included service

## ◆ service_uuid_len

uint8_t ble_gatt_evt_included_service_found_t::service_uuid_len

handle of the last attribute of the included service

## ◆ service_uuid

uint8_t ble_gatt_evt_included_service_found_t::service_uuid[16]

uuid length of the included service

## ◆ include

struct { ... } ble_gatt_evt_included_service_found_t::include[1]

number of included services in this event