| Nano100BN Series BSP V3.03.002 The Board Support Package for Nano100BN Series

Functions
lcd.c File Reference

Nano100 series LCD driver header file The LCD driver can directly drives a LCD glass by creating the ac segment and common voltage signals automatically. It can support static, 1/2 duty, 1/3 duty, 1/4 duty, 1/5 duty, 1/6 duty LCD glass with up to 34 segments with 6 COM or 36 segments with 4 COM. More...

`#include <stdio.h>`
`#include <string.h>`
`#include <stdlib.h>`
`#include "Nano100Series.h"`

Go to the source code of this file.

## Functions
void | LCD_SetPixel (uint32_t u32Com, uint32_t u32Seg, uint32_t u32OnFlag)
| Enables a segment on the LCD display. More...
void | LCD_SetAllPixels (uint32_t u32OnOff)
| LCD Enable/Disable all segments. More...
uint32_t | LCD_EnableFrameCounter (uint32_t u32Count)
| Set Frame Count and Enable frame count. More...
void | LCD_DisableFrameCounter (void)
| Disable frame count function. More...
uint32_t | LCD_Open (uint32_t u32DrivingType, uint32_t u32ComNum, uint32_t u32BiasLevel, uint32_t u32FramerateDiv, uint32_t u32DrivingVol)
| LCD Initialization routine. More...
void | LCD_Close (void)
| The function is used to disable LCD controller. More...
uint32_t | LCD_EnableBlink (uint32_t u32ms)
| Enable Blink function in LCD controller. More...
void | LCD_DisableBlink (void)
| Disable Blink function in LCD controller. More...
void | LCD_EnableInt (uint32_t IntSrc)
| This function is used to enable LCD interrupt. More...
void | LCD_DisableInt (uint32_t IntSrc)
| This function is used to disable LCD specified interrupt. More...

## Detailed Description

Nano100 series LCD driver header file The LCD driver can directly drives a LCD glass by creating the ac segment and common voltage signals automatically. It can support static, 1/2 duty, 1/3 duty, 1/4 duty, 1/5 duty, 1/6 duty LCD glass with up to 34 segments with 6 COM or 36 segments with 4 COM.

Version
  V1.00

Revision
  9

Date
  15/07/06 2:08p

Note
  Copyright (C) 2013~2014 Nuvoton Technology Corp. All rights reserved.

Definition in file lcd.c.