| Nano100BN Series BSP V3.03.002 The Board Support Package for Nano100BN Series

LCDLIB.h
Go to the documentation of this file.
1 /**************************************************************************/
11 #ifndef __NANO100_LCDLIB_H
12 #define __NANO100_LCDLIB_H
13
14 #ifdef __cplusplus
15 extern "C"
16 {
17 #endif
18
32 typedef struct
33 {
34 uint32_t Sub_Zone_Num;
35 uint32_t Zone_Digit_SegNum;
36 } ZoneInfo_TypeDef;
37 /* end of group NANO100_LCDLIB_EXPORTED_STRUCTS */
39
40
45 void LCDLIB_Printf(uint32_t u32Zone, char *string);
46 void LCDLIB_PutChar(uint32_t u32Zone, uint32_t u32Index, uint8_t u8Ch);
47 void LCDLIB_SetSymbol(uint32_t u32Zone, uint32_t u32Index, uint32_t u32OnOff);
48 void LCDLIB_PrintNumber(uint32_t u32Zone, long long value);
49
50 /* end of group NANO100_LCDLIB_EXPORTED_FUNCTIONS */
52 /* end of group NANO100_LCDLIB_Driver */
54 /* end of group NANO100_Library */
56
57
58
59 #ifdef __cplusplus
60 }
61 #endif
62
63 #endif /* __NANO100_LCDLIB_H */
64
65
66
67 /*** (C) COPYRIGHT 2013 Nuvoton Technology Corp. ***/
68
LCDLIB_PrintNumber
void LCDLIB_PrintNumber(uint32_t u32Zone, long long value)
Display number on LCD.
Definition: LCDLIB.c:110
ZoneInfo_TypeDef
Definition: LCDLIB.h:32
LCDLIB_SetSymbol
void LCDLIB_SetSymbol(uint32_t u32Zone, uint32_t u32Index, uint32_t u32OnOff)
Display symbol on LCD.
Definition: LCDLIB.c:230
ZoneInfo_TypeDef::Sub_Zone_Num
uint32_t Sub_Zone_Num
Definition: LCDLIB.h:34
ZoneInfo_TypeDef::Zone_Digit_SegNum
uint32_t Zone_Digit_SegNum
Definition: LCDLIB.h:35
LCDLIB_PutChar
void LCDLIB_PutChar(uint32_t u32Zone, uint32_t u32Index, uint8_t u8Ch)
Display character on LCD.
Definition: LCDLIB.c:181
LCDLIB_Printf
void LCDLIB_Printf(uint32_t u32Zone, char *string)
Display text on LCD.
Definition: LCDLIB.c:52
value
return value
Definition: semihosting.h:98