| NUC472_NUC442_BSP V3.03.003 The Board Support Package for NUC472/NUC442

Modules | Macros
PDMA Exported Constants
NUC472/NUC442 Device Driver » PDMA Driver
Collaboration diagram for PDMA Exported Constants:

## Modules
| PDMA Exported Functions

## Macros
#define | PDMA_CH_MAX
#define | PDMA_OP_STOP
#define | PDMA_OP_BASIC
#define | PDMA_OP_SCATTER
#define | PDMA_WIDTH_8
#define | PDMA_WIDTH_16
#define | PDMA_WIDTH_32
#define | PDMA_SAR_INC
#define | PDMA_SAR_FIX
#define | PDMA_DAR_INC
#define | PDMA_DAR_FIX
#define | PDMA_REQ_SINGLE
#define | PDMA_REQ_BURST
#define | PDMA_BURST_128
#define | PDMA_BURST_64
#define | PDMA_BURST_32
#define | PDMA_BURST_16
#define | PDMA_BURST_8
#define | PDMA_BURST_4
#define | PDMA_BURST_2
#define | PDMA_BURST_1
#define | PDMA_SPI0_TX
#define | PDMA_SPI1_TX
#define | PDMA_SPI2_TX
#define | PDMA_SPI3_TX
#define | PDMA_UART0_TX
#define | PDMA_UART1_TX
#define | PDMA_UART2_TX
#define | PDMA_UART3_TX
#define | PDMA_UART4_TX
#define | PDMA_UART5_TX
#define | PDMA_I2S0_TX
#define | PDMA_I2S1_TX
#define | PDMA_SPI0_RX
#define | PDMA_SPI1_RX
#define | PDMA_SPI2_RX
#define | PDMA_SPI3_RX
#define | PDMA_UART0_RX
#define | PDMA_UART1_RX
#define | PDMA_UART2_RX
#define | PDMA_UART3_RX
#define | PDMA_UART4_RX
#define | PDMA_UART5_RX
#define | PDMA_ADC
#define | PDMA_I2S0_RX
#define | PDMA_I2S1_RX
#define | PDMA_MEM

## Detailed Description

## Macro Definition Documentation

## ◆ PDMA_ADC

#define PDMA_ADC

DMA Connect to ADC

Definition at line 96 of file pdma.h.

## ◆ PDMA_BURST_1

#define PDMA_BURST_1

DMA Burst 1 Transfers

Definition at line 69 of file pdma.h.

## ◆ PDMA_BURST_128

#define PDMA_BURST_128

DMA Burst 128 Transfers

Definition at line 62 of file pdma.h.

## ◆ PDMA_BURST_16

#define PDMA_BURST_16

DMA Burst 16 Transfers

Definition at line 65 of file pdma.h.

## ◆ PDMA_BURST_2

#define PDMA_BURST_2

DMA Burst 2 Transfers

Definition at line 68 of file pdma.h.

## ◆ PDMA_BURST_32

#define PDMA_BURST_32

DMA Burst 32 Transfers

Definition at line 64 of file pdma.h.

## ◆ PDMA_BURST_4

#define PDMA_BURST_4

DMA Burst 4 Transfers

Definition at line 67 of file pdma.h.

## ◆ PDMA_BURST_64

#define PDMA_BURST_64

DMA Burst 64 Transfers

Definition at line 63 of file pdma.h.

## ◆ PDMA_BURST_8

#define PDMA_BURST_8

DMA Burst 8 Transfers

Definition at line 66 of file pdma.h.

## ◆ PDMA_CH_MAX

#define PDMA_CH_MAX

Specify Maximum Channels of PDMA

Definition at line 32 of file pdma.h.

## ◆ PDMA_DAR_FIX

#define PDMA_DAR_FIX

DMA DAR fix address

Definition at line 54 of file pdma.h.

## ◆ PDMA_DAR_INC

#define PDMA_DAR_INC

DMA DAR increment

Definition at line 53 of file pdma.h.

## ◆ PDMA_I2S0_RX

#define PDMA_I2S0_RX

DMA Connect to I2S TX

Definition at line 97 of file pdma.h.

## ◆ PDMA_I2S0_TX

#define PDMA_I2S0_TX

DMA Connect to I2S TX

Definition at line 84 of file pdma.h.

## ◆ PDMA_I2S1_RX

#define PDMA_I2S1_RX

DMA Connect to I2S1 TX

Definition at line 98 of file pdma.h.

## ◆ PDMA_I2S1_TX

#define PDMA_I2S1_TX

DMA Connect to I2S1 TX

Definition at line 85 of file pdma.h.

## ◆ PDMA_MEM

#define PDMA_MEM

DMA Connect to Memory

Definition at line 99 of file pdma.h.

## ◆ PDMA_OP_BASIC

#define PDMA_OP_BASIC

DMA Basic Mode

Definition at line 38 of file pdma.h.

## ◆ PDMA_OP_SCATTER

#define PDMA_OP_SCATTER

DMA Scatter-gather Mode

Definition at line 39 of file pdma.h.

## ◆ PDMA_OP_STOP

#define PDMA_OP_STOP

DMA Stop Mode

Definition at line 37 of file pdma.h.

## ◆ PDMA_REQ_BURST

#define PDMA_REQ_BURST

DMA Burst Request

Definition at line 60 of file pdma.h.

## ◆ PDMA_REQ_SINGLE

#define PDMA_REQ_SINGLE

DMA Single Request

Definition at line 59 of file pdma.h.

## ◆ PDMA_SAR_FIX

#define PDMA_SAR_FIX

DMA SAR fix address

Definition at line 52 of file pdma.h.

## ◆ PDMA_SAR_INC

#define PDMA_SAR_INC

DMA SAR increment

Definition at line 51 of file pdma.h.

## ◆ PDMA_SPI0_RX

#define PDMA_SPI0_RX

DMA Connect to SPI0 RX

Definition at line 86 of file pdma.h.

## ◆ PDMA_SPI0_TX

#define PDMA_SPI0_TX

DMA Connect to SPI0 TX

Definition at line 74 of file pdma.h.

## ◆ PDMA_SPI1_RX

#define PDMA_SPI1_RX

DMA Connect to SPI1 RX

Definition at line 87 of file pdma.h.

## ◆ PDMA_SPI1_TX

#define PDMA_SPI1_TX

DMA Connect to SPI1 TX

Definition at line 75 of file pdma.h.

## ◆ PDMA_SPI2_RX

#define PDMA_SPI2_RX

DMA Connect to SPI2 RX

Definition at line 88 of file pdma.h.

## ◆ PDMA_SPI2_TX

#define PDMA_SPI2_TX

DMA Connect to SPI2 TX

Definition at line 76 of file pdma.h.

## ◆ PDMA_SPI3_RX

#define PDMA_SPI3_RX

DMA Connect to SPI3 RX

Definition at line 89 of file pdma.h.

## ◆ PDMA_SPI3_TX

#define PDMA_SPI3_TX

DMA Connect to SPI3 TX

Definition at line 77 of file pdma.h.

## ◆ PDMA_UART0_RX

#define PDMA_UART0_RX

DMA Connect to UART0 RX

Definition at line 90 of file pdma.h.

## ◆ PDMA_UART0_TX

#define PDMA_UART0_TX

DMA Connect to UART0 TX

Definition at line 78 of file pdma.h.

## ◆ PDMA_UART1_RX

#define PDMA_UART1_RX

DMA Connect to UART1 RX

Definition at line 91 of file pdma.h.

## ◆ PDMA_UART1_TX

#define PDMA_UART1_TX

DMA Connect to UART1 TX

Definition at line 79 of file pdma.h.

## ◆ PDMA_UART2_RX

#define PDMA_UART2_RX

DMA Connect to UART2 RX

Definition at line 92 of file pdma.h.

## ◆ PDMA_UART2_TX

#define PDMA_UART2_TX

DMA Connect to UART2 TX

Definition at line 80 of file pdma.h.

## ◆ PDMA_UART3_RX

#define PDMA_UART3_RX

DMA Connect to UART3 RX

Definition at line 93 of file pdma.h.

## ◆ PDMA_UART3_TX

#define PDMA_UART3_TX

DMA Connect to UART3 TX

Definition at line 81 of file pdma.h.

## ◆ PDMA_UART4_RX

#define PDMA_UART4_RX

DMA Connect to UART4 RX

Definition at line 94 of file pdma.h.

## ◆ PDMA_UART4_TX

#define PDMA_UART4_TX

DMA Connect to UART4 TX

Definition at line 82 of file pdma.h.

## ◆ PDMA_UART5_RX

#define PDMA_UART5_RX

DMA Connect to UART5 RX

Definition at line 95 of file pdma.h.

## ◆ PDMA_UART5_TX

#define PDMA_UART5_TX

DMA Connect to UART5 TX

Definition at line 83 of file pdma.h.

## ◆ PDMA_WIDTH_16

#define PDMA_WIDTH_16

DMA Transfer Width 16-bit

Definition at line 45 of file pdma.h.

## ◆ PDMA_WIDTH_32

#define PDMA_WIDTH_32

DMA Transfer Width 32-bit

Definition at line 46 of file pdma.h.

## ◆ PDMA_WIDTH_8

#define PDMA_WIDTH_8

DMA Transfer Width 8-bit

Definition at line 44 of file pdma.h.