## f_mount

The f_mount fucntion registers/unregisters file system object to the FatFs module.

    FRESULT f_mount (
      FATFS*       fs,    /* [IN] File system object */
      const TCHAR* path,  /* [IN] Logical drive number */
      BYTE         opt    /* [IN] Initialization option */
    );

#### Parameters

fs
  Pointer to the file system object to be registered and cleared. Null pointer unregisters the registered file system object.
path
  Pointer to the null-terminated string that specifies the logical drive. The string without drive number means the default drive.
opt
  Initialization option. 0: Do not mount now (to be mounted later), 1: Force mounted the volume to check if the FAT volume is ready to work.

#### Return Values

FR_OK, FR_INVALID_DRIVE, FR_DISK_ERR, FR_NOT_READY, FR_NO_FILESYSTEM

#### Description

The `f_mount` function registers/unregisters a file system object used for the logical drive to the FatFs module as follows:

1. Determines the logical drive which specified by `path`.
2. Clears and unregisters the regsitered work area of the drive.
3. Clears and registers the new work area to the drive if `fs` is not NULL.
4. Performs volume mount process to the drive if forced mount is specified.

The file system object is the work area needed for each logical drive. It must be given to the logical drive with this function prior to use any other file functions except for `f_fdisk` function to the logical drive. To unregister the work area, specify a NULL to the `fs`, and then the work area can be discarded.

If forced mounting is not specified, this function always succeeds regardless of the physical drive status due to delayed mount feature. It only clears (de-initializes) the given work area and registers its address to the internal table. No activity of the physical drive in this function. It can also be used to force de-initialized the registered work area of a logical drive. The volume mount processes, initialize the corresponding physical drive, find the FAT volume in it and initialize the work area, is performed in the subsequent file access functions when either or both of following condition is true.

- File system object is not initialized. It is de-initialized by `f_mount` function.
- Physical drive is not initialized. It is de-initialized by system reset or media removal.

If the function with forced mounting failed, it means that the file system object has been registered successfully but the volume is currently not ready to work. The volume mount process will also be attempted at subsequent file access functions.

If implementation of the disk I/O layer lacks media change detection, application program needs to perform a `f_mount` function after each media change to force cleared the file system object.

#### QuickInfo

Always available.

#### See Also

`f_open`, `FATFS`

Return