CMSIS-RTOS2: Thread Management

| CMSIS-RTOS2 Version 2.1.1 Real-Time Operating System: API and RTX Reference Implementation

- Main Page
- Usage and Description
- Reference

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Structures | Macros | Typedefs | Enumerations | Enumerator | Functions
Thread Management
CMSIS-RTOS2 API

Define, create, and control thread functions. More...

## Data Structures
struct | osThreadAttr_t
| Attributes structure for thread. More...

## Macros
#define | osThreadJoinable 0x00000001U
| Thread created in joinable mode. More...
#define | osThreadDetached 0x00000000U
| Thread created in detached mode (default) More...

## Typedefs
typedef void(* | osThreadFunc_t )(void *argument)
| Entry point of a thread. More...
typedef void * | osThreadId_t

## Enumerations
enum | osThreadState_t { osThreadInactive = 0, osThreadReady = 1, osThreadRunning = 2, osThreadBlocked = 3, osThreadTerminated = 4, osThreadError = -1, osThreadReserved = 0x7FFFFFFF }
| Thread state. More...
enum | osPriority_t { osPriorityNone = 0, osPriorityIdle = 1, osPriorityLow = 8, osPriorityLow1 = 8+1, osPriorityLow2 = 8+2, osPriorityLow3 = 8+3, osPriorityLow4 = 8+4, osPriorityLow5 = 8+5, osPriorityLow6 = 8+6, osPriorityLow7 = 8+7, osPriorityBelowNormal = 16, osPriorityBelowNormal1 = 16+1, osPriorityBelowNormal2 = 16+2, osPriorityBelowNormal3 = 16+3, osPriorityBelowNormal4 = 16+4, osPriorityBelowNormal5 = 16+5, osPriorityBelowNormal6 = 16+6, osPriorityBelowNormal7 = 16+7, osPriorityNormal = 24, osPriorityNormal1 = 24+1, osPriorityNormal2 = 24+2, osPriorityNormal3 = 24+3, osPriorityNormal4 = 24+4, osPriorityNormal5 = 24+5, osPriorityNormal6 = 24+6, osPriorityNormal7 = 24+7, osPriorityAboveNormal = 32, osPriorityAboveNormal1 = 32+1, osPriorityAboveNormal2 = 32+2, osPriorityAboveNormal3 = 32+3, osPriorityAboveNormal4 = 32+4, osPriorityAboveNormal5 = 32+5, osPriorityAboveNormal6 = 32+6, osPriorityAboveNormal7 = 32+7, osPriorityHigh = 40, osPriorityHigh1 = 40+1, osPriorityHigh2 = 40+2, osPriorityHigh3 = 40+3, osPriorityHigh4 = 40+4, osPriorityHigh5 = 40+5, osPriorityHigh6 = 40+6, osPriorityHigh7 = 40+7, osPriorityRealtime = 48, osPriorityRealtime1 = 48+1, osPriorityRealtime2 = 48+2, osPriorityRealtime3 = 48+3, osPriorityRealtime4 = 48+4, osPriorityRealtime5 = 48+5, osPriorityRealtime6 = 48+6, osPriorityRealtime7 = 48+7, osPriorityISR = 56, osPriorityError = -1, osPriorityReserved = 0x7FFFFFFF }
| Priority values. More...

## Functions
osThreadId_t | osThreadNew (osThreadFunc_t func, void *argument, const osThreadAttr_t *attr)
| Create a thread and add it to Active Threads. More...
const char * | osThreadGetName (osThreadId_t thread_id)
| Get name of a thread. More...
osThreadId_t | osThreadGetId (void)
| Return the thread ID of the current running thread. More...
osThreadState_t | osThreadGetState (osThreadId_t thread_id)
| Get current thread state of a thread. More...
osStatus_t | osThreadSetPriority (osThreadId_t thread_id, osPriority_t priority)
| Change priority of a thread. More...
osPriority_t | osThreadGetPriority (osThreadId_t thread_id)
| Get current priority of a thread. More...
osStatus_t | osThreadYield (void)
| Pass control to next thread that is in state READY. More...
osStatus_t | osThreadSuspend (osThreadId_t thread_id)
| Suspend execution of a thread. More...
osStatus_t | osThreadResume (osThreadId_t thread_id)
| Resume execution of a thread. More...
osStatus_t | osThreadDetach (osThreadId_t thread_id)
| Detach a thread (thread storage can be reclaimed when thread terminates). More...
osStatus_t | osThreadJoin (osThreadId_t thread_id)
| Wait for specified thread to terminate. More...
__NO_RETURN void | osThreadExit (void)
| Terminate execution of current running thread. More...
osStatus_t | osThreadTerminate (osThreadId_t thread_id)
| Terminate execution of a thread. More...
uint32_t | osThreadGetStackSize (osThreadId_t thread_id)
| Get stack size of a thread. More...
uint32_t | osThreadGetStackSpace (osThreadId_t thread_id)
| Get available stack space of a thread based on stack watermark recording during execution. More...
uint32_t | osThreadGetCount (void)
| Get number of active threads. More...
uint32_t | osThreadEnumerate (osThreadId_t *thread_array, uint32_t array_items)
| Enumerate active threads. More...

## Description

The Thread Management function group allows defining, creating, and controlling thread functions in the system.

Note
  Thread management functions cannot be called from Interrupt Service Routines.

## Thread states

Threads can be in the following states:

- RUNNING: The thread that is currently running is in the RUNNING state. Only one thread at a time can be in this state.
- READY: Threads which are ready to run are in the READY state. Once the RUNNING thread has terminated, or is BLOCKED, the next READY thread with the highest priority becomes the RUNNING thread.
- BLOCKED: Threads that are blocked either delayed, waiting for an event to occur or suspended are in the BLOCKED state.
- TERMINATED: When osThreadTerminate is called, threads are TERMINATED with resources not yet released.
- INACTIVE: Threads that are not created or have been terminated with all resources released are in the INACTIVE state.

Thread State and State Transitions

A CMSIS-RTOS assumes that threads are scheduled as shown in the figure Thread State and State Transitions. The thread states change as follows:

- A thread is created using the function osThreadNew. This puts the thread into the READY or RUNNING state (depending on the thread priority).
- CMSIS-RTOS is pre-emptive. The active thread with the highest priority becomes the RUNNING thread provided it does not wait for any event. The initial priority of a thread is defined with the osThreadAttr_t but may be changed during execution using the function osThreadSetPriority.
- The RUNNING thread transfers into the BLOCKED state when it is delayed, waiting for an event or suspended.
- Active threads can be terminated any time using the function osThreadTerminate. Threads can terminate also by just returning from the thread function. Threads that are terminated are in the INACTIVE state and typically do not consume any dynamic memory resources.

Note
  Refer to Thread Configuration for RTX5 configuration options.

# Thread Examples

The following examples show various scenarios to create threads:

Example 1 - Create a simple thread

Create a thread out of the function thread1 using all default values for thread attributes and memory from the Global Memory Pool.

__NO_RETURN void thread1 (void *argument) {
// ...
for (;;) {}
}
int main (void) {
osKernelInitialize();
;
osThreadNew(thread1, NULL, NULL); // Create thread with default settings
;
osKernelStart();
}

Example 2 - Create thread with stack non-default stack size

Similar to the simple thread all attributes are default. The stack is dynamically allocated from the Global Memory Pool

osThreadAttr_t::stack_size is used to pass the stack size in Bytes to osThreadNew.

__NO_RETURN void thread1 (void *argument) {
// ...
for (;;) {}
}
const osThreadAttr_t thread1_attr = {
.stack_size = 1024 // Create the thread stack with a size of 1024 bytes
};
int main (void) {
;
osThreadNew(thread1, NULL, &thread1_attr); // Create thread with custom sized stack memory
;
}

Example 3 - Create thread with statically allocated stack

Similar to the simple thread all attributes are default. The stack is statically allocated using the `uint64_t` array `thread1_stk_1`. This allocates 64*8 Bytes (=512 Bytes) with an alignment of 8 Bytes (mandatory for Cortex-M stack memory).

osThreadAttr_t::stack_mem holds a pointer to the stacks lowest address.

osThreadAttr_t::stack_size is used to pass the stack size in Bytes to osThreadNew.

__NO_RETURN void thread1 (void *argument) {
// ...
for (;;) {}
}
static uint64_t thread1_stk_1[64];
const osThreadAttr_t thread1_attr = {
.stack_mem = &thread1_stk_1[0],
.stack_size = sizeof(thread1_stk_1)
};
int main (void) {
;
osThreadNew(thread1, NULL, &thread1_attr); // Create thread with statically allocated stack memory
;
}

Example 4 - Thread with statically allocated task control block

Typically this method is chosen together with a statically allocated stack as shown in Example 2.

#include "cmsis_os2.h"
//include rtx_os.h for types of RTX objects
#include "rtx_os.h"
__NO_RETURN void thread1 (void *argument) {
// ...
for (;;) {}
}
static osRtxThread_t thread1_tcb;
const osThreadAttr_t thread1_attr = {
.cb_mem = &thread1_tcb,
.cb_size = sizeof(thread1_tcb),
};
int main (void) {
;
osThreadNew(thread1, NULL, &thread1_attr); // Create thread with custom tcb memory
;
}

Example 5 - Create thread with a different priority

The default priority of RTX is osPriorityNormal. Often you want to run a task with a higher or lower priority. Using the osThreadAttr_t control structure you can set any initial priority required.

__NO_RETURN void thread1 (void *argument) {
// ...
for (;;) {}
}
const osThreadAttr_t thread1_attr = {
.priority = osPriorityHigh //Set initial thread priority to high
};
int main (void) {
;
osThreadNew(thread1, NULL, &thread1_attr);
;
}

Example 6 - Joinable threads

In this example a master thread creates four threads with the osThreadJoinable attribute. These will do some work and return using the osThreadExit call after finished. osThreadJoin is used to synchronize the thread termination.

__NO_RETURN void worker (void *argument) {
; // work a lot on data[]
osDelay(1000);
osThreadExit();
}
__NO_RETURN void thread1 (void *argument) {
osThreadAttr_t worker_attr;
osThreadId_t worker_ids[4];
uint8_t data[4][10];
memset(&worker_attr, 0, sizeof(worker_attr));
worker_attr.attr_bits = osThreadJoinable;
worker_ids[0] = osThreadNew(worker, &data[0][0], &worker_attr);
worker_ids[1] = osThreadNew(worker, &data[1][0], &worker_attr);
worker_ids[2] = osThreadNew(worker, &data[2][0], &worker_attr);
worker_ids[3] = osThreadNew(worker, &data[3][0], &worker_attr);
osThreadJoin(worker_ids[0]);
osThreadJoin(worker_ids[1]);
osThreadJoin(worker_ids[2]);
osThreadJoin(worker_ids[3]);
osThreadExit();
}

## Data Structure Documentation

struct osThreadAttr_t

Data Fields
const char * | name | name of the thread Pointer to a string with a human readable name of the thread object. Default: NULL.
uint32_t | attr_bits | attribute bits The following predefined bit masks can be assigned to set options for a thread object.
Bit Mask | Description
--- | ---
osThreadDetached | Create thread in a detached mode (default).
osThreadJoinable | Create thread in joinable mode, see osThreadJoin.
void * | cb_mem | memory for control block Pointer to a memory location for the thread control block object. This can optionally be used for custom memory management systems. Default: NULL (uses kernel memory management).
uint32_t | cb_size | size of provided memory for control block The size of the memory block passed with cb_mem. Must be the size of a thread control block object or larger.
void * | stack_mem | memory for stack Pointer to a memory location for the thread stack, must be 64-bit aligned. This can optionally be used for custom memory management systems. Default: NULL (uses kernel memory management).
uint32_t | stack_size | size of stack The size of the stack specified by stack_mem in Bytes.
osPriority_t | priority | initial thread priority (default: osPriorityNormal) Specifies the initial thread priority with a value from osPriority_t. Default: osPriorityNormal
TZ_ModuleId_t | tz_module | TrustZone module identifier. TrustZone Thread Context Management Identifier to allocate context memory for threads. The RTOS kernel that runs in non-secure state calls the interface functions defined by the header file TZ_context.h. See TrustZone RTOS Context Management.
uint32_t | reserved | reserved (must be 0) Reserved for future use (set to '0'). Default: 0.

## Macro Definition Documentation

#define osThreadJoinable 0x00000001U

A thread in this state can be joined using osThreadJoin.

#define osThreadDetached 0x00000000U

A thread in this state cannot be joined using osThreadJoin.

## Typedef Documentation

void(* osThreadFunc_t)(void *argument)

Entry function for threads. Setting up a new thread (osThreadNew) will start execution with a call into this entry function. The optional argument can be used to hand over arbitrary user data to the thread, i.e. to identify the thread or for runtime parameters.

Parameters

  [in] | argument | Arbitrary user data set on osThreadNew.

osThreadId_t

Thread ID identifies the thread.

Returned by:

- osThreadNew
- osThreadGetId
- osThreadEnumerate
- osMutexGetOwner

## Enumeration Type Documentation

enum osThreadState_t

State of a thread as retrieved by osThreadGetState. In case osThreadGetState fails or if it is called from an ISR, it will return `osThreadError`, otherwise it returns the thread state.

Enumerator
osThreadInactive | Inactive. The thread is created but not actively used, or has been terminated.
osThreadReady | Ready. The thread is ready for execution but not currently running.
osThreadRunning | Running. The thread is currently running.
osThreadBlocked | Blocked. The thread is currently blocked (delayed, waiting for an event or suspended).
osThreadTerminated | Terminated. The thread is terminated and all its resources are freed.
osThreadError | Error. The thread thread has raised an error condition and cannot be scheduled.
osThreadReserved | Prevents enum down-size compiler optimization.

enum osPriority_t

The osPriority_t value specifies the priority for a thread. The default thread priority should be osPriorityNormal. If an active thread becomes ready that has a higher priority than the currently running thread then a thread switch occurs immediately. The system continues executing the thread with the higher priority.

To prevent from a priority inversion, a CMSIS-RTOS compliant OS may optionally implement a priority inheritance method. A priority inversion occurs when a high priority thread is waiting for a resource or event that is controlled by a thread with a lower priority. Thus causing the high priority thread potentially beeing blocked forever by another thread with lower priority. To come over this issue the low priority thread controlling the resource should be treated as having the higher priority until it releases the resource.

Note
  Priority inheritance only applies to mutexes.

Enumerator
osPriorityNone | No priority (not initialized).
osPriorityIdle | Reserved for Idle thread. This lowest priority should not be used for any other thread.
osPriorityLow | Priority: low.
osPriorityLow1 | Priority: low + 1.
osPriorityLow2 | Priority: low + 2.
osPriorityLow3 | Priority: low + 3.
osPriorityLow4 | Priority: low + 4.
osPriorityLow5 | Priority: low + 5.
osPriorityLow6 | Priority: low + 6.
osPriorityLow7 | Priority: low + 7.
osPriorityBelowNormal | Priority: below normal.
osPriorityBelowNormal1 | Priority: below normal + 1.
osPriorityBelowNormal2 | Priority: below normal + 2.
osPriorityBelowNormal3 | Priority: below normal + 3.
osPriorityBelowNormal4 | Priority: below normal + 4.
osPriorityBelowNormal5 | Priority: below normal + 5.
osPriorityBelowNormal6 | Priority: below normal + 6.
osPriorityBelowNormal7 | Priority: below normal + 7.
osPriorityNormal | Priority: normal.
osPriorityNormal1 | Priority: normal + 1.
osPriorityNormal2 | Priority: normal + 2.
osPriorityNormal3 | Priority: normal + 3.
osPriorityNormal4 | Priority: normal + 4.
osPriorityNormal5 | Priority: normal + 5.
osPriorityNormal6 | Priority: normal + 6.
osPriorityNormal7 | Priority: normal + 7.
osPriorityAboveNormal | Priority: above normal.
osPriorityAboveNormal1 | Priority: above normal + 1.
osPriorityAboveNormal2 | Priority: above normal + 2.
osPriorityAboveNormal3 | Priority: above normal + 3.
osPriorityAboveNormal4 | Priority: above normal + 4.
osPriorityAboveNormal5 | Priority: above normal + 5.
osPriorityAboveNormal6 | Priority: above normal + 6.
osPriorityAboveNormal7 | Priority: above normal + 7.
osPriorityHigh | Priority: high.
osPriorityHigh1 | Priority: high + 1.
osPriorityHigh2 | Priority: high + 2.
osPriorityHigh3 | Priority: high + 3.
osPriorityHigh4 | Priority: high + 4.
osPriorityHigh5 | Priority: high + 5.
osPriorityHigh6 | Priority: high + 6.
osPriorityHigh7 | Priority: high + 7.
osPriorityRealtime | Priority: realtime.
osPriorityRealtime1 | Priority: realtime + 1.
osPriorityRealtime2 | Priority: realtime + 2.
osPriorityRealtime3 | Priority: realtime + 3.
osPriorityRealtime4 | Priority: realtime + 4.
osPriorityRealtime5 | Priority: realtime + 5.
osPriorityRealtime6 | Priority: realtime + 6.
osPriorityRealtime7 | Priority: realtime + 7.
osPriorityISR | Reserved for ISR deferred thread. This highest priority might be used by the RTOS implementation but must not be used for any user thread.
osPriorityError | System cannot determine priority or illegal priority.
osPriorityReserved | Prevents enum down-size compiler optimization.

## Function Documentation

osThreadId_t osThreadNew | ( | osThreadFunc_t | func,
|  | void * | argument,
|  | const osThreadAttr_t * | attr
| ) |  |

Parameters

  [in] | func | thread function.
  [in] | argument | pointer that is passed to the thread function as start argument.
  [in] | attr | thread attributes; NULL: default values.

Returns
  thread ID for reference by other functions or NULL in case of error.

The function osThreadNew starts a thread function by adding it to the list of active threads and sets it to state READY. Arguments for the thread function are passed using the parameter pointer *argument. When the priority of the created thread function is higher than the current RUNNING thread, the created thread function starts instantly and becomes the new RUNNING thread. Thread attributes are defined with the parameter pointer attr. Attributes include settings for thread priority, stack size, or memory allocation.

The function can be safely called before the RTOS is started (call to osKernelStart), but not before it is initialized (call to osKernelInitialize).

The function osThreadNew returns the pointer to the thread object identifier or NULL in case of an error.

Note
  Cannot be called from Interrupt Service Routines.

Code Example

Refer to the Thread Examples section.

const char * osThreadGetName | ( | osThreadId_t | thread_id | ) |

Parameters

  [in] | thread_id | thread ID obtained by osThreadNew or osThreadGetId.

Returns
  name as NULL terminated string.

The function osThreadGetName returns the pointer to the name string of the thread identified by parameter thread_id or NULL in case of an error.

Note
  This function cannot be called from Interrupt Service Routines.

Code Example

void ThreadGetName_example (void) {
osThreadId_t thread_id = osThreadGetId ();
const char* name = osThreadGetName (thread_id);
if (name == NULL) {
// Failed to get the thread name; not in a thread
}
}

osThreadId_t osThreadGetId | ( | void |  | ) |

Returns
  thread ID for reference by other functions or NULL in case of error.

The function osThreadGetId returns the thread object ID of the currently running thread or NULL in case of an error.

Note
  This function cannot be called from Interrupt Service Routines.

Code Example

void ThreadGetId_example (void) {
osThreadId_t id; // id for the currently running thread
id = osThreadGetId ();
if (id == NULL) {
// Failed to get the id; not in a thread
}
}

osThreadState_t osThreadGetState | ( | osThreadId_t | thread_id | ) |

Parameters

  [in] | thread_id | thread ID obtained by osThreadNew or osThreadGetId.

Returns
  current thread state of the specified thread.

The function osThreadGetState returns the state of the thread identified by parameter thread_id. In case it fails or if it is called from an ISR, it will return `osThreadError`, otherwise it returns the thread state (refer to osThreadState_t for the list of thread states).

Note
  This function cannot be called from Interrupt Service Routines.

osStatus_t osThreadSetPriority | ( | osThreadId_t | thread_id,
|  | osPriority_t | priority
| ) |  |

Parameters

  [in] | thread_id | thread ID obtained by osThreadNew or osThreadGetId.
  [in] | priority | new priority value for the thread function.

Returns
  status code that indicates the execution status of the function.

The function osThreadSetPriority changes the priority of an active thread specified by the parameter thread_id to the priority specified by the parameter priority.

Possible osStatus_t return values:

- osOK: the priority of the specified thread has been changed successfully.
- osErrorParameter: thread_id is NULL or invalid or priority is incorrect.
- osErrorResource: thread specified by parameter thread_id is in an invalid thread state.
- osErrorISR: the function osThreadSetPriority cannot be called from interrupt service routines.

Note
  This function cannot be called from Interrupt Service Routines.

Code Example

#include "cmsis_os2.h"
void Thread_1 (void const *arg) { // Thread function
osThreadId_t id; // id for the currently running thread
osStatus_t status; // status of the executed function
:
id = osThreadGetId (); // Obtain ID of current running thread
status = osThreadSetPriority (id, osPriorityBelowNormal); // Set thread priority
if (status == osOK) {
// Thread priority changed to BelowNormal
}
else {
// Failed to set the priority
}
:
}

osPriority_t osThreadGetPriority | ( | osThreadId_t | thread_id | ) |

Parameters

  [in] | thread_id | thread ID obtained by osThreadNew or osThreadGetId.

Returns
  current priority value of the specified thread.

The function osThreadGetPriority returns the priority of an active thread specified by the parameter thread_id.

Possible osPriority_t return values:

- priority: the priority of the specified thread.
- osPriorityError: priority cannot be determined or is illegal. It is also returned when the function is called from Interrupt Service Routines.

Note
  This function cannot be called from Interrupt Service Routines.

Code Example

#include "cmsis_os2.h"
void Thread_1 (void const *arg) { // Thread function
osThreadId_t id; // id for the currently running thread
osPriority_t priority; // thread priority
id = osThreadGetId (); // Obtain ID of current running thread
priority = osThreadGetPriority (id); // Obtain the thread priority
}

osStatus_t osThreadYield | ( | void |  | ) |

Returns
  status code that indicates the execution status of the function.

The function osThreadYield passes control to the next thread with the same priority that is in the READY state. If there is no other thread with the same priority in state READY, then the current thread continues execution and no thread switch occurs. osThreadYield does not set the thread to state BLOCKED. Thus no thread with a lower priority will be scheduled even if threads in state READY are available.

Possible osStatus_t return values:

- osOK: control has been passed to the next thread successfully.
- osError: an unspecified error has occurred.
- osErrorISR: the function osThreadYield cannot be called from interrupt service routines.

Note
  This function cannot be called from Interrupt Service Routines.
  This function has no impact when called when the kernel is locked, see osKernelLock.

Code Example

#include "cmsis_os2.h"
void Thread_1 (void const *arg) { // Thread function
osStatus_t status; // status of the executed function
:
while (1) {
status = osThreadYield(); //
if (status != osOK) {
// an error occurred
}
}
}

osStatus_t osThreadSuspend | ( | osThreadId_t | thread_id | ) |

Parameters

  [in] | thread_id | thread ID obtained by osThreadNew or osThreadGetId.

Returns
  status code that indicates the execution status of the function.

The function osThreadSuspend suspends the execution of the thread identified by parameter thread_id. The thread is put into the BLOCKED state (osThreadBlocked). Suspending the running thread will cause a context switch to another thread in READY state immediately. The suspended thread is not executed until explicitly resumed with the function osThreadResume.

Threads that are already BLOCKED are removed from any wait list and become ready when they are resumed. Thus it is not recommended to suspend an already blocked thread.

Possible osStatus_t return values:

- osOK: the thread has been suspended successfully.
- osErrorParameter: thread_id is NULL or invalid.
- osErrorResource: thread specified by parameter thread_id is in an invalid thread state.
- osErrorISR: the function osThreadSuspend cannot be called from interrupt service routines.

Note
  This function cannot be called from Interrupt Service Routines.
  This function must not be called to suspend the running thread when the kernel is locked, i.e. osKernelLock.

osStatus_t osThreadResume | ( | osThreadId_t | thread_id | ) |

Parameters

  [in] | thread_id | thread ID obtained by osThreadNew or osThreadGetId.

Returns
  status code that indicates the execution status of the function.

The function osThreadResume puts the thread identified by parameter thread_id (which has to be in BLOCKED state) back to the READY state. If the resumed thread has a higher priority than the running thread a context switch occurs immediately.

The thread becomes ready regardless of the reason why the thread was blocked. Thus it is not recommended to resume a thread not suspended by osThreadSuspend.

Functions that will put a thread into BLOCKED state are: osEventFlagsWait and osThreadFlagsWait, osDelay and osDelayUntil, osMutexAcquire and osSemaphoreAcquire, osMessageQueueGet, osMemoryPoolAlloc, osThreadJoin, osThreadSuspend.

Possible osStatus_t return values:

- osOK: the thread has been resumed successfully.
- osErrorParameter: thread_id is NULL or invalid.
- osErrorResource: thread specified by parameter thread_id is in an invalid thread state.
- osErrorISR: the function osThreadResume cannot be called from interrupt service routines.

Note
  This function cannot be called from Interrupt Service Routines.
  This function may be called when kernel is locked (osKernelLock). Under this circumstances a potential context switch is delayed until the kernel gets unlocked, i.e. osKernelUnlock or osKernelRestoreLock.

osStatus_t osThreadDetach | ( | osThreadId_t | thread_id | ) |

Parameters

  [in] | thread_id | thread ID obtained by osThreadNew or osThreadGetId.

Returns
  status code that indicates the execution status of the function.

The function osThreadDetach changes the attribute of a thread (specified by thread_id) to osThreadDetached. Detached threads are not joinable with osThreadJoin. When a detached thread is terminated, all resources are returned to the system. The behavior of osThreadDetach on an already detached thread is undefined.

Possible osStatus_t return values:

- osOK: the attribute of the specified thread has been changed to detached successfully.
- osErrorParameter: thread_id is NULL or invalid.
- osErrorResource: thread specified by parameter thread_id is in an invalid thread state.
- osErrorISR: the function osThreadDetach cannot be called from interrupt service routines.

Note
  This function cannot be called from Interrupt Service Routines.

osStatus_t osThreadJoin | ( | osThreadId_t | thread_id | ) |

Parameters

  [in] | thread_id | thread ID obtained by osThreadNew or osThreadGetId.

Returns
  status code that indicates the execution status of the function.

The function osThreadJoin waits for the thread specified by thread_id to terminate. If that thread has already terminated, then osThreadJoin returns immediately. The thread must be joinable. By default threads are created with the attribute osThreadDetached.

Possible osStatus_t return values:

- osOK: if the thread has already been terminated and joined or once the thread has been terminated and the join operations succeeds.
- osErrorParameter: thread_id is NULL or invalid.
- osErrorResource: parameter thread_id is NULL or refers to a thread that is not an active thread or the thread is not joinable.
- osErrorISR: the function osThreadJoin cannot be called from interrupt service routines.

Note
  This function cannot be called from Interrupt Service Routines.

__NO_RETURN void osThreadExit | ( | void |  | ) |

The function osThreadExit terminates the calling thread. This allows the thread to be synchronized with osThreadJoin.

Note
  This function cannot be called from Interrupt Service Routines.

Code Example

__NO_RETURN void worker (void *argument) {
// do something
osDelay(1000);
osThreadExit();
}

osStatus_t osThreadTerminate | ( | osThreadId_t | thread_id | ) |

Parameters

  [in] | thread_id | thread ID obtained by osThreadNew or osThreadGetId.

Returns
  status code that indicates the execution status of the function.

The function osThreadTerminate removes the thread specified by parameter thread_id from the list of active threads. If the thread is currently RUNNING, the thread terminates and the execution continues with the next READY thread. If no such thread exists, the function will not terminate the running thread, but return osErrorResource.

Possible osStatus_t return values:

- osOK: the specified thread has been removed from the active thread list successfully.
- osErrorParameter: thread_id is NULL or invalid.
- osErrorResource: thread specified by parameter thread_id is in an invalid thread state or no other READY thread exists.
- osErrorISR: the function osThreadTerminate cannot be called from interrupt service routines.

Note
  This function cannot be called from Interrupt Service Routines.
  Avoid calling the function with a thread_id that does not exist or has been terminated already.

Code Example

#include "cmsis_os2.h"
void Thread_1 (void *arg); // function prototype for Thread_1
void ThreadTerminate_example (void) {
osStatus_t status;
osThreadId_t id;
id = osThreadNew (Thread_1, NULL, NULL); // create the thread
// do something
status = osThreadTerminate (id); // stop the thread
if (status == osOK) {
// Thread was terminated successfully
}
else {
// Failed to terminate a thread
}
}

uint32_t osThreadGetStackSize | ( | osThreadId_t | thread_id | ) |

Parameters

  [in] | thread_id | thread ID obtained by osThreadNew or osThreadGetId.

Returns
  stack size in bytes.

The function osThreadGetStackSize returns the stack size of the thread specified by parameter thread_id. In case of an error, it returns 0.

Note
  This function cannot be called from Interrupt Service Routines.

uint32_t osThreadGetStackSpace | ( | osThreadId_t | thread_id | ) |

Parameters

  [in] | thread_id | thread ID obtained by osThreadNew or osThreadGetId.

Returns
  remaining stack space in bytes.

The function osThreadGetStackSpace returns the size of unused stack space for the thread specified by parameter thread_id. Stack watermark recording during execution needs to be enabled (refer to Thread Configuration). In case of an error, it returns 0.

Note
  This function cannot be called from Interrupt Service Routines.

uint32_t osThreadGetCount | ( | void |  | ) |

Returns
  number of active threads.

The function osThreadGetCount returns the number of active threads or 0 in case of an error.

Note
  This function cannot be called from Interrupt Service Routines.

uint32_t osThreadEnumerate | ( | osThreadId_t * | thread_array,
|  | uint32_t | array_items
| ) |  |

Parameters

  [out] | thread_array | pointer to array for retrieving thread IDs.
  [in] | array_items | maximum number of items in array for retrieving thread IDs.

Returns
  number of enumerated threads.

The function osThreadEnumerate returns the number of enumerated threads or 0 in case of an error.

Note
  This function cannot be called from Interrupt Service Routines.