CMSIS-DAP: Validate Debug Unit

| CMSIS-DAP Version 1.2.0 (Proposal) Interface Firmware for CoreSight Debug Access Port

- Main Page
- Usage and Description
- Reference

All Functions Groups Pages
Validate Debug Unit

A CMSIS-DAP conforming Debug Unit must be validated. More...

A CMSIS-DAP conforming Debug Unit must be validated.

A CMSIS-DAP Debug Unit must be validate using the Keil MDK-ARM Debugger. A validation project for MDK is provided in the folder .\Validation\MDK. The project Blinky.uvproj is a "Blinky" application and needs to be adapted for the target hardware that is connected to the Debug Unit. Once the adaptation is complete, you may open a Command Prompt and call the batch file TestAll.bat optionally with the path to UV4.EXE. This should generate the following output.

Validate Debug Unit using a target hardware and MDK