..\..\..\..\..\ML51_BSP\Library\Startup\exe\hex2bin.exe  .\output\@L.hex

hex2bin.exe  .\output\@L.hex
    *By default, unused location will be filled with FF

hex2bin.exe  .\output\@L.hex -P 0x00
   * With parameter ¡VP or ¡Vp filled with data defined following. In this case will be filled with 00.

hex2bin.exe  .\output\@L.hex -p 0xFF
    *Same as ¡VP. in this case filled with FF

hex2bin.exe  .\output\@L.hex 0x0 0x1000 0xFF80 0x80
    *Create two bin file. Unused location filled with 00.The first file <project>.bin data create start from 0x00 and file size is0x1000. The second file  <project name1>.bin create start from 0xFF80 file size is 0x80.

hex2bin.exe  .\output\@L.hex -P 0xFF 0x0 0x1000 0xFF80 0x80
    *Create two bin file. Unused location filled parameter after ¡VP defined. In this case will be filled with  FF.
